(module TI_WSON8_2x2mm_p0.65mm (layer F.Cu) (tedit 5BF575E8)
  (fp_text reference REF** (at 0 2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TI_WSON8_2x2mm_p0.65mm (at 0 -1.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.95 -0.9) (end -0.95 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.95 -1) (end 1 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -1) (end 1 -0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.9) (end 1 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 1) (end -1 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 1) (end -1 0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3 -0.65) (end -1.4 -0.75) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.4 -0.75) (end -1.4 -0.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.4 -0.55) (end -1.3 -0.65) (layer F.SilkS) (width 0.15))
  (pad 1 smd roundrect (at -0.975 -0.65) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 2 smd roundrect (at -0.975 0) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 3 smd roundrect (at -0.975 0.65) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 4 smd roundrect (at 0.975 -0.65) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 5 smd roundrect (at 0.975 0) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 6 smd roundrect (at 0.975 0.65) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.16))
  (pad 7 smd roundrect (at 0 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.05))
)
