(module LED_Kingbright_APHB1608 (layer F.Cu) (tedit 5BF577B1)
  (fp_text reference REF** (at 0 1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED_Kingbright_APHB1608 (at 0 -1.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.25 0.4) (end 0.25 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.8 0.05) (end 0.8 -0.05) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.8 0.05) (end -0.8 -0.05) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 -0.4) (end 0.25 -0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.05 0.4) (end 0.05 -0.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.95 0.35) (end 1.05 0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.95 0.35) (end 1.05 0.45) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.05 0.45) (end 1.05 0.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.05 0) (end -0.1 0) (layer F.SilkS) (width 0.15))
  (pad 4 smd rect (at -0.6 -0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.6 -0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.6 0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0.6 0.35) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask))
)
