(module FuseHolder_SMD_Shurter_0031.7701.11 (layer F.Cu) (tedit 5BF57487)
  (fp_text reference REF** (at 0 4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FuseHolder_SMD_Shurter_0031.7701.11 (at 0 -4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1 -3) (end 1 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 3) (end 1 3) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -4 0) (size 5 6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4 0) (size 5 6) (layers F.Cu F.Paste F.Mask))
)
