(module DipSW_CHP-081TA (layer F.Cu) (tedit 5BF57BC7)
  (fp_text reference REF** (at 4.318 -4.318) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DipSW_CHP-081TA (at 0 -4.445) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 5 -3) (end 6.1 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.1 -3) (end 6.1 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.1 3) (end 5 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -5 3.1) (end -6 3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 3.1) (end -6 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -3) (end -5 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.7 1.6) (end -4.2 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.2 1.6) (end -4.2 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.7 1.6) (end -4.7 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.7 1.1) (end -4.2 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.43 1.6) (end -2.93 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.43 1.1) (end -2.93 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.43 1.6) (end -3.43 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.93 1.6) (end -2.93 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.16 1.6) (end -1.66 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.66 1.6) (end -1.66 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.16 1.6) (end -2.16 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.16 1.1) (end -1.66 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.89 1.6) (end -0.39 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.39 1.6) (end -0.39 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.89 1.6) (end -0.89 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.89 1.1) (end -0.39 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.38 1.6) (end 0.38 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.88 1.6) (end 0.88 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.38 1.6) (end 0.88 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.38 1.1) (end 0.88 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 1.1) (end 2.15 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 1.6) (end 1.65 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.15 1.6) (end 2.15 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.65 1.6) (end 2.15 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.92 1.6) (end 2.92 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.42 1.6) (end 3.42 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.92 1.1) (end 3.42 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.92 1.6) (end 3.42 1.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.69 1.6) (end 4.69 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.19 1.1) (end 4.69 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.19 1.6) (end 4.19 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.19 1.6) (end 4.69 1.6) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -4.445 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.175 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.905 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.635 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.635 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.905 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 3.175 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 4.445 2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 4.445 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 3.175 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.905 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0.635 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -0.635 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -1.905 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -3.175 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -4.445 -2.54) (size 0.76 1.6) (layers F.Cu F.Paste F.Mask))
)
