EESchema-DOCLIB  Version 2.0
#
$CMP 5P49V6965
D VersaClock® 6E Programmable Clock Generator 1kHz-350MHz
K clock pll reference
$ENDCMP
#
$CMP CBTL02043A
D 3.3 V, 2 differential channel, 2:1 MUX/deMUX switch, up to 10Gbps
$ENDCMP
#
#End Doc Library
