(module Crystal_Epsom_TSX-3225 (layer F.Cu) (tedit 5BF5790A)
  (fp_text reference REF** (at 0 2.45) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Crystal_Epsom_TSX-3225 (at 0 -2.55) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.3 1.25) (end 0.3 1.25) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.3 -1.25) (end 0.3 -1.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.6 0.1) (end 1.6 -0.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.6 0.1) (end -1.6 -0.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.95 0.75) (end -2.05 0.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.05 0.6) (end -2.05 0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.05 0.9) (end -1.95 0.75) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.1 0.8) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.1 0.8) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.1 -0.8) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.1 -0.8) (size 1.4 1.15) (layers F.Cu F.Paste F.Mask))
)
