(module max1112x-tqfn28:MAX1112x-TQFN-28-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 5B9AA36A)
  (descr "28-Lead Plastic Quad Flat, No Lead Package (MQ) - 5x5x0.9 mm Body [QFN or VQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "TQFN 0.5")
  (attr smd)
  (fp_text reference U8 (at 0 -3.875) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MAX11125 (at 0 3.875) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -3.048 -2.032) (end -2.9464 -2.032) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.625 -2.625) (end -1.875 -2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -2.5) (end 2.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 2.5 -2.5) (end 2.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 2.5 2.5) (end -2.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -2.5 2.5) (end -2.5 -1.5) (layer F.Fab) (width 0.15))
  (fp_line (start -2.5 -1.5) (end -1.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.15 -3.15) (end -3.15 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.15 -3.15) (end 3.15 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 -3.15) (end 3.15 -3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.15 3.15) (end 3.15 3.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.625 -2.625) (end 2.625 -1.875) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.625 2.625) (end -2.625 1.875) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.625 2.625) (end 2.625 1.875) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.625 -2.625) (end -2.625 -1.875) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.625 2.625) (end -1.875 2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.625 2.625) (end 1.875 2.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.625 -2.625) (end 1.875 -2.625) (layer F.SilkS) (width 0.15))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.625 -1.875) (end -1.875 -2.625) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -2.34 -1.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -2.34 -1) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -2.34 -0.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -2.34 0) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -2.34 0.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -2.34 1) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -2.34 1.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at -1.5 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at -1 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at -0.5 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 0 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 0.5 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 1 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 1.5 2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 2.34 1.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at 2.34 1) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 2.34 0.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 2.34 0) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 2.34 -0.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at 2.34 -1) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at 2.34 -1.5) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at 1.5 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at 1 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at 0.5 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd oval (at 0 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd oval (at -0.5 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd oval (at -1 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd oval (at -1.5 -2.34 90) (size 0.95 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 0.8125 0.8125) (size 1.625 1.625) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin_ratio -0.2))
  (pad 29 smd rect (at 0.8125 -0.8125) (size 1.625 1.625) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin_ratio -0.2))
  (pad 29 smd rect (at -0.8125 0.8125) (size 1.625 1.625) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin_ratio -0.2))
  (pad 29 smd rect (at -0.8125 -0.8125) (size 1.625 1.625) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin_ratio -0.2))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
