(module oscxo:Crystal_SMD_7050_4Pads (layer F.Cu) (tedit 5BC099EC)
  (descr "Crystal oscillator, 7.0x5.0mm, 4 Pads")
  (tags "crystal oscillator quartz SMD SMT 7050")
  (attr smd)
  (fp_text reference Y1 (at 0 3.556) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FNETHE025 (at 0 3.193) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.5 2.5) (end -3.5 1.5) (layer F.Fab) (width 0.15))
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.75 -3.1) (end 4.75 3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.75 3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.5 1.1) (end 3.5 -1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.2 -2.5) (end 1.2 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.75 -3.1) (end -4.75 -3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.75 -3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.5 1.1) (end -4.35 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.2 2.5) (end 1.2 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 -1.1) (end -3.5 1.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.8 2.5) (end -4.35 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5 -2.5) (end 3.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 -2.5) (end 3.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 2.5) (end -2.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.5 1.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
  (pad 4 smd rect (at -2.54 -2.2) (size 2.2 1.8) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.15))
  (pad 3 smd rect (at 2.54 -2.2) (size 2.2 1.8) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.15))
  (pad 2 smd rect (at 2.54 2.2) (size 2.2 1.8) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.15))
  (pad 1 smd rect (at -2.54 2.2) (size 2.2 1.8) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.15))
  (model ./footprints/crystal/oscxo.3dshapes/oscxo.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.3937 0.3937 0.3937))
    (rotate (xyz 0 0 0))
  )
)
