(module ESP3212 (layer F.Cu) (tedit 57E6F83E)
  (fp_text reference REF** (at -6.096 -12.827) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ESP3212 (at 4.953 -12.954) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5 0) (end -1.5 0) (layer Dwgs.User) (width 0.05))
  (fp_line (start 0 -1.5) (end 0 1.5) (layer Dwgs.User) (width 0.05))
  (fp_text user "NO COPPER" (at 0 -8.763) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Espressif (at -6.096 7.112 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text user ESP3212 (at -4.445 7.112 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_line (start -8 -6) (end 8 -6) (layer F.SilkS) (width 0.2))
  (fp_line (start -8 -12) (end 8 -12) (layer F.SilkS) (width 0.2))
  (fp_line (start 8 -12) (end 8 12) (layer F.SilkS) (width 0.2))
  (fp_line (start 8 12) (end -8 12) (layer F.SilkS) (width 0.2))
  (fp_line (start -8 12) (end -8 -12) (layer F.SilkS) (width 0.2))
  (pad 31 smd rect (at 8 -4.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 8 -3) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 8 -1.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 8 0) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 8 1.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 8.001 4.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 8 6) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 8 7.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 8 9) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 8 10.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -8 10.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -8 9) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -8 7.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -8 6) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -8 4.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -8 3) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -8 1.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -8 0) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -8 -1.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -8 -3) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 8 3) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -8 -4.5) (size 2 0.9) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -6 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -4.5 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -3 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -1.5 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 0 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 1.5 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 3 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 4.524 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 6 12) (size 0.9 2) (layers F.Cu F.Paste F.Mask))
)
