(module ft231x:FT231X-SSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 5BC5CC01)
  (descr "FT231X SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)")
  (tags "FT231X SSOP 0.65")
  (attr smd)
  (fp_text reference U6 (at -3.556 -4.318) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FT231XS (at 0 5.08) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.2 -3.25) (end 2.2 -3.25) (layer F.Fab) (width 0.15))
  (fp_line (start 2.2 -3.25) (end 2.2 3.25) (layer F.Fab) (width 0.15))
  (fp_line (start 2.2 3.25) (end -2.2 3.25) (layer F.Fab) (width 0.15))
  (fp_line (start -2.2 3.25) (end -2.2 -2.25) (layer F.Fab) (width 0.15))
  (fp_line (start -2.2 -2.25) (end -1.2 -3.25) (layer F.Fab) (width 0.15))
  (fp_line (start -3.65 -3.55) (end -3.65 3.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.65 -3.55) (end 3.65 3.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.65 -3.55) (end 3.65 -3.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.65 3.55) (end 3.65 3.55) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 -4.191) (end -0.508 -4.191) (angle -180) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.508 -4.191) (end 2.286 -4.191) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.286 -4.191) (end 2.286 -3.429) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 -4.191) (end -2.286 -4.191) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 -4.191) (end -2.286 -3.429) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 -3.429) (end -3.302 -3.429) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 3.429) (end -2.286 4.191) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 4.191) (end 2.286 4.191) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.286 4.191) (end 2.286 3.429) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -2.7 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -2.7 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -2.7 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -2.7 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -2.7 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -2.7 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -2.7 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at -2.7 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at -2.7 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at -2.7 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at 2.7 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 2.7 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 2.7 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 2.7 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 2.7 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at 2.7 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 2.7 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 2.7 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 2.7 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at 2.7 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_4.4x6.5mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 0.93 1 1))
    (rotate (xyz 0 0 0))
  )
)
