(module Keystone_3000_1x12mm-CoinCell:Keystone_3000_1x12mm-CoinCell (layer F.Cu) (tedit 5BC09877)
  (descr http://www.keyelco.com/product-pdf.cfm?p=777)
  (tags "Keystone type 3000 coin cell retainer")
  (attr smd)
  (fp_text reference BAT1 (at -0.907 12.685 -90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CR1225 (at 0 7.5) (layer F.Fab) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_text user %R (at 0 0 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.7 -4) (end 6.7 4) (layer F.Fab) (width 0.1))
  (fp_line (start 6.7 -4) (end 6 -4) (layer F.Fab) (width 0.1))
  (fp_line (start 6.7 4) (end 6 4) (layer F.Fab) (width 0.1))
  (fp_line (start 6 -4) (end 3.4 -6.6) (layer F.Fab) (width 0.1))
  (fp_line (start 6 4) (end 3.4 6.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.4 -6.6) (end -4.1 -6.6) (layer F.Fab) (width 0.1))
  (fp_line (start 3.4 6.6) (end -4.1 6.6) (layer F.Fab) (width 0.1))
  (fp_arc (start -4.1 -5.25) (end -5.45 -5.3) (angle 90) (layer F.Fab) (width 0.1))
  (fp_line (start -2.15 10.15) (end -2.15 7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 10.15) (end -2.15 10.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 7.25) (end 2.15 10.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.15 -10.15) (end -2.15 -7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 -10.15) (end -2.15 -10.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 -7.25) (end 2.15 -10.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.45 6.75) (end 2 6.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.05 4.15) (end 3.45 6.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.85 4.15) (end 6.05 4.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.85 -4.15) (end 6.85 4.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.05 -4.15) (end 6.85 -4.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.45 -6.75) (end 6.05 -4.15) (layer F.SilkS) (width 0.12))
  (fp_line (start 2 -6.75) (end 3.45 -6.75) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.15 -7.25) (end 3.8 -7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 -7.25) (end 6.4 -4.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.4 -4.65) (end 7.35 -4.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 7.35 -4.65) (end 7.35 4.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.4 4.65) (end 7.35 4.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.8 7.25) (end 6.4 4.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.15 7.25) (end 3.8 7.25) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -4.1 5.25) (end -5.45 5.3) (angle -90) (layer F.Fab) (width 0.1))
  (fp_line (start -2 -6.75) (end -4.1 -6.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2 6.75) (end -4.1 6.75) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.15 7.25) (end -4.1 7.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.15 -7.25) (end -4.1 -7.25) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -4.1 -5.25) (end -5.6 -5.3) (angle 90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -4.1 5.25) (end -5.6 5.3) (angle -90) (layer F.SilkS) (width 0.12))
  (fp_arc (start -4.1 -5.25) (end -6.1 -5.3) (angle 90) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -8.9 0) (end -5.1 -4.6) (angle 101) (layer F.Fab) (width 0.1))
  (fp_arc (start -4.6 -5.29) (end -5.1 -4.6) (angle 60) (layer F.Fab) (width 0.1))
  (fp_arc (start -4.6 5.29) (end -5.1 4.6) (angle -60) (layer F.Fab) (width 0.1))
  (fp_arc (start -4.6 -5.29) (end -5.2 -4.5) (angle 60) (layer F.SilkS) (width 0.12))
  (fp_arc (start -4.6 5.29) (end -5.2 4.5) (angle -60) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 0) (end -6.25 0) (layer F.Fab) (width 0.15))
  (fp_arc (start -4.6 -5.29) (end -5.65 -4.22) (angle 54.1) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -4.6 5.29) (end -5.65 4.22) (angle -54.1) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -4.1 5.25) (end -6.1 5.3) (angle -90) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end -6.75 0) (angle -36.6) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -9.15 0.11) (end -5.65 -4.22) (angle 3.1) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -9.15 0.11) (end -5.65 4.22) (angle -3.1) (layer F.CrtYd) (width 0.05))
  (fp_arc (start 0 0) (end -6.75 0) (angle 36.6) (layer F.CrtYd) (width 0.05))
  (fp_arc (start -8.9 0) (end -5.2 -4.5) (angle 22.6) (layer F.SilkS) (width 0.12))
  (fp_arc (start -8.9 0) (end -3.8 2.8) (angle 21.8) (layer F.SilkS) (width 0.12))
  (pad 2 smd circle (at 0 0 270) (size 9 9) (layers F.Cu F.Mask))
  (pad 1 smd rect (at 0 7.9 270) (size 3.7 3.5) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.2) (clearance 0.7))
  (pad 1 smd rect (at 0 -7.9 270) (size 3.7 3.5) (layers F.Cu F.Paste F.Mask)
    (solder_paste_margin -0.2) (clearance 0.7))
  (model ${KIPRJMOD}/footprints/battery/keystone3000tr.3dshapes/keystone3000tr.wrl
    (offset (xyz 0 0 3))
    (scale (xyz 0.3931 0.3931 0.3931))
    (rotate (xyz -90 0 -90))
  )
)
