(module abs25:Crystal_SMD_ABS25 (layer F.Cu) (tedit 59D2C237)
  (descr "Abracon ABS25 Plastic SMD Crystal http://www.abracon.com/Resonators/abs25.pdf")
  (tags "plastic smd crystal")
  (attr smd)
  (fp_text reference Y2 (at 0 -3.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 32768Hz (at 0 3.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 -2.2) (end -4 2.2) (layer F.Fab) (width 0.15))
  (fp_line (start 4 -2.2) (end -4 -2.2) (layer F.Fab) (width 0.15))
  (fp_line (start 4 2.2) (end 4 -2.2) (layer F.Fab) (width 0.15))
  (fp_line (start -4 2.2) (end 4 2.2) (layer F.Fab) (width 0.15))
  (fp_line (start -3 -0.4) (end -3 0.4) (layer F.Fab) (width 0.15))
  (fp_line (start 3.6 -0.4) (end 3.6 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 -1.8) (end 1.8 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.8 -0.4) (end -2.8 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 -0.4) (end -3.6 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.4 -2.2) (end -4.4 2.2) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.4 -2.2) (end 4.4 2.2) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.4 2.2) (end 4.4 2.2) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.4 -2.2) (end 4.4 -2.2) (layer F.CrtYd) (width 0.15))
  (pad 4 smd rect (at -2.8 -1.4) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.8 -1.4) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.8 1.4) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.8 1.4) (size 1.8 1.4) (layers F.Cu F.Paste F.Mask))
)
