(module oled:oled_13xx (layer F.Cu) (tedit 59C40388)
  (descr "SPI OLED 0.96\"")
  (tags "SPI OLED socket strip")
  (fp_text reference OLED1 (at 6.985 -3.175) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SSD_1331 (at -5.715 -3.175) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user CS (at 7.62 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user DC (at 5.08 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user RES (at 2.54 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user SDA (at 0 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user SCL (at -2.54 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user VCC (at -5.08 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_text user GND (at -7.62 2.54) (layer F.SilkS)
    (effects (font (size 1 0.75) (thickness 0.15)))
  )
  (fp_circle (center -12.065 27.305) (end -12.065 25.4) (layer F.Fab) (width 0.15))
  (fp_circle (center 12.065 27.305) (end 12.065 29.21) (layer F.Fab) (width 0.15))
  (fp_circle (center 12.065 0.635) (end 12.065 -1.27) (layer F.Fab) (width 0.15))
  (fp_circle (center -12.065 0.635) (end -12.065 -1.27) (layer F.Fab) (width 0.15))
  (fp_text user 0.96" (at 0 27.305) (layer F.Fab)
    (effects (font (size 2 2) (thickness 0.15)))
  )
  (fp_text user "OLED DISPLAY" (at 0.635 24.765) (layer F.Fab)
    (effects (font (size 2 2) (thickness 0.15)))
  )
  (fp_line (start -13.97 22.86) (end -13.97 3.81) (layer F.Fab) (width 0.15))
  (fp_line (start 13.97 22.86) (end -13.97 22.86) (layer F.Fab) (width 0.15))
  (fp_line (start 13.97 3.81) (end 13.97 22.86) (layer F.Fab) (width 0.15))
  (fp_line (start -13.97 3.81) (end 13.97 3.81) (layer F.Fab) (width 0.15))
  (fp_line (start -15.24 30.48) (end -15.24 -2.54) (layer F.Fab) (width 0.15))
  (fp_line (start 15.24 30.48) (end -15.24 30.48) (layer F.Fab) (width 0.15))
  (fp_line (start 15.24 -2.54) (end 15.24 30.48) (layer F.Fab) (width 0.15))
  (fp_line (start -15.24 -2.54) (end 15.24 -2.54) (layer F.Fab) (width 0.15))
  (fp_line (start -9.37 -1.75) (end -9.37 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.38 -1.75) (end 9.38 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.37 -1.75) (end 9.38 -1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -9.37 1.75) (end 9.38 1.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -6.35 1.27) (end 8.89 1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.89 1.27) (end 8.89 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start 8.89 -1.27) (end -6.35 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.17 1.55) (end -7.62 1.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.35 1.27) (end -6.35 -1.27) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.62 -1.55) (end -9.17 -1.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -9.17 -1.55) (end -9.17 1.55) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at -7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at -5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at -2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x07.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
