(module Crystals:Crystal_SMD_7050_4Pads (layer F.Cu) (tedit 58EE0D05)
  (descr "Crystal oscillator, 7.0x5.0mm, 4 Pads")
  (tags "crystal oscillator quartz SMD SMT 7050")
  (attr smd)
  (fp_text reference Y1 (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value FNETHE025 (at 0 4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.5 2.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 2.5) (end -3.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 -2.5) (end 3.5 2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.5 -2.5) (end 3.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.6 2.3) (end -4.15 2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 2.6) (end 3.6 2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 -2.6) (end 3.6 -2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 -2.6) (end -3.6 -2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 2.6) (end -3.6 2.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 2.6) (end 3.6 2.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 0.2) (end -4.15 0.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.75 -3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.75 -3.1) (end -4.75 -3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 -2.6) (end 3.6 -2.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.6 0.2) (end 3.6 -0.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.6 0.2) (end -3.6 -0.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.75 3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.75 -3.1) (end 4.75 3.1) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -3.15 1.25) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.15 1.25) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 3.15 -1.25) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -3.15 -1.25) (size 2.2 1.4) (layers F.Cu F.Paste F.Mask))
)
