EESchema-DOCLIB  Version 2.0
#
$CMP FXMA108
D Dual-Supply, 8-Bit Signal Translator with Configurable Voltage Supplies and Signals Levels, 3-State Outputs and Auto Direction Sensing, WQFN-20
K Level shifter translator bidirectional
F http://www.onsemi.com/pub/Collateral/FXMA108-D.pdf
$ENDCMP
#
$CMP SN74AUP1T34DCK
D 1-Bit Unidirectional Voltage-Level Translator
K Level Translator 1-bit Unidirectional Noninverting
F http://www.ti.com/lit/ds/symlink/sn74aup1t34.pdf
$ENDCMP
#
$CMP TXB0102DCT
D 2-Bit Bidirectional Voltage-Level Translator in TSSOP Package With Auto Direction Sensing and ±15-kV ESD Protection
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0102.pdf
$ENDCMP
#
$CMP TXB0102DCU
D 2-Bit Bidirectional Voltage-Level Translator in VSSOP Package With Auto Direction Sensing and ±15-kV ESD Protection
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0102.pdf
$ENDCMP
#
$CMP TXB0102YZP
D 2-Bit Bidirectional Voltage-Level Translator in DSBGA Package  With Auto Direction Sensing and ±15-kV ESD Protection
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0102.pdf
$ENDCMP
#
$CMP TXB0104D
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, SOIC-14
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0104PW
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, TSSOP-14
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0104RGY
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, Texas_PVGFN-14
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0104RUT
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, Texas_PUQFN-12
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0104YZT
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, DSBGA-12
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0104ZXU
D 4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6 V APort, 1.65 - 5.5 V BPort, Texas_Junior-12
K Level-Shifter CMOS-TTL-Translation
F http://www.ti.com/lit/ds/symlink/txb0104.pdf
$ENDCMP
#
$CMP TXB0108DQSR
D 8-bit bidirectional voltage level translator with auto-direction sensing USON package
K bidirectional voltage level translator
F http://www.ti.com/lit/ds/symlink/txb0108.pdf
$ENDCMP
#
#End Doc Library
