(module J_NC_0402 (layer F.Cu) (tedit 562D3DBA)
  (descr "Jumper N-O SMD 0402")
  (tags "jumper 0402")
  (attr smd)
  (fp_text reference REF** (at 0 -1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value J_0402 (at 0 1.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1 -0.8) (end -1 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 -0.8) (end -1 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1 0.8) (end 1 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 0.8) (end 1 -0.8) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -0.5 0) (size 0.6 1.2) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 0.5 0) (size 0.6 1.2) (layers F.Cu F.Mask))
  (pad 3 smd rect (at 0 0) (size 0.4 0.3) (layers F.Cu F.Mask))
)
