(module USB_A_SOCKET (layer F.Cu) (tedit 562C296A)
  (descr "USB A socket Amphenol UE27 right-angle thru")
  (tags "USB USB_A")
  (fp_text reference REF** (at 0 -2.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_SOCKET (at 3.5 6.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 10 4.5) (end 10 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 4.5) (end -3 7.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -1) (end 10 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 -1) (end 10 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -1) (end -3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -1) (end -3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
  (pad 4 thru_hole circle (at 7 0 270) (size 1.50114 1.50114) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 4.5 0 270) (size 1.50114 1.50114) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.5 0 270) (size 1.50114 1.50114) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 0 0 270) (size 1.50114 1.50114) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 10.07 2.71 270) (size 2.8 2.8) (drill 2.3) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -3.07 2.71 270) (size 2.8 2.8) (drill 2.3) (layers *.Cu *.Mask F.SilkS))
)
