(module SW_TACT (layer F.Cu) (tedit 562C3E17)
  (descr "Tactile switch 6x6mm thru")
  (fp_text reference REF** (at 0 -4.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_TACT (at 0 4.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 -1) (end -3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.5 -3) (end -2.5 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 1) (end 3 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5 3) (end 2.5 3) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 0 -1.755) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 3.25 -2.25) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 3.25 2.25) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -3.25 -2.25) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -3.25 2.25) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask F.SilkS))
)
