(export (version D)
  (design
    (source /home/me/USBdevel/USG/Git/Hardware/USG.sch)
    (date "Mon 26 Oct 2015 22:32:00 NZDT")
    (tool "Eeschema (2015-10-16 BZR 6271)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source USG.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value STM32F401xB)
      (footprint USG_footprints:LQFP-64_10x10mm_Pitch0.5mm)
      (libsource (lib USG_parts) (part STM32F401xB))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628A3CA))
    (comp (ref C9)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628BC20))
    (comp (ref C10)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628C063))
    (comp (ref C11)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628C0A3))
    (comp (ref C12)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628C0CC))
    (comp (ref C13)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628C140))
    (comp (ref C5)
      (value 4.7u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628C5AD))
    (comp (ref C8)
      (value 4.7u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628CBAA))
    (comp (ref C2)
      (value 18p)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628CF9A))
    (comp (ref C3)
      (value 18p)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628D0DA))
    (comp (ref R5)
      (value 220)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628D2EB))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystals:Crystal_HC49-SD_SMD)
      (libsource (lib device) (part Crystal_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628D59F))
    (comp (ref U3)
      (value AZ1117CH-3.3)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib regul) (part AP1117))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628E5FD))
    (comp (ref C15)
      (value 22u)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628ECAB))
    (comp (ref C14)
      (value 10u)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5628ED71))
    (comp (ref P1)
      (value USB_A_PLUG)
      (footprint USG_footprints:USB_A_PLUG)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5629023B))
    (comp (ref R4)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 5629EF83))
    (comp (ref R2)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 5629F905))
    (comp (ref C1)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5629F00B))
    (comp (ref BOOT_UPST1)
      (value Jumper_NO_Small)
      (footprint USG_footprints:J_NO_0402)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562A0390))
    (comp (ref R6)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562AE813))
    (comp (ref R8)
      (value 22)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562AF0F6))
    (comp (ref R7)
      (value 22)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562AFBCB))
    (comp (ref C7)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B08FA))
    (comp (ref U1)
      (value NUP4114)
      (footprint TO_SOT_Packages_SMD:SC-70-6)
      (libsource (lib USG_parts) (part NUP4114))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B0EC7))
    (comp (ref C6)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B50DC))
    (comp (ref JTAG_UPST1)
      (value CONN_02X05)
      (footprint USG_footprints:Pin_Header_Straight_2x05_Pitch1.27mm)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B573D))
    (comp (ref R1)
      (value 220)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B1E82))
    (comp (ref C4)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B2023))
    (comp (ref FAULT_UPST1)
      (value LED)
      (footprint LEDs:LED-0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B2CC0))
    (comp (ref R3)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562B2DE7))
    (comp (ref ID_UPST1)
      (value Jumper_NO_Small)
      (footprint USG_footprints:J_NO_0402)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BA570))
    (comp (ref ID_UPST_BOARD0)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BA5EC))
    (comp (ref ID_UPST_BOARD1)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BA662))
    (comp (ref ID_UPST_BOARD2)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BA6DF))
    (comp (ref U4)
      (value STM32F401xB)
      (footprint USG_footprints:LQFP-64_10x10mm_Pitch0.5mm)
      (libsource (lib USG_parts) (part STM32F401xB))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE700))
    (comp (ref C21)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE706))
    (comp (ref C22)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE712))
    (comp (ref C23)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE718))
    (comp (ref C24)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE71E))
    (comp (ref C25)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE724))
    (comp (ref C19)
      (value 4.7u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE730))
    (comp (ref C20)
      (value 4.7u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE748))
    (comp (ref C17)
      (value 18p)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE754))
    (comp (ref C18)
      (value 18p)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE75A))
    (comp (ref R12)
      (value 220)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE760))
    (comp (ref Y2)
      (value 8MHz)
      (footprint Crystals:Crystal_HC49-SD_SMD)
      (libsource (lib device) (part Crystal_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE766))
    (comp (ref P2)
      (value USB_A_SOCKET)
      (footprint USG_footprints:USB_A_SOCKET)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE77E))
    (comp (ref R11)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE790))
    (comp (ref R9)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7A2))
    (comp (ref C16)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7A8))
    (comp (ref BOOT_DNST1)
      (value Jumper_NO_Small)
      (footprint USG_footprints:J_NO_0402)
      (libsource (lib device) (part Jumper_NO_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7AE))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7C0))
    (comp (ref R15)
      (value 22)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7C6))
    (comp (ref R14)
      (value 22)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7DE))
    (comp (ref C27)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7EA))
    (comp (ref U5)
      (value NUP4114)
      (footprint TO_SOT_Packages_SMD:SC-70-6)
      (libsource (lib USG_parts) (part NUP4114))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE7FC))
    (comp (ref C26)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE802))
    (comp (ref JTAG_DNST1)
      (value CONN_02X05)
      (footprint USG_footprints:Pin_Header_Straight_2x05_Pitch1.27mm)
      (libsource (lib conn) (part CONN_02X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE814))
    (comp (ref R16)
      (value 220)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE89E))
    (comp (ref C28)
      (value 0.1u)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8A4))
    (comp (ref FAULT_DNST1)
      (value LED)
      (footprint LEDs:LED-0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8B2))
    (comp (ref R10)
      (value 1k)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib USG_parts) (part RR))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8B8))
    (comp (ref ID_DNST1)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8C7))
    (comp (ref ID_DNST_BOARD0)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8CD))
    (comp (ref ID_DNST_BOARD1)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8D3))
    (comp (ref ID_DNST_BOARD2)
      (value Jumper_NC_Small)
      (footprint USG_footprints:J_NC_0402)
      (libsource (lib device) (part Jumper_NC_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 562BE8D9))
    (comp (ref D1)
      (value DOUBLE_DIODE_CCOM)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib USG_parts) (part DOUBLE_DIODE_CCOM))
      (sheetpath (names /) (tstamps /))
      (tstamp 562D027C))
    (comp (ref RESET1)
      (value SW_PUSH)
      (footprint USG_footprints:SW_TACT)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 562D2889))
    (comp (ref P3)
      (value USB_OTG)
      (footprint Connect:USB_Micro-B)
      (libsource (lib conn) (part USB_OTG))
      (sheetpath (names /) (tstamps /))
      (tstamp 562D02AE)))
  (libparts
    (libpart (lib conn) (part CONN_02X05)
      (footprints
        (fp Pin_Header_Straight_2X05)
        (fp Pin_Header_Angled_2X05)
        (fp Socket_Strip_Straight_2X05)
        (fp Socket_Strip_Angled_2X05))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))))
    (libpart (lib conn) (part USB_A)
      (description "A connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name shield) (type passive))))
    (libpart (lib conn) (part USB_OTG)
      (description "micro/mini connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_OTG))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name shield) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal_Small)
      (description "Two pin crystal")
      (footprints
        (fp Crystal_))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Jumper_NC_Small)
      (description "Jumper normally close")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part Jumper_NO_Small)
      (description "Jumper normally open")
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NO_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description Button)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib regul) (part AP1117)
      (aliases
        (alias AP1117D15)
        (alias AP1117D18)
        (alias AP1117D25)
        (alias AP1117D33)
        (alias AP1117D50)
        (alias AP1117E15)
        (alias AP1117E18)
        (alias AP1117E25)
        (alias AP1117E33)
        (alias AP1117E50)
        (alias AP1117K15)
        (alias AP1117K18)
        (alias AP1117K25)
        (alias AP1117K33)
        (alias AP1117K50)
        (alias AP1117T15)
        (alias AP1117T18)
        (alias AP1117T25)
        (alias AP1117T33)
        (alias AP1117T50)
        (alias AP1117Y15)
        (alias AP1117Y18)
        (alias AP1117Y25)
        (alias AP1117Y33)
        (alias AP1117Y50))
      (description "Fixed/Adjustable 1A Low Dropout regulator, Positive")
      (docs http://www.diodes.com/datasheets/AP1117.pdf)
      (footprints
        (fp SOT223)
        (fp SOT89-3)
        (fp TO220-3)
        (fp TO252)
        (fp TO263))
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib USG_parts) (part DOUBLE_DIODE_CCOM)
      (fields
        (field (name Reference) D)
        (field (name Value) DOUBLE_DIODE_CCOM))
      (pins
        (pin (num 1) (name Anode) (type passive))
        (pin (num 2) (name cathode) (type passive))
        (pin (num 3) (name AK) (type passive))))
    (libpart (lib USG_parts) (part NUP4114)
      (fields
        (field (name Reference) U)
        (field (name Value) NUP4114))
      (pins
        (pin (num 1) (name IO1) (type BiDi))
        (pin (num 2) (name GND) (type BiDi))
        (pin (num 3) (name IO3) (type BiDi))
        (pin (num 4) (name IO4) (type BiDi))
        (pin (num 5) (name Vcc) (type BiDi))
        (pin (num 6) (name IO2) (type BiDi))))
    (libpart (lib USG_parts) (part RR)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) RR))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib USG_parts) (part STM32F401xB)
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F401xB)
        (field (name Footprint) LQFP64))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13/RTC_TAMP1) (type BiDi))
        (pin (num 3) (name PC14/OSC32_IN) (type BiDi))
        (pin (num 4) (name PC15/OSC32_OUT) (type BiDi))
        (pin (num 5) (name PH0/OSC_IN) (type input))
        (pin (num 6) (name PH1/OSC_OUT) (type output))
        (pin (num 7) (name ~NRST) (type BiDi))
        (pin (num 8) (name PC0/ADC1_IN10) (type BiDi))
        (pin (num 9) (name PC1/ADC1_IN11) (type BiDi))
        (pin (num 10) (name PC2/ADC1_IN12/SPI2_MISO) (type BiDi))
        (pin (num 11) (name PC3/ADC1_IN13/SPI2_MOSI) (type BiDi))
        (pin (num 12) (name VSSA/VREF-) (type power_in))
        (pin (num 13) (name VDDA/VREF+) (type power_in))
        (pin (num 14) (name USART2_CTS/TIM2_CH1/TIM2_ETR/TIM5_CH1/WKUP/ADC1_IN0/PA0) (type BiDi))
        (pin (num 15) (name USART2_RTS/TIM2_CH2/TIM5_CH2/ADC1_IN1/PA1) (type BiDi))
        (pin (num 16) (name USART2_TX/TIM2_CH3/TIM5_CH3/TIM9_CH1/ADC1_IN2/PA2) (type BiDi))
        (pin (num 17) (name USART2_RX/TIM2_CH4/TIM5_CH4/TIM9_CH2/ADC1_IN3/PA3) (type BiDi))
        (pin (num 18) (name VSS) (type power_in))
        (pin (num 19) (name VDD) (type power_in))
        (pin (num 20) (name SPI1_NSS/SPI3_NSS/I2S3_WS/USART2_CK/ADC1_IN4/PA4) (type BiDi))
        (pin (num 21) (name SPI1_SCK/TIM2_CH1/TIM2_ETR/ADC1_IN5/PA5) (type BiDi))
        (pin (num 22) (name SPI1_MISO/TIM1_BKIN/TIM3_CH1/ADC1_IN6/PA6) (type BiDi))
        (pin (num 23) (name SPI1_MOSI/TIM1_CH1N/TIM3_CH2/ADC1_IN7/PA7) (type BiDi))
        (pin (num 24) (name PC4/ADC1_IN14) (type BiDi))
        (pin (num 25) (name PC5/ADC1_IN15) (type BiDi))
        (pin (num 26) (name TIM1_CH2N/TIM3_CH3/ADC1_IN8/PB0) (type BiDi))
        (pin (num 27) (name TIM1_CH3N/TIM3_CH4/ADC1_IN9/PB1) (type BiDi))
        (pin (num 28) (name BOOT1/PB2) (type BiDi))
        (pin (num 29) (name SPI2_SCK/I2S2_CK/I2C2_SCL/TIM2_CH3/PB10) (type BiDi))
        (pin (num 30) (name VCAP_1) (type BiDi))
        (pin (num 31) (name VSS) (type power_in))
        (pin (num 32) (name VDD) (type power_in))
        (pin (num 33) (name SPI2_NSS/I2S2_WS/I2C2_SMBA/TIM1_BKIN/PB12) (type BiDi))
        (pin (num 34) (name SPI2_SCK/I2S2_CK/TIM1_CH1N/PB13) (type BiDi))
        (pin (num 35) (name SPI2_MISO/I2S2ext_SD/TIM1_CH2N/PB14) (type BiDi))
        (pin (num 36) (name SPI2_MOSI/I2S2_SD/TIM1_CH3N/RTC_REFIN/PB15) (type BiDi))
        (pin (num 37) (name PC6/I2S2_MCK/USART6_TX/TIM3_CH1/SDIO_D6) (type BiDi))
        (pin (num 38) (name PC7/I2S3_MCK/USART6_RX/TIM3_CH2/SDIO_D7) (type BiDi))
        (pin (num 39) (name PC8/USART6_CK/TIM3_CH3/SDIO_D0) (type BiDi))
        (pin (num 40) (name PC9/I2S_CKIN/I2C3_SDA/TIM3_CH4/SDIO_D1/MCO_2) (type BiDi))
        (pin (num 41) (name I2C3_SCL/USART1_CK/TIM1_CH1/OTG_FS_SOF/MCO_1/PA8) (type BiDi))
        (pin (num 42) (name I2C3_SMBA/USART1_TX/TIM1_CH2/OTG_FS_VBUS/PA9) (type BiDi))
        (pin (num 43) (name USART1_RX/TIM1_CH3/OTG_FS_ID/PA10) (type BiDi))
        (pin (num 44) (name USART1_CTS/USART6_TX/TIM1_CH4/OTG_FS_DM/PA11) (type BiDi))
        (pin (num 45) (name USART1_RTS/USART6_RX/TIM1_ETR/OTG_FS_DP/PA12) (type BiDi))
        (pin (num 46) (name JTMS-SWDIO/PA13) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))
        (pin (num 49) (name JTCK-SWCLK/PA14) (type BiDi))
        (pin (num 50) (name JTDI/SPI1_NSS/SPI3_NSS/I2S3_WS/TIM2_CH1/TIM2_ETR/PA15) (type BiDi))
        (pin (num 51) (name PC10/SPI3_SCK/I2S3_CK/SDIO_D2) (type BiDi))
        (pin (num 52) (name PC11/I2S3ext_SD/SPI3_MISO/SDIO_D3) (type BiDi))
        (pin (num 53) (name PC12/SPI3_MOSI/I2S3_SD/SDIO_CK) (type BiDi))
        (pin (num 54) (name PD2/TIM3_ETR/SDIO_CMD) (type BiDi))
        (pin (num 55) (name JTDO-SWO/SPI1_SCK/SPI3_SCK/I2S3_CK/I2C2_SDA/TIM2_CH2/PB3) (type BiDi))
        (pin (num 56) (name NJTRST/SPI1_MISO/SPI3_MISO/I2S3ext_SD/I2C3_SDA/TIM3_CH1/PB4) (type BiDi))
        (pin (num 57) (name SPI1_MOSI/SPI3_MOSI/I2S3_SD/I2C1_SMBA/TIM3_CH2/PB5) (type BiDi))
        (pin (num 58) (name I2C1_SCL/USART1_TX/TIM4_CH1/PB6) (type BiDi))
        (pin (num 59) (name I2C1_SDA/USART1_RX/TIM4_CH2/PB7) (type BiDi))
        (pin (num 60) (name BOOT0/Vpp) (type BiDi))
        (pin (num 61) (name I2C1_SCL/TIM4_CH3/TIM10_CH1/SDIO_D4/PB8) (type BiDi))
        (pin (num 62) (name SPI2_NSS/I2S2_WS/I2C1_SDA/TIM4_CH4/TIM11_CH1/SDIO_D5/PB9) (type BiDi))
        (pin (num 63) (name VSS) (type power_in))
        (pin (num 64) (name VDD) (type power_in)))))
  (libraries
    (library (logical conn)
      (uri /usr/local/share/kicad/library/conn.lib))
    (library (logical device)
      (uri /usr/local/share/kicad/library/device.lib))
    (library (logical regul)
      (uri /usr/local/share/kicad/library/regul.lib))
    (library (logical USG_parts)
      (uri /home/me/USBdevel/USG/Git/Hardware/USG_parts.lib)))
  (nets
    (net (code 1) (name "Net-(BOOT_UPST1-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref BOOT_UPST1) (pin 1)))
    (net (code 2) (name "Net-(R6-Pad1)")
      (node (ref U2) (pin 60))
      (node (ref R6) (pin 1)))
    (net (code 3) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 4) (name "Net-(P1-Pad2)")
      (node (ref U1) (pin 6))
      (node (ref P1) (pin 2))
      (node (ref R7) (pin 1))
      (node (ref P3) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 5) (name "Net-(P1-Pad3)")
      (node (ref P3) (pin 3))
      (node (ref R8) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref P1) (pin 3))
      (node (ref U1) (pin 4)))
    (net (code 6) (name "Net-(R7-Pad2)")
      (node (ref R7) (pin 2))
      (node (ref U2) (pin 44)))
    (net (code 7) (name "Net-(R8-Pad2)")
      (node (ref R8) (pin 2))
      (node (ref U2) (pin 45)))
    (net (code 8) (name +3V3)
      (node (ref C7) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref C25) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref C23) (pin 2))
      (node (ref BOOT_UPST1) (pin 2))
      (node (ref JTAG_DNST1) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref U4) (pin 19))
      (node (ref C22) (pin 2))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 32))
      (node (ref C15) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 48))
      (node (ref U2) (pin 56))
      (node (ref U2) (pin 19))
      (node (ref C8) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref U2) (pin 64))
      (node (ref C20) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref BOOT_DNST1) (pin 2))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 32))
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 56))
      (node (ref U4) (pin 64))
      (node (ref FAULT_UPST1) (pin 2))
      (node (ref C27) (pin 1))
      (node (ref FAULT_DNST1) (pin 2))
      (node (ref JTAG_UPST1) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref U4) (pin 48)))
    (net (code 9) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 10) (name "Net-(FAULT_DNST1-Pad1)")
      (node (ref FAULT_DNST1) (pin 1))
      (node (ref R10) (pin 2)))
    (net (code 11) (name "Net-(ID_DNST1-Pad2)")
      (node (ref U4) (pin 11))
      (node (ref ID_DNST1) (pin 2)))
    (net (code 12) (name "Net-(ID_DNST_BOARD0-Pad2)")
      (node (ref ID_DNST_BOARD0) (pin 2))
      (node (ref U4) (pin 8)))
    (net (code 13) (name "Net-(ID_DNST_BOARD1-Pad2)")
      (node (ref ID_DNST_BOARD1) (pin 2))
      (node (ref U4) (pin 9)))
    (net (code 14) (name /JTCK_DNST)
      (node (ref U4) (pin 49))
      (node (ref JTAG_DNST1) (pin 4)))
    (net (code 15) (name GND)
      (node (ref JTAG_UPST1) (pin 5))
      (node (ref JTAG_UPST1) (pin 3))
      (node (ref JTAG_UPST1) (pin 7))
      (node (ref C6) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref P1) (pin 4))
      (node (ref C14) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref P2) (pin 4))
      (node (ref U5) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C25) (pin 1))
      (node (ref U4) (pin 63))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 31))
      (node (ref U4) (pin 28))
      (node (ref U4) (pin 18))
      (node (ref U4) (pin 47))
      (node (ref ID_UPST1) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref C24) (pin 1))
      (node (ref ID_UPST_BOARD0) (pin 1))
      (node (ref ID_UPST_BOARD2) (pin 1))
      (node (ref ID_UPST_BOARD1) (pin 1))
      (node (ref U2) (pin 31))
      (node (ref C8) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 63))
      (node (ref C7) (pin 2))
      (node (ref C23) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref C17) (pin 2))
      (node (ref JTAG_UPST1) (pin 9))
      (node (ref C20) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref U2) (pin 28))
      (node (ref U2) (pin 18))
      (node (ref U2) (pin 47))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref JTAG_DNST1) (pin 7))
      (node (ref JTAG_DNST1) (pin 9))
      (node (ref JTAG_DNST1) (pin 5))
      (node (ref ID_DNST_BOARD1) (pin 1))
      (node (ref ID_DNST_BOARD0) (pin 1))
      (node (ref ID_DNST1) (pin 1))
      (node (ref P3) (pin 5))
      (node (ref ID_DNST_BOARD2) (pin 1))
      (node (ref C28) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref JTAG_DNST1) (pin 3))
      (node (ref RESET1) (pin 1)))
    (net (code 16) (name +5V)
      (node (ref C26) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref P3) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref P1) (pin 1)))
    (net (code 17) (name /JTMS_DNST)
      (node (ref JTAG_DNST1) (pin 2))
      (node (ref U4) (pin 46)))
    (net (code 18) (name "Net-(ID_DNST_BOARD2-Pad2)")
      (node (ref ID_DNST_BOARD2) (pin 2))
      (node (ref U4) (pin 10)))
    (net (code 19) (name /JTDO_DNST)
      (node (ref U4) (pin 55))
      (node (ref JTAG_DNST1) (pin 6)))
    (net (code 20) (name /JTDI_DNST)
      (node (ref JTAG_DNST1) (pin 8))
      (node (ref U4) (pin 50)))
    (net (code 21) (name /RESET_DNST)
      (node (ref D1) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref C16) (pin 1))
      (node (ref R11) (pin 2))
      (node (ref JTAG_DNST1) (pin 10)))
    (net (code 22) (name "Net-(C5-Pad1)")
      (node (ref U2) (pin 30))
      (node (ref C5) (pin 1)))
    (net (code 23) (name /RESET_UPST)
      (node (ref D1) (pin 2))
      (node (ref JTAG_UPST1) (pin 10))
      (node (ref R4) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 24) (name "Net-(D1-Pad3)")
      (node (ref D1) (pin 3))
      (node (ref RESET1) (pin 2)))
    (net (code 25) (name /SPI_TX_OK)
      (node (ref U4) (pin 17))
      (node (ref U2) (pin 17)))
    (net (code 26) (name /SPI_NSS)
      (node (ref U4) (pin 20))
      (node (ref U2) (pin 20)))
    (net (code 27) (name /SPI_SCK)
      (node (ref U4) (pin 21))
      (node (ref U2) (pin 21)))
    (net (code 28) (name /SPI_MISO)
      (node (ref U4) (pin 22))
      (node (ref U2) (pin 22)))
    (net (code 29) (name /SPI_MOSI)
      (node (ref U2) (pin 23))
      (node (ref U4) (pin 23)))
    (net (code 30) (name "Net-(R14-Pad2)")
      (node (ref U4) (pin 44))
      (node (ref R14) (pin 2)))
    (net (code 31) (name "Net-(R15-Pad2)")
      (node (ref R15) (pin 2))
      (node (ref U4) (pin 45)))
    (net (code 32) (name "Net-(P3-Pad4)")
      (node (ref P3) (pin 4)))
    (net (code 33) (name "Net-(C19-Pad1)")
      (node (ref C19) (pin 1))
      (node (ref U4) (pin 30)))
    (net (code 34) (name "Net-(R12-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 35) (name "Net-(FAULT_UPST1-Pad1)")
      (node (ref FAULT_UPST1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 36) (name "Net-(R3-Pad1)")
      (node (ref U2) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 37) (name "Net-(ID_UPST_BOARD0-Pad2)")
      (node (ref ID_UPST_BOARD0) (pin 2))
      (node (ref U2) (pin 8)))
    (net (code 38) (name "Net-(ID_UPST_BOARD1-Pad2)")
      (node (ref ID_UPST_BOARD1) (pin 2))
      (node (ref U2) (pin 9)))
    (net (code 39) (name "Net-(ID_UPST_BOARD2-Pad2)")
      (node (ref ID_UPST_BOARD2) (pin 2))
      (node (ref U2) (pin 10)))
    (net (code 40) (name "Net-(ID_UPST1-Pad2)")
      (node (ref ID_UPST1) (pin 2))
      (node (ref U2) (pin 11)))
    (net (code 41) (name "Net-(P2-Pad3)")
      (node (ref U5) (pin 4))
      (node (ref P2) (pin 3))
      (node (ref U5) (pin 3))
      (node (ref R15) (pin 1)))
    (net (code 42) (name "Net-(P2-Pad2)")
      (node (ref R14) (pin 1))
      (node (ref U5) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref U5) (pin 6)))
    (net (code 43) (name "Net-(BOOT_DNST1-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref BOOT_DNST1) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 44) (name "Net-(R13-Pad1)")
      (node (ref U4) (pin 60))
      (node (ref R13) (pin 1)))
    (net (code 45) (name "Net-(C4-Pad1)")
      (node (ref P3) (pin 6))
      (node (ref C4) (pin 1))
      (node (ref P1) (pin 5))
      (node (ref R1) (pin 1)))
    (net (code 46) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 47) (name "Net-(C3-Pad1)")
      (node (ref R5) (pin 2))
      (node (ref Y1) (pin 2))
      (node (ref C3) (pin 1)))
    (net (code 48) (name "Net-(U2-Pad34)")
      (node (ref U2) (pin 34)))
    (net (code 49) (name "Net-(U2-Pad42)")
      (node (ref U2) (pin 42)))
    (net (code 50) (name "Net-(U2-Pad52)")
      (node (ref U2) (pin 52)))
    (net (code 51) (name "Net-(U2-Pad62)")
      (node (ref U2) (pin 62)))
    (net (code 52) (name "Net-(U2-Pad33)")
      (node (ref U2) (pin 33)))
    (net (code 53) (name "Net-(U2-Pad43)")
      (node (ref U2) (pin 43)))
    (net (code 54) (name "Net-(U2-Pad53)")
      (node (ref U2) (pin 53)))
    (net (code 55) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 56) (name "Net-(U2-Pad24)")
      (node (ref U2) (pin 24)))
    (net (code 57) (name "Net-(U2-Pad54)")
      (node (ref U2) (pin 54)))
    (net (code 58) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 59) (name "Net-(U2-Pad25)")
      (node (ref U2) (pin 25)))
    (net (code 60) (name "Net-(U2-Pad35)")
      (node (ref U2) (pin 35)))
    (net (code 61) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 62) (name "Net-(U2-Pad26)")
      (node (ref U2) (pin 26)))
    (net (code 63) (name "Net-(U2-Pad36)")
      (node (ref U2) (pin 36)))
    (net (code 64) (name "Net-(U2-Pad40)")
      (node (ref U2) (pin 40)))
    (net (code 65) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 66) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 67) (name "Net-(U2-Pad41)")
      (node (ref U2) (pin 41)))
    (net (code 68) (name "Net-(U2-Pad51)")
      (node (ref U2) (pin 51)))
    (net (code 69) (name "Net-(U2-Pad61)")
      (node (ref U2) (pin 61)))
    (net (code 70) (name "Net-(U2-Pad27)")
      (node (ref U2) (pin 27)))
    (net (code 71) (name "Net-(U2-Pad37)")
      (node (ref U2) (pin 37)))
    (net (code 72) (name "Net-(U2-Pad57)")
      (node (ref U2) (pin 57)))
    (net (code 73) (name "Net-(U2-Pad38)")
      (node (ref U2) (pin 38)))
    (net (code 74) (name "Net-(U2-Pad58)")
      (node (ref U2) (pin 58)))
    (net (code 75) (name "Net-(U2-Pad29)")
      (node (ref U2) (pin 29)))
    (net (code 76) (name "Net-(U2-Pad39)")
      (node (ref U2) (pin 39)))
    (net (code 77) (name "Net-(U2-Pad59)")
      (node (ref U2) (pin 59)))
    (net (code 78) (name "Net-(C17-Pad1)")
      (node (ref C17) (pin 1))
      (node (ref Y2) (pin 1))
      (node (ref U4) (pin 5)))
    (net (code 79) (name "Net-(C18-Pad1)")
      (node (ref Y2) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref C18) (pin 1)))
    (net (code 80) (name "Net-(U4-Pad58)")
      (node (ref U4) (pin 58)))
    (net (code 81) (name "Net-(U4-Pad29)")
      (node (ref U4) (pin 29)))
    (net (code 82) (name "Net-(U4-Pad39)")
      (node (ref U4) (pin 39)))
    (net (code 83) (name "Net-(U4-Pad59)")
      (node (ref U4) (pin 59)))
    (net (code 84) (name "Net-(C28-Pad1)")
      (node (ref R16) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref P2) (pin 5)))
    (net (code 85) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 86) (name "Net-(U4-Pad4)")
      (node (ref U4) (pin 4)))
    (net (code 87) (name /JTMS_UPST)
      (node (ref JTAG_UPST1) (pin 2))
      (node (ref U2) (pin 46)))
    (net (code 88) (name /JTCK_UPST)
      (node (ref JTAG_UPST1) (pin 4))
      (node (ref U2) (pin 49)))
    (net (code 89) (name /JTDO_UPST)
      (node (ref JTAG_UPST1) (pin 6))
      (node (ref U2) (pin 55)))
    (net (code 90) (name /JTDI_UPST)
      (node (ref JTAG_UPST1) (pin 8))
      (node (ref U2) (pin 50)))
    (net (code 91) (name "Net-(U4-Pad26)")
      (node (ref U4) (pin 26)))
    (net (code 92) (name "Net-(U4-Pad24)")
      (node (ref U4) (pin 24)))
    (net (code 93) (name "Net-(U4-Pad34)")
      (node (ref U4) (pin 34)))
    (net (code 94) (name "Net-(U4-Pad54)")
      (node (ref U4) (pin 54)))
    (net (code 95) (name "Net-(U4-Pad15)")
      (node (ref U4) (pin 15)))
    (net (code 96) (name "Net-(U4-Pad25)")
      (node (ref U4) (pin 25)))
    (net (code 97) (name "Net-(U4-Pad35)")
      (node (ref U4) (pin 35)))
    (net (code 98) (name "Net-(U4-Pad16)")
      (node (ref U4) (pin 16)))
    (net (code 99) (name "Net-(U4-Pad14)")
      (node (ref U4) (pin 14)))
    (net (code 100) (name "Net-(U4-Pad36)")
      (node (ref U4) (pin 36)))
    (net (code 101) (name "Net-(U4-Pad27)")
      (node (ref U4) (pin 27)))
    (net (code 102) (name "Net-(U4-Pad37)")
      (node (ref U4) (pin 37)))
    (net (code 103) (name "Net-(U4-Pad57)")
      (node (ref U4) (pin 57)))
    (net (code 104) (name "Net-(U4-Pad38)")
      (node (ref U4) (pin 38)))
    (net (code 105) (name "Net-(U4-Pad40)")
      (node (ref U4) (pin 40)))
    (net (code 106) (name "Net-(U4-Pad41)")
      (node (ref U4) (pin 41)))
    (net (code 107) (name "Net-(U4-Pad51)")
      (node (ref U4) (pin 51)))
    (net (code 108) (name "Net-(U4-Pad61)")
      (node (ref U4) (pin 61)))
    (net (code 109) (name "Net-(U4-Pad42)")
      (node (ref U4) (pin 42)))
    (net (code 110) (name "Net-(U4-Pad52)")
      (node (ref U4) (pin 52)))
    (net (code 111) (name "Net-(U4-Pad62)")
      (node (ref U4) (pin 62)))
    (net (code 112) (name "Net-(U4-Pad33)")
      (node (ref U4) (pin 33)))
    (net (code 113) (name "Net-(U4-Pad43)")
      (node (ref U4) (pin 43)))
    (net (code 114) (name "Net-(U4-Pad53)")
      (node (ref U4) (pin 53)))))