(module Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 562D3C6A)
  (descr "Through hole pin header, pitch 1.27mm, shrouded")
  (tags "pin header")
  (fp_text reference REF** (at 0.508 -4.826) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_02X05 (at 0 9.906) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.524 1.27) (end -1.524 3.81) (layer F.SilkS) (width 0.7))
  (fp_line (start -2.286 -4.064) (end 3.556 -4.064) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.556 -4.064) (end 3.556 9.144) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.556 9.144) (end -2.286 9.144) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.286 9.144) (end -2.286 -4.064) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.185 8.865) (end 3.185 -3.785) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.185 8.865) (end -1.915 8.865) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.915 8.865) (end -1.915 -3.785) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.185 -3.785) (end -1.915 -3.785) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 0 1.27) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 0 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at 0 3.81) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at 0 5.08) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 1.27 1.27) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 1.27 2.54) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at 1.27 3.81) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at 1.27 5.08) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 1.27 0) (size 1.05 1.05) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
)
