(export (version D)
  (design
    (source /home/antonlysak/KiCAD/wasd-keyboard/wasd-keyboard/wasd-keyboard.sch)
    (date "Thu 13 Feb 2020 00:57:54 +06")
    (tool "Eeschema 5.1.5-52549c5~84~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source wasd-keyboard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref SW1)
      (value Esc)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DDDC764))
    (comp (ref D1)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DDDC76A))
    (comp (ref R1)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DDDC778))
    (comp (ref SW2)
      (value Reserved)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E061D3E))
    (comp (ref D2)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E061D44))
    (comp (ref R2)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E061D52))
    (comp (ref SW3)
      (value F1)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E063555))
    (comp (ref D3)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E06355B))
    (comp (ref R3)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E063569))
    (comp (ref SW4)
      (value F2)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730CC))
    (comp (ref D4)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730D2))
    (comp (ref R4)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730E0))
    (comp (ref SW5)
      (value F3)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730EA))
    (comp (ref D5)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730F0))
    (comp (ref R5)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0730FE))
    (comp (ref SW6)
      (value F4)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E073108))
    (comp (ref D6)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E07310E))
    (comp (ref R6)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E07311C))
    (comp (ref SW7)
      (value F5)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B490))
    (comp (ref D7)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B496))
    (comp (ref R7)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4A4))
    (comp (ref SW8)
      (value F6)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4AE))
    (comp (ref D8)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4B4))
    (comp (ref R8)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4C2))
    (comp (ref SW9)
      (value F7)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4CC))
    (comp (ref D9)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4D2))
    (comp (ref R9)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B4E0))
    (comp (ref SW10)
      (value F8)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B508))
    (comp (ref D10)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B50E))
    (comp (ref R10)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B51C))
    (comp (ref SW11)
      (value F9)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B526))
    (comp (ref D11)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B52C))
    (comp (ref R11)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B53A))
    (comp (ref SW12)
      (value F10)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B544))
    (comp (ref D12)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B54A))
    (comp (ref R12)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E08B558))
    (comp (ref SW13)
      (value F11)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C14))
    (comp (ref D13)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C1A))
    (comp (ref R13)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C28))
    (comp (ref SW14)
      (value F12)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C32))
    (comp (ref D14)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C38))
    (comp (ref R14)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C46))
    (comp (ref SW15)
      (value PrScr)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C50))
    (comp (ref D15)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C56))
    (comp (ref R15)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C64))
    (comp (ref SW16)
      (value ScrLock)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C8C))
    (comp (ref D16)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9C92))
    (comp (ref R16)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CA0))
    (comp (ref SW17)
      (value Pause)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CAA))
    (comp (ref D17)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CB0))
    (comp (ref R17)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CBE))
    (comp (ref SW18)
      (value Tilde)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CC8))
    (comp (ref D18)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CCE))
    (comp (ref R18)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9CDC))
    (comp (ref SW19)
      (value 1)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D04))
    (comp (ref D19)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D0A))
    (comp (ref R19)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D18))
    (comp (ref SW20)
      (value 2)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D22))
    (comp (ref D20)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D28))
    (comp (ref R20)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D36))
    (comp (ref SW21)
      (value 3)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D40))
    (comp (ref D21)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D46))
    (comp (ref R21)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D54))
    (comp (ref SW22)
      (value 4)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D7C))
    (comp (ref D22)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D82))
    (comp (ref R22)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D90))
    (comp (ref SW23)
      (value 5)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9D9A))
    (comp (ref D23)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9DA0))
    (comp (ref R23)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9DAE))
    (comp (ref SW24)
      (value 6)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9DB8))
    (comp (ref D24)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9DBE))
    (comp (ref R24)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E0E9DCC))
    (comp (ref SW25)
      (value 7)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D868))
    (comp (ref D25)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D86E))
    (comp (ref R25)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D87C))
    (comp (ref SW26)
      (value 8)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8A4))
    (comp (ref D26)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8AA))
    (comp (ref R26)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8B8))
    (comp (ref SW27)
      (value 9)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8C2))
    (comp (ref D27)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8C8))
    (comp (ref R27)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8D6))
    (comp (ref SW28)
      (value 0)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8E0))
    (comp (ref D28)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8E6))
    (comp (ref R28)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D8F4))
    (comp (ref SW29)
      (value -)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D91C))
    (comp (ref D29)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D922))
    (comp (ref R29)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D930))
    (comp (ref SW30)
      (value +)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D93A))
    (comp (ref D30)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D940))
    (comp (ref R30)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D94E))
    (comp (ref SW31)
      (value "JIS |")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D958))
    (comp (ref D31)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D95E))
    (comp (ref R31)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D96C))
    (comp (ref SW32)
      (value "JIS Backspace")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D994))
    (comp (ref D32)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D99A))
    (comp (ref SW33)
      (value Ins)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9B2))
    (comp (ref D33)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9B8))
    (comp (ref R33)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9C6))
    (comp (ref SW34)
      (value Home)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9D0))
    (comp (ref D34)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9D6))
    (comp (ref R34)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9E4))
    (comp (ref SW35)
      (value PgUp)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA0C))
    (comp (ref D35)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA12))
    (comp (ref R35)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA20))
    (comp (ref SW36)
      (value Tab)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.50u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA2A))
    (comp (ref D36)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA30))
    (comp (ref R36)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA3E))
    (comp (ref SW37)
      (value Q)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA48))
    (comp (ref D37)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA4E))
    (comp (ref R37)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA5C))
    (comp (ref SW38)
      (value W)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA66))
    (comp (ref D38)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA6C))
    (comp (ref R38)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DA7A))
    (comp (ref SW39)
      (value E)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAA2))
    (comp (ref D39)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAA8))
    (comp (ref R39)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAB6))
    (comp (ref SW40)
      (value R)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAC0))
    (comp (ref D40)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAC6))
    (comp (ref R40)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAD4))
    (comp (ref SW41)
      (value T)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DADE))
    (comp (ref D41)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAE4))
    (comp (ref R41)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DAF2))
    (comp (ref SW42)
      (value Y)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB1A))
    (comp (ref D42)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB20))
    (comp (ref R42)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB2E))
    (comp (ref SW43)
      (value U)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB38))
    (comp (ref D43)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB3E))
    (comp (ref R43)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB4C))
    (comp (ref SW44)
      (value I)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB56))
    (comp (ref D44)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB5C))
    (comp (ref R44)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB6A))
    (comp (ref SW45)
      (value O)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB92))
    (comp (ref D45)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DB98))
    (comp (ref R45)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBA6))
    (comp (ref SW46)
      (value P)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBB0))
    (comp (ref D46)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBB6))
    (comp (ref R46)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBC4))
    (comp (ref SW47)
      (value [)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBCE))
    (comp (ref D47)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBD4))
    (comp (ref R47)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DBE2))
    (comp (ref SW48)
      (value ])
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DC0A))
    (comp (ref D48)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DC10))
    (comp (ref R48)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13DC1E))
    (comp (ref SW49)
      (value "ANSI \\")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.50u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6D82))
    (comp (ref D49)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6D88))
    (comp (ref R49)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6D96))
    (comp (ref SW50)
      (value Del)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DA0))
    (comp (ref D50)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DA6))
    (comp (ref R50)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DB4))
    (comp (ref SW51)
      (value End)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DBE))
    (comp (ref D51)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DC4))
    (comp (ref R51)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DD2))
    (comp (ref SW52)
      (value PgDown)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6DFA))
    (comp (ref D52)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E00))
    (comp (ref R52)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E0E))
    (comp (ref SW53)
      (value CapsLock)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.75u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E18))
    (comp (ref D53)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E1E))
    (comp (ref R53)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E2C))
    (comp (ref SW54)
      (value A)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E36))
    (comp (ref D54)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E3C))
    (comp (ref SW55)
      (value S)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E72))
    (comp (ref D55)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E78))
    (comp (ref R55)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E86))
    (comp (ref SW56)
      (value D)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E90))
    (comp (ref D56)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E96))
    (comp (ref R56)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EA4))
    (comp (ref SW57)
      (value F)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EAE))
    (comp (ref D57)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EB4))
    (comp (ref R57)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EC2))
    (comp (ref SW58)
      (value G)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EEA))
    (comp (ref D58)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EF0))
    (comp (ref R58)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6EFE))
    (comp (ref SW59)
      (value H)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F08))
    (comp (ref D59)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F0E))
    (comp (ref R59)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F1C))
    (comp (ref SW60)
      (value J)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F26))
    (comp (ref D60)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F2C))
    (comp (ref R60)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F3A))
    (comp (ref SW61)
      (value K)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F80))
    (comp (ref D61)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F86))
    (comp (ref R61)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F94))
    (comp (ref SW62)
      (value L)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6F9E))
    (comp (ref D62)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FA4))
    (comp (ref R62)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FB2))
    (comp (ref SW63)
      (value :)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FBC))
    (comp (ref D63)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FC2))
    (comp (ref R63)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FD0))
    (comp (ref SW64)
      (value "\"")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FF8))
    (comp (ref D64)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6FFE))
    (comp (ref R64)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A700C))
    (comp (ref SW65)
      (value "ISO #")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7016))
    (comp (ref D65)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A701C))
    (comp (ref R65)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A702A))
    (comp (ref SW66)
      (value "ANSI Enter")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_2.25u_PCB_LED_Inv)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7034))
    (comp (ref D66)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A703A))
    (comp (ref R66)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7048))
    (comp (ref SW67)
      (value "ISO L_Shift")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7070))
    (comp (ref R67)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7084))
    (comp (ref SW68)
      (value "ISO \\")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A708E))
    (comp (ref D68)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7094))
    (comp (ref R68)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70A2))
    (comp (ref SW69)
      (value Z)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70AC))
    (comp (ref D69)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70B2))
    (comp (ref R69)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70C0))
    (comp (ref SW70)
      (value X)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70E8))
    (comp (ref D70)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70EE))
    (comp (ref R70)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A70FC))
    (comp (ref SW71)
      (value C)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7106))
    (comp (ref D71)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A710C))
    (comp (ref R71)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A711A))
    (comp (ref SW72)
      (value V)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7124))
    (comp (ref D72)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A712A))
    (comp (ref R72)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7138))
    (comp (ref SW73)
      (value B)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0A8))
    (comp (ref D73)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0AE))
    (comp (ref R73)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0BC))
    (comp (ref SW74)
      (value N)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0E4))
    (comp (ref D74)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0EA))
    (comp (ref R74)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E0F8))
    (comp (ref SW75)
      (value M)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E102))
    (comp (ref D75)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E108))
    (comp (ref R75)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E116))
    (comp (ref SW76)
      (value <)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E120))
    (comp (ref D76)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E126))
    (comp (ref R76)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E134))
    (comp (ref SW77)
      (value >)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E15C))
    (comp (ref D77)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E162))
    (comp (ref R77)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E170))
    (comp (ref SW78)
      (value ?)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E17A))
    (comp (ref D78)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E180))
    (comp (ref R78)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E18E))
    (comp (ref SW79)
      (value "JIS _")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E198))
    (comp (ref D79)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E19E))
    (comp (ref R79)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1AC))
    (comp (ref SW80)
      (value "JIS R_Shift")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.75u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1D4))
    (comp (ref D80)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1DA))
    (comp (ref R80)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1E8))
    (comp (ref SW81)
      (value Reserved)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1F2))
    (comp (ref D81)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E1F8))
    (comp (ref R81)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E206))
    (comp (ref SW82)
      (value Up)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E210))
    (comp (ref D82)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E216))
    (comp (ref R82)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E224))
    (comp (ref SW83)
      (value Reserved)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E24C))
    (comp (ref D83)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E252))
    (comp (ref R83)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E260))
    (comp (ref SW84)
      (value L_Ctrl)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E26A))
    (comp (ref D84)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E270))
    (comp (ref R84)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E27E))
    (comp (ref SW85)
      (value L_OS)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2A6))
    (comp (ref D85)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2AC))
    (comp (ref R85)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2BA))
    (comp (ref SW88)
      (value Space)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_6.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E31E))
    (comp (ref D88)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E324))
    (comp (ref R88)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E332))
    (comp (ref SW89)
      (value "JIS Henk")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E35A))
    (comp (ref D89)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E360))
    (comp (ref R89)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E36E))
    (comp (ref SW90)
      (value "JIS Kana")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E378))
    (comp (ref D90)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E37E))
    (comp (ref R90)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E38C))
    (comp (ref SW91)
      (value R_Alt)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E396))
    (comp (ref D91)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E39C))
    (comp (ref R91)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3AA))
    (comp (ref SW92)
      (value R_OS)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3D2))
    (comp (ref D92)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3D8))
    (comp (ref R92)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3E6))
    (comp (ref SW93)
      (value Menu)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3F0))
    (comp (ref D93)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E3F6))
    (comp (ref R93)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E404))
    (comp (ref SW94)
      (value R_Ctrl)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E40E))
    (comp (ref D94)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E414))
    (comp (ref R94)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E422))
    (comp (ref SW95)
      (value Left)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E44A))
    (comp (ref D95)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E450))
    (comp (ref R95)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E45E))
    (comp (ref SW320)
      (value Backspace)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_2.00u_PCB_LED_Inv)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DE988BA))
    (comp (ref SW670)
      (value "ANSI L_Shift")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_2.25u_PCB_LED_Inv)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB8DF6))
    (comp (ref SW800)
      (value R_Shift)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_2.75u_PCB_LED_Inv)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1324AB))
    (comp (ref SW86)
      (value L_Alt)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.25u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2E2))
    (comp (ref D86)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2E8))
    (comp (ref R86)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E2F6))
    (comp (ref SW87)
      (value "JIS Mhen")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E300))
    (comp (ref D87)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E306))
    (comp (ref R87)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E23E314))
    (comp (ref SW96)
      (value Down)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BAA))
    (comp (ref D96)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BB0))
    (comp (ref R96)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BBE))
    (comp (ref SW97)
      (value Right)
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BC8))
    (comp (ref D97)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BCE))
    (comp (ref R97)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E956BDC))
    (comp (ref SW880)
      (value "JIS Space")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_2.75u_PCB_LED)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F9FD530))
    (comp (ref SW660)
      (value "ISO Enter")
      (footprint Button_Switch_Keyboard:SW_Cherry_MX_ISOEnter_PCB_LED_Rot)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push_LED) (description "Push button switch with LED, generic"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FAA416A))
    (comp (ref R32)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E13D9A8))
    (comp (ref R54)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25104))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A6E4A))
    (comp (ref D67)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (fields
        (field (name LCSC) C68948))
      (libsource (lib Device) (part D) (description Diode))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E1A7076))
    (comp (ref D101)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DFCA6EA))
    (comp (ref C101)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DFD1ED1))
    (comp (ref D102)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E394B6B))
    (comp (ref C102)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E394B71))
    (comp (ref D103)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4091A0))
    (comp (ref C103)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4091A6))
    (comp (ref D104)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E47EA81))
    (comp (ref C104)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E47EA87))
    (comp (ref D105)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4F560E))
    (comp (ref C105)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4F5614))
    (comp (ref D106)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E56F666))
    (comp (ref C106)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E56F66C))
    (comp (ref D107)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E7FCE))
    (comp (ref C107)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5E7FD4))
    (comp (ref D108)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E661DE2))
    (comp (ref C108)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E661DE8))
    (comp (ref D109)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E6DCA16))
    (comp (ref C109)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E6DCA1C))
    (comp (ref D110)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E75924C))
    (comp (ref C110)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E759252))
    (comp (ref D111)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7D6216))
    (comp (ref C111)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7D621C))
    (comp (ref D112)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E8561CC))
    (comp (ref C112)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E8561D2))
    (comp (ref D113)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E8D41BE))
    (comp (ref C113)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E8D41C4))
    (comp (ref D114)
      (value WS2812B)
      (footprint LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm)
      (datasheet https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (fields
        (field (name LCSC) C114586))
      (libsource (lib LED) (part WS2812B) (description "RGB LED with integrated controller"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E953E25))
    (comp (ref C114)
      (value 15pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1548))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E953E2B))
    (comp (ref Q1)
      (value BC817)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.fairchildsemi.com/ds/BC/BC817.pdf)
      (fields
        (field (name LCSC) C8589))
      (libsource (lib Transistor_BJT) (part BC817) (description "0.8A Ic, 45V Vce, NPN Transistor, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 65411C92))
    (comp (ref R200)
      (value 3K3)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25890))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 655507A0))
    (comp (ref J1)
      (value Conn_01x30)
      (footprint Connector_FFC-FPC:TE_3-84953-0_1x30-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x30) (description "Generic connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5B68CD)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x30)
      (description "Generic connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x30))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib LED) (part WS2812B)
      (description "RGB LED with integrated controller")
      (docs https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
      (footprints
        (fp LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*))
      (fields
        (field (name Reference) D)
        (field (name Value) WS2812B)
        (field (name Footprint) LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name DOUT) (type output))
        (pin (num 3) (name VSS) (type power_in))
        (pin (num 4) (name DIN) (type input))))
    (libpart (lib Switch) (part SW_Push_LED)
      (description "Push button switch with LED, generic")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push_LED))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name K) (type passive))
        (pin (num 4) (name A) (type passive))))
    (libpart (lib Transistor_BJT) (part BC817)
      (aliases
        (alias BC818)
        (alias BC846)
        (alias BC847)
        (alias BC848)
        (alias BC849)
        (alias BC850)
        (alias MMBT3904)
        (alias MMBT5550L)
        (alias MMBT5551L))
      (description "0.8A Ic, 45V Vce, NPN Transistor, SOT-23")
      (docs http://www.fairchildsemi.com/ds/BC/BC817.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC817)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical LED)
      (uri /usr/share/kicad/library/LED.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Transistor_BJT)
      (uri /usr/share/kicad/library/Transistor_BJT.lib)))
  (nets
    (net (code 1) (name /66D)
      (node (ref SW660) (pin 2))
      (node (ref D66) (pin 2))
      (node (ref SW66) (pin 2)))
    (net (code 2) (name /66LED)
      (node (ref SW66) (pin 3))
      (node (ref R66) (pin 1))
      (node (ref SW660) (pin 3)))
    (net (code 3) (name /COL4)
      (node (ref J1) (pin 21))
      (node (ref SW58) (pin 1))
      (node (ref SW59) (pin 1))
      (node (ref SW51) (pin 1))
      (node (ref SW50) (pin 1))
      (node (ref SW55) (pin 1))
      (node (ref SW49) (pin 1))
      (node (ref SW56) (pin 1))
      (node (ref SW57) (pin 1))
      (node (ref SW53) (pin 1))
      (node (ref SW54) (pin 1))
      (node (ref SW52) (pin 1))
      (node (ref SW60) (pin 1))
      (node (ref SW660) (pin 1)))
    (net (code 4) (name /32LED)
      (node (ref SW320) (pin 3))
      (node (ref R32) (pin 1))
      (node (ref SW32) (pin 3)))
    (net (code 5) (name /88D)
      (node (ref SW88) (pin 2))
      (node (ref SW880) (pin 2))
      (node (ref D88) (pin 2)))
    (net (code 6) (name /88LED)
      (node (ref SW880) (pin 3))
      (node (ref SW88) (pin 3))
      (node (ref R88) (pin 1)))
    (net (code 7) (name /COL7)
      (node (ref SW95) (pin 1))
      (node (ref SW91) (pin 1))
      (node (ref SW90) (pin 1))
      (node (ref J1) (pin 24))
      (node (ref SW85) (pin 1))
      (node (ref SW96) (pin 1))
      (node (ref SW89) (pin 1))
      (node (ref SW94) (pin 1))
      (node (ref SW93) (pin 1))
      (node (ref SW88) (pin 1))
      (node (ref SW92) (pin 1))
      (node (ref SW97) (pin 1))
      (node (ref SW86) (pin 1))
      (node (ref SW87) (pin 1))
      (node (ref SW880) (pin 1)))
    (net (code 8) (name /LED_DRV)
      (node (ref R41) (pin 2))
      (node (ref R56) (pin 2))
      (node (ref R88) (pin 2))
      (node (ref R55) (pin 2))
      (node (ref R85) (pin 2))
      (node (ref R90) (pin 2))
      (node (ref R52) (pin 2))
      (node (ref R91) (pin 2))
      (node (ref R53) (pin 2))
      (node (ref R50) (pin 2))
      (node (ref R92) (pin 2))
      (node (ref R51) (pin 2))
      (node (ref R47) (pin 2))
      (node (ref R95) (pin 2))
      (node (ref R49) (pin 2))
      (node (ref R48) (pin 2))
      (node (ref R32) (pin 2))
      (node (ref R94) (pin 2))
      (node (ref R97) (pin 2))
      (node (ref R40) (pin 2))
      (node (ref R89) (pin 2))
      (node (ref Q1) (pin 3))
      (node (ref R61) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R63) (pin 2))
      (node (ref R62) (pin 2))
      (node (ref R65) (pin 2))
      (node (ref R64) (pin 2))
      (node (ref R58) (pin 2))
      (node (ref R57) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R69) (pin 2))
      (node (ref R67) (pin 2))
      (node (ref R66) (pin 2))
      (node (ref R70) (pin 2))
      (node (ref R68) (pin 2))
      (node (ref R44) (pin 2))
      (node (ref R43) (pin 2))
      (node (ref R46) (pin 2))
      (node (ref R60) (pin 2))
      (node (ref R59) (pin 2))
      (node (ref R39) (pin 2))
      (node (ref R72) (pin 2))
      (node (ref R71) (pin 2))
      (node (ref R74) (pin 2))
      (node (ref R75) (pin 2))
      (node (ref R73) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref R27) (pin 2))
      (node (ref R42) (pin 2))
      (node (ref R25) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref R45) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R34) (pin 2))
      (node (ref R35) (pin 2))
      (node (ref R33) (pin 2))
      (node (ref R37) (pin 2))
      (node (ref R36) (pin 2))
      (node (ref R38) (pin 2))
      (node (ref R29) (pin 2))
      (node (ref R30) (pin 2))
      (node (ref R86) (pin 2))
      (node (ref R54) (pin 2))
      (node (ref R77) (pin 2))
      (node (ref R93) (pin 2))
      (node (ref R78) (pin 2))
      (node (ref R81) (pin 2))
      (node (ref R87) (pin 2))
      (node (ref R82) (pin 2))
      (node (ref R80) (pin 2))
      (node (ref R79) (pin 2))
      (node (ref R84) (pin 2))
      (node (ref R83) (pin 2))
      (node (ref R96) (pin 2))
      (node (ref R76) (pin 2)))
    (net (code 9) (name "Net-(R97-Pad1)")
      (node (ref SW97) (pin 3))
      (node (ref R97) (pin 1)))
    (net (code 10) (name /ROW0)
      (node (ref D37) (pin 1))
      (node (ref D73) (pin 1))
      (node (ref D25) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref D85) (pin 1))
      (node (ref D49) (pin 1)))
    (net (code 11) (name /ROW7)
      (node (ref D66) (pin 1))
      (node (ref D91) (pin 1))
      (node (ref D78) (pin 1))
      (node (ref D18) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref D30) (pin 1))
      (node (ref D42) (pin 1)))
    (net (code 12) (name /ROW6)
      (node (ref D77) (pin 1))
      (node (ref D54) (pin 1))
      (node (ref D90) (pin 1))
      (node (ref D17) (pin 1))
      (node (ref D29) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref J1) (pin 7))
      (node (ref D65) (pin 1)))
    (net (code 13) (name /ROW5)
      (node (ref D64) (pin 1))
      (node (ref J1) (pin 6))
      (node (ref D5) (pin 1))
      (node (ref D16) (pin 1))
      (node (ref D41) (pin 1))
      (node (ref D53) (pin 1))
      (node (ref D89) (pin 1)))
    (net (code 14) (name /ROW4)
      (node (ref D76) (pin 1))
      (node (ref J1) (pin 5))
      (node (ref D52) (pin 1))
      (node (ref D40) (pin 1))
      (node (ref D28) (pin 1))
      (node (ref D88) (pin 1))
      (node (ref D4) (pin 1)))
    (net (code 15) (name /ROW3)
      (node (ref D75) (pin 1))
      (node (ref J1) (pin 4))
      (node (ref D63) (pin 1))
      (node (ref D39) (pin 1))
      (node (ref D15) (pin 1))
      (node (ref D27) (pin 1)))
    (net (code 16) (name /ROW2)
      (node (ref D3) (pin 1))
      (node (ref D74) (pin 1))
      (node (ref J1) (pin 3))
      (node (ref D26) (pin 1))
      (node (ref D51) (pin 1))
      (node (ref D87) (pin 1))
      (node (ref D14) (pin 1))
      (node (ref D62) (pin 1)))
    (net (code 17) (name /ROW1)
      (node (ref D50) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref D61) (pin 1))
      (node (ref D13) (pin 1))
      (node (ref D86) (pin 1))
      (node (ref D38) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 18) (name /ROW14)
      (node (ref D12) (pin 1))
      (node (ref D97) (pin 1))
      (node (ref D35) (pin 1))
      (node (ref J1) (pin 15))
      (node (ref D60) (pin 1))
      (node (ref D71) (pin 1))
      (node (ref D83) (pin 1))
      (node (ref D23) (pin 1)))
    (net (code 19) (name /80LED)
      (node (ref R80) (pin 1))
      (node (ref SW800) (pin 3))
      (node (ref SW80) (pin 3)))
    (net (code 20) (name /67LED)
      (node (ref R67) (pin 1))
      (node (ref SW67) (pin 3))
      (node (ref SW670) (pin 3)))
    (net (code 21) (name "Net-(R54-Pad1)")
      (node (ref R54) (pin 1))
      (node (ref SW54) (pin 3)))
    (net (code 22) (name "Net-(D86-Pad2)")
      (node (ref SW86) (pin 2))
      (node (ref D86) (pin 2)))
    (net (code 23) (name "Net-(R86-Pad1)")
      (node (ref R86) (pin 1))
      (node (ref SW86) (pin 3)))
    (net (code 24) (name "Net-(D87-Pad2)")
      (node (ref SW87) (pin 2))
      (node (ref D87) (pin 2)))
    (net (code 25) (name "Net-(R87-Pad1)")
      (node (ref R87) (pin 1))
      (node (ref SW87) (pin 3)))
    (net (code 26) (name /80D)
      (node (ref SW800) (pin 2))
      (node (ref SW80) (pin 2))
      (node (ref D80) (pin 2)))
    (net (code 27) (name /COL6)
      (node (ref SW80) (pin 1))
      (node (ref SW83) (pin 1))
      (node (ref J1) (pin 23))
      (node (ref SW84) (pin 1))
      (node (ref SW78) (pin 1))
      (node (ref SW75) (pin 1))
      (node (ref SW81) (pin 1))
      (node (ref SW73) (pin 1))
      (node (ref SW74) (pin 1))
      (node (ref SW76) (pin 1))
      (node (ref SW77) (pin 1))
      (node (ref SW800) (pin 1))
      (node (ref SW79) (pin 1))
      (node (ref SW82) (pin 1)))
    (net (code 28) (name /67D)
      (node (ref SW67) (pin 2))
      (node (ref D67) (pin 2))
      (node (ref SW670) (pin 2)))
    (net (code 29) (name /COL5)
      (node (ref SW670) (pin 1))
      (node (ref SW63) (pin 1))
      (node (ref SW65) (pin 1))
      (node (ref SW64) (pin 1))
      (node (ref SW66) (pin 1))
      (node (ref SW62) (pin 1))
      (node (ref SW71) (pin 1))
      (node (ref SW61) (pin 1))
      (node (ref SW72) (pin 1))
      (node (ref J1) (pin 22))
      (node (ref SW67) (pin 1))
      (node (ref SW68) (pin 1))
      (node (ref SW69) (pin 1))
      (node (ref SW70) (pin 1)))
    (net (code 30) (name "Net-(D96-Pad2)")
      (node (ref D96) (pin 2))
      (node (ref SW96) (pin 2)))
    (net (code 31) (name "Net-(D97-Pad2)")
      (node (ref SW97) (pin 2))
      (node (ref D97) (pin 2)))
    (net (code 32) (name "Net-(R96-Pad1)")
      (node (ref SW96) (pin 3))
      (node (ref R96) (pin 1)))
    (net (code 33) (name /ROW13)
      (node (ref D59) (pin 1))
      (node (ref D11) (pin 1))
      (node (ref D47) (pin 1))
      (node (ref D70) (pin 1))
      (node (ref D22) (pin 1))
      (node (ref J1) (pin 14))
      (node (ref D96) (pin 1)))
    (net (code 34) (name /ROW8)
      (node (ref D79) (pin 1))
      (node (ref D55) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref D31) (pin 1))
      (node (ref J1) (pin 9))
      (node (ref D43) (pin 1))
      (node (ref D92) (pin 1)))
    (net (code 35) (name GND)
      (node (ref C102) (pin 1))
      (node (ref C107) (pin 1))
      (node (ref D107) (pin 3))
      (node (ref D114) (pin 3))
      (node (ref C106) (pin 1))
      (node (ref C114) (pin 1))
      (node (ref C103) (pin 1))
      (node (ref C105) (pin 1))
      (node (ref C108) (pin 1))
      (node (ref D109) (pin 3))
      (node (ref C109) (pin 1))
      (node (ref C104) (pin 1))
      (node (ref D108) (pin 3))
      (node (ref D102) (pin 3))
      (node (ref D106) (pin 3))
      (node (ref C111) (pin 1))
      (node (ref D111) (pin 3))
      (node (ref D105) (pin 3))
      (node (ref D104) (pin 3))
      (node (ref D101) (pin 3))
      (node (ref C101) (pin 1))
      (node (ref J1) (pin 30))
      (node (ref J1) (pin 29))
      (node (ref D103) (pin 3))
      (node (ref C113) (pin 1))
      (node (ref D113) (pin 3))
      (node (ref C112) (pin 1))
      (node (ref D112) (pin 3))
      (node (ref Q1) (pin 2))
      (node (ref C110) (pin 1))
      (node (ref D110) (pin 3)))
    (net (code 36) (name +5V)
      (node (ref SW52) (pin 4))
      (node (ref SW6) (pin 4))
      (node (ref SW9) (pin 4))
      (node (ref SW10) (pin 4))
      (node (ref SW56) (pin 4))
      (node (ref SW48) (pin 4))
      (node (ref SW35) (pin 4))
      (node (ref SW22) (pin 4))
      (node (ref SW23) (pin 4))
      (node (ref SW51) (pin 4))
      (node (ref SW20) (pin 4))
      (node (ref SW21) (pin 4))
      (node (ref SW660) (pin 4))
      (node (ref SW27) (pin 4))
      (node (ref SW50) (pin 4))
      (node (ref SW30) (pin 4))
      (node (ref SW36) (pin 4))
      (node (ref SW7) (pin 4))
      (node (ref SW31) (pin 4))
      (node (ref SW32) (pin 4))
      (node (ref SW33) (pin 4))
      (node (ref SW87) (pin 4))
      (node (ref SW29) (pin 4))
      (node (ref SW55) (pin 4))
      (node (ref SW38) (pin 4))
      (node (ref SW49) (pin 4))
      (node (ref SW86) (pin 4))
      (node (ref SW37) (pin 4))
      (node (ref SW34) (pin 4))
      (node (ref SW96) (pin 4))
      (node (ref SW70) (pin 4))
      (node (ref SW58) (pin 4))
      (node (ref SW59) (pin 4))
      (node (ref SW69) (pin 4))
      (node (ref SW44) (pin 4))
      (node (ref SW65) (pin 4))
      (node (ref SW45) (pin 4))
      (node (ref SW66) (pin 4))
      (node (ref C101) (pin 2))
      (node (ref SW62) (pin 4))
      (node (ref SW43) (pin 4))
      (node (ref SW64) (pin 4))
      (node (ref SW47) (pin 4))
      (node (ref SW63) (pin 4))
      (node (ref SW13) (pin 4))
      (node (ref SW74) (pin 4))
      (node (ref D102) (pin 1))
      (node (ref SW75) (pin 4))
      (node (ref C102) (pin 2))
      (node (ref SW68) (pin 4))
      (node (ref SW72) (pin 4))
      (node (ref SW73) (pin 4))
      (node (ref D105) (pin 1))
      (node (ref D103) (pin 1))
      (node (ref SW60) (pin 4))
      (node (ref SW67) (pin 4))
      (node (ref SW71) (pin 4))
      (node (ref SW61) (pin 4))
      (node (ref SW57) (pin 4))
      (node (ref SW41) (pin 4))
      (node (ref SW16) (pin 4))
      (node (ref SW670) (pin 4))
      (node (ref D104) (pin 1))
      (node (ref SW4) (pin 4))
      (node (ref SW5) (pin 4))
      (node (ref SW54) (pin 4))
      (node (ref SW53) (pin 4))
      (node (ref SW1) (pin 4))
      (node (ref SW880) (pin 4))
      (node (ref SW800) (pin 4))
      (node (ref SW3) (pin 4))
      (node (ref SW2) (pin 4))
      (node (ref SW8) (pin 4))
      (node (ref SW40) (pin 4))
      (node (ref SW14) (pin 4))
      (node (ref SW46) (pin 4))
      (node (ref SW11) (pin 4))
      (node (ref SW12) (pin 4))
      (node (ref C103) (pin 2))
      (node (ref SW39) (pin 4))
      (node (ref SW18) (pin 4))
      (node (ref SW97) (pin 4))
      (node (ref SW19) (pin 4))
      (node (ref C104) (pin 2))
      (node (ref SW15) (pin 4))
      (node (ref SW42) (pin 4))
      (node (ref SW17) (pin 4))
      (node (ref D101) (pin 1))
      (node (ref J1) (pin 25))
      (node (ref J1) (pin 28))
      (node (ref C109) (pin 2))
      (node (ref C105) (pin 2))
      (node (ref D106) (pin 1))
      (node (ref C107) (pin 2))
      (node (ref D107) (pin 1))
      (node (ref D109) (pin 1))
      (node (ref C106) (pin 2))
      (node (ref D112) (pin 1))
      (node (ref SW84) (pin 4))
      (node (ref SW83) (pin 4))
      (node (ref SW77) (pin 4))
      (node (ref SW78) (pin 4))
      (node (ref C112) (pin 2))
      (node (ref D108) (pin 1))
      (node (ref C108) (pin 2))
      (node (ref D113) (pin 1))
      (node (ref C113) (pin 2))
      (node (ref D110) (pin 1))
      (node (ref C110) (pin 2))
      (node (ref C111) (pin 2))
      (node (ref D111) (pin 1))
      (node (ref SW80) (pin 4))
      (node (ref SW88) (pin 4))
      (node (ref SW89) (pin 4))
      (node (ref SW79) (pin 4))
      (node (ref SW95) (pin 4))
      (node (ref SW320) (pin 4))
      (node (ref SW92) (pin 4))
      (node (ref SW94) (pin 4))
      (node (ref SW93) (pin 4))
      (node (ref SW90) (pin 4))
      (node (ref SW76) (pin 4))
      (node (ref SW91) (pin 4))
      (node (ref SW82) (pin 4))
      (node (ref D114) (pin 1))
      (node (ref SW28) (pin 4))
      (node (ref SW85) (pin 4))
      (node (ref C114) (pin 2))
      (node (ref SW24) (pin 4))
      (node (ref SW26) (pin 4))
      (node (ref SW25) (pin 4))
      (node (ref SW81) (pin 4)))
    (net (code 37) (name /RGB_IN)
      (node (ref J1) (pin 27))
      (node (ref D101) (pin 4)))
    (net (code 38) (name "Net-(D101-Pad2)")
      (node (ref D102) (pin 4))
      (node (ref D101) (pin 2)))
    (net (code 39) (name "Net-(D103-Pad2)")
      (node (ref D103) (pin 2))
      (node (ref D104) (pin 4)))
    (net (code 40) (name "Net-(D102-Pad2)")
      (node (ref D102) (pin 2))
      (node (ref D103) (pin 4)))
    (net (code 41) (name /COL0)
      (node (ref SW11) (pin 1))
      (node (ref SW3) (pin 1))
      (node (ref SW10) (pin 1))
      (node (ref SW12) (pin 1))
      (node (ref SW7) (pin 1))
      (node (ref SW2) (pin 1))
      (node (ref SW9) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref SW4) (pin 1))
      (node (ref SW5) (pin 1))
      (node (ref J1) (pin 17))
      (node (ref SW6) (pin 1))
      (node (ref SW8) (pin 1)))
    (net (code 42) (name /COL1)
      (node (ref SW13) (pin 1))
      (node (ref SW18) (pin 1))
      (node (ref SW22) (pin 1))
      (node (ref J1) (pin 18))
      (node (ref SW14) (pin 1))
      (node (ref SW16) (pin 1))
      (node (ref SW15) (pin 1))
      (node (ref SW17) (pin 1))
      (node (ref SW24) (pin 1))
      (node (ref SW23) (pin 1))
      (node (ref SW21) (pin 1))
      (node (ref SW20) (pin 1))
      (node (ref SW19) (pin 1)))
    (net (code 43) (name /COL2)
      (node (ref SW26) (pin 1))
      (node (ref SW35) (pin 1))
      (node (ref SW32) (pin 1))
      (node (ref SW25) (pin 1))
      (node (ref J1) (pin 19))
      (node (ref SW30) (pin 1))
      (node (ref SW28) (pin 1))
      (node (ref SW31) (pin 1))
      (node (ref SW33) (pin 1))
      (node (ref SW34) (pin 1))
      (node (ref SW36) (pin 1))
      (node (ref SW320) (pin 1))
      (node (ref SW29) (pin 1))
      (node (ref SW27) (pin 1)))
    (net (code 44) (name /COL3)
      (node (ref SW48) (pin 1))
      (node (ref SW41) (pin 1))
      (node (ref J1) (pin 20))
      (node (ref SW43) (pin 1))
      (node (ref SW38) (pin 1))
      (node (ref SW46) (pin 1))
      (node (ref SW42) (pin 1))
      (node (ref SW47) (pin 1))
      (node (ref SW45) (pin 1))
      (node (ref SW44) (pin 1))
      (node (ref SW40) (pin 1))
      (node (ref SW37) (pin 1))
      (node (ref SW39) (pin 1)))
    (net (code 45) (name /ROW15)
      (node (ref D24) (pin 1))
      (node (ref D72) (pin 1))
      (node (ref J1) (pin 16))
      (node (ref D36) (pin 1))
      (node (ref D48) (pin 1))
      (node (ref D84) (pin 1)))
    (net (code 46) (name /ROW12)
      (node (ref D46) (pin 1))
      (node (ref D58) (pin 1))
      (node (ref D95) (pin 1))
      (node (ref D82) (pin 1))
      (node (ref D34) (pin 1))
      (node (ref D10) (pin 1))
      (node (ref J1) (pin 13)))
    (net (code 47) (name /ROW11)
      (node (ref D21) (pin 1))
      (node (ref J1) (pin 12))
      (node (ref D33) (pin 1))
      (node (ref D45) (pin 1))
      (node (ref D69) (pin 1))
      (node (ref D81) (pin 1))
      (node (ref D94) (pin 1)))
    (net (code 48) (name /ROW10)
      (node (ref D57) (pin 1))
      (node (ref D20) (pin 1))
      (node (ref J1) (pin 11))
      (node (ref D9) (pin 1))
      (node (ref D80) (pin 1))
      (node (ref D93) (pin 1))
      (node (ref D68) (pin 1))
      (node (ref D32) (pin 1)))
    (net (code 49) (name /ROW9)
      (node (ref D67) (pin 1))
      (node (ref J1) (pin 10))
      (node (ref D8) (pin 1))
      (node (ref D44) (pin 1))
      (node (ref D19) (pin 1))
      (node (ref D56) (pin 1)))
    (net (code 50) (name /32D)
      (node (ref D32) (pin 2))
      (node (ref SW320) (pin 2))
      (node (ref SW32) (pin 2)))
    (net (code 51) (name /PWM_IN)
      (node (ref R200) (pin 2))
      (node (ref J1) (pin 26)))
    (net (code 52) (name "Net-(D82-Pad2)")
      (node (ref D82) (pin 2))
      (node (ref SW82) (pin 2)))
    (net (code 53) (name "Net-(R82-Pad1)")
      (node (ref SW82) (pin 3))
      (node (ref R82) (pin 1)))
    (net (code 54) (name "Net-(D83-Pad2)")
      (node (ref SW83) (pin 2))
      (node (ref D83) (pin 2)))
    (net (code 55) (name "Net-(R83-Pad1)")
      (node (ref R83) (pin 1))
      (node (ref SW83) (pin 3)))
    (net (code 56) (name "Net-(R81-Pad1)")
      (node (ref SW81) (pin 3))
      (node (ref R81) (pin 1)))
    (net (code 57) (name "Net-(D81-Pad2)")
      (node (ref SW81) (pin 2))
      (node (ref D81) (pin 2)))
    (net (code 58) (name "Net-(D85-Pad2)")
      (node (ref D85) (pin 2))
      (node (ref SW85) (pin 2)))
    (net (code 59) (name "Net-(R85-Pad1)")
      (node (ref SW85) (pin 3))
      (node (ref R85) (pin 1)))
    (net (code 60) (name "Net-(R84-Pad1)")
      (node (ref SW84) (pin 3))
      (node (ref R84) (pin 1)))
    (net (code 61) (name "Net-(D84-Pad2)")
      (node (ref SW84) (pin 2))
      (node (ref D84) (pin 2)))
    (net (code 62) (name "Net-(R77-Pad1)")
      (node (ref SW77) (pin 3))
      (node (ref R77) (pin 1)))
    (net (code 63) (name "Net-(D77-Pad2)")
      (node (ref D77) (pin 2))
      (node (ref SW77) (pin 2)))
    (net (code 64) (name "Net-(D78-Pad2)")
      (node (ref D78) (pin 2))
      (node (ref SW78) (pin 2)))
    (net (code 65) (name "Net-(R78-Pad1)")
      (node (ref R78) (pin 1))
      (node (ref SW78) (pin 3)))
    (net (code 66) (name "Net-(R76-Pad1)")
      (node (ref SW76) (pin 3))
      (node (ref R76) (pin 1)))
    (net (code 67) (name "Net-(D76-Pad2)")
      (node (ref D76) (pin 2))
      (node (ref SW76) (pin 2)))
    (net (code 68) (name "Net-(R79-Pad1)")
      (node (ref SW79) (pin 3))
      (node (ref R79) (pin 1)))
    (net (code 69) (name "Net-(D79-Pad2)")
      (node (ref D79) (pin 2))
      (node (ref SW79) (pin 2)))
    (net (code 70) (name "Net-(R93-Pad1)")
      (node (ref R93) (pin 1))
      (node (ref SW93) (pin 3)))
    (net (code 71) (name "Net-(D93-Pad2)")
      (node (ref SW93) (pin 2))
      (node (ref D93) (pin 2)))
    (net (code 72) (name "Net-(D94-Pad2)")
      (node (ref D94) (pin 2))
      (node (ref SW94) (pin 2)))
    (net (code 73) (name "Net-(R94-Pad1)")
      (node (ref SW94) (pin 3))
      (node (ref R94) (pin 1)))
    (net (code 74) (name "Net-(R92-Pad1)")
      (node (ref SW92) (pin 3))
      (node (ref R92) (pin 1)))
    (net (code 75) (name "Net-(D92-Pad2)")
      (node (ref D92) (pin 2))
      (node (ref SW92) (pin 2)))
    (net (code 76) (name "Net-(R95-Pad1)")
      (node (ref SW95) (pin 3))
      (node (ref R95) (pin 1)))
    (net (code 77) (name "Net-(D95-Pad2)")
      (node (ref SW95) (pin 2))
      (node (ref D95) (pin 2)))
    (net (code 78) (name "Net-(D89-Pad2)")
      (node (ref SW89) (pin 2))
      (node (ref D89) (pin 2)))
    (net (code 79) (name "Net-(R89-Pad1)")
      (node (ref R89) (pin 1))
      (node (ref SW89) (pin 3)))
    (net (code 80) (name "Net-(R91-Pad1)")
      (node (ref R91) (pin 1))
      (node (ref SW91) (pin 3)))
    (net (code 81) (name "Net-(D91-Pad2)")
      (node (ref SW91) (pin 2))
      (node (ref D91) (pin 2)))
    (net (code 82) (name "Net-(D104-Pad2)")
      (node (ref D104) (pin 2))
      (node (ref D105) (pin 4)))
    (net (code 83) (name "Net-(R90-Pad1)")
      (node (ref R90) (pin 1))
      (node (ref SW90) (pin 3)))
    (net (code 84) (name "Net-(D90-Pad2)")
      (node (ref SW90) (pin 2))
      (node (ref D90) (pin 2)))
    (net (code 85) (name "Net-(Q1-Pad1)")
      (node (ref R200) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 86) (name "Net-(D110-Pad2)")
      (node (ref D110) (pin 2))
      (node (ref D111) (pin 4)))
    (net (code 87) (name "Net-(D113-Pad2)")
      (node (ref D113) (pin 2))
      (node (ref D114) (pin 4)))
    (net (code 88) (name "Net-(D111-Pad2)")
      (node (ref D112) (pin 4))
      (node (ref D111) (pin 2)))
    (net (code 89) (name "Net-(D112-Pad2)")
      (node (ref D113) (pin 4))
      (node (ref D112) (pin 2)))
    (net (code 90) (name "Net-(D105-Pad2)")
      (node (ref D105) (pin 2))
      (node (ref D106) (pin 4)))
    (net (code 91) (name "Net-(D106-Pad2)")
      (node (ref D106) (pin 2))
      (node (ref D107) (pin 4)))
    (net (code 92) (name "Net-(D109-Pad2)")
      (node (ref D110) (pin 4))
      (node (ref D109) (pin 2)))
    (net (code 93) (name "Net-(D107-Pad2)")
      (node (ref D107) (pin 2))
      (node (ref D108) (pin 4)))
    (net (code 94) (name "Net-(D108-Pad2)")
      (node (ref D109) (pin 4))
      (node (ref D108) (pin 2)))
    (net (code 95) (name "Net-(D114-Pad2)")
      (node (ref D114) (pin 2)))
    (net (code 96) (name "Net-(D25-Pad2)")
      (node (ref SW25) (pin 2))
      (node (ref D25) (pin 2)))
    (net (code 97) (name "Net-(R25-Pad1)")
      (node (ref SW25) (pin 3))
      (node (ref R25) (pin 1)))
    (net (code 98) (name "Net-(D26-Pad2)")
      (node (ref SW26) (pin 2))
      (node (ref D26) (pin 2)))
    (net (code 99) (name "Net-(R26-Pad1)")
      (node (ref SW26) (pin 3))
      (node (ref R26) (pin 1)))
    (net (code 100) (name "Net-(R24-Pad1)")
      (node (ref R24) (pin 1))
      (node (ref SW24) (pin 3)))
    (net (code 101) (name "Net-(D24-Pad2)")
      (node (ref SW24) (pin 2))
      (node (ref D24) (pin 2)))
    (net (code 102) (name "Net-(D28-Pad2)")
      (node (ref SW28) (pin 2))
      (node (ref D28) (pin 2)))
    (net (code 103) (name "Net-(R28-Pad1)")
      (node (ref R28) (pin 1))
      (node (ref SW28) (pin 3)))
    (net (code 104) (name "Net-(R27-Pad1)")
      (node (ref SW27) (pin 3))
      (node (ref R27) (pin 1)))
    (net (code 105) (name "Net-(D27-Pad2)")
      (node (ref D27) (pin 2))
      (node (ref SW27) (pin 2)))
    (net (code 106) (name "Net-(R20-Pad1)")
      (node (ref SW20) (pin 3))
      (node (ref R20) (pin 1)))
    (net (code 107) (name "Net-(D21-Pad2)")
      (node (ref SW21) (pin 2))
      (node (ref D21) (pin 2)))
    (net (code 108) (name "Net-(R21-Pad1)")
      (node (ref R21) (pin 1))
      (node (ref SW21) (pin 3)))
    (net (code 109) (name "Net-(D20-Pad2)")
      (node (ref D20) (pin 2))
      (node (ref SW20) (pin 2)))
    (net (code 110) (name "Net-(R19-Pad1)")
      (node (ref SW19) (pin 3))
      (node (ref R19) (pin 1)))
    (net (code 111) (name "Net-(R23-Pad1)")
      (node (ref R23) (pin 1))
      (node (ref SW23) (pin 3)))
    (net (code 112) (name "Net-(D23-Pad2)")
      (node (ref D23) (pin 2))
      (node (ref SW23) (pin 2)))
    (net (code 113) (name "Net-(R22-Pad1)")
      (node (ref R22) (pin 1))
      (node (ref SW22) (pin 3)))
    (net (code 114) (name "Net-(D22-Pad2)")
      (node (ref D22) (pin 2))
      (node (ref SW22) (pin 2)))
    (net (code 115) (name "Net-(D35-Pad2)")
      (node (ref SW35) (pin 2))
      (node (ref D35) (pin 2)))
    (net (code 116) (name "Net-(R35-Pad1)")
      (node (ref SW35) (pin 3))
      (node (ref R35) (pin 1)))
    (net (code 117) (name "Net-(R34-Pad1)")
      (node (ref SW34) (pin 3))
      (node (ref R34) (pin 1)))
    (net (code 118) (name "Net-(D36-Pad2)")
      (node (ref D36) (pin 2))
      (node (ref SW36) (pin 2)))
    (net (code 119) (name "Net-(D34-Pad2)")
      (node (ref D34) (pin 2))
      (node (ref SW34) (pin 2)))
    (net (code 120) (name "Net-(R33-Pad1)")
      (node (ref SW33) (pin 3))
      (node (ref R33) (pin 1)))
    (net (code 121) (name "Net-(R38-Pad1)")
      (node (ref R38) (pin 1))
      (node (ref SW38) (pin 3)))
    (net (code 122) (name "Net-(D38-Pad2)")
      (node (ref D38) (pin 2))
      (node (ref SW38) (pin 2)))
    (net (code 123) (name "Net-(R37-Pad1)")
      (node (ref SW37) (pin 3))
      (node (ref R37) (pin 1)))
    (net (code 124) (name "Net-(D37-Pad2)")
      (node (ref SW37) (pin 2))
      (node (ref D37) (pin 2)))
    (net (code 125) (name "Net-(R36-Pad1)")
      (node (ref SW36) (pin 3))
      (node (ref R36) (pin 1)))
    (net (code 126) (name "Net-(D30-Pad2)")
      (node (ref D30) (pin 2))
      (node (ref SW30) (pin 2)))
    (net (code 127) (name "Net-(R30-Pad1)")
      (node (ref R30) (pin 1))
      (node (ref SW30) (pin 3)))
    (net (code 128) (name "Net-(D31-Pad2)")
      (node (ref D31) (pin 2))
      (node (ref SW31) (pin 2)))
    (net (code 129) (name "Net-(R31-Pad1)")
      (node (ref SW31) (pin 3))
      (node (ref R31) (pin 1)))
    (net (code 130) (name "Net-(R29-Pad1)")
      (node (ref R29) (pin 1))
      (node (ref SW29) (pin 3)))
    (net (code 131) (name "Net-(D29-Pad2)")
      (node (ref D29) (pin 2))
      (node (ref SW29) (pin 2)))
    (net (code 132) (name "Net-(D33-Pad2)")
      (node (ref SW33) (pin 2))
      (node (ref D33) (pin 2)))
    (net (code 133) (name "Net-(R6-Pad1)")
      (node (ref SW6) (pin 3))
      (node (ref R6) (pin 1)))
    (net (code 134) (name "Net-(D7-Pad2)")
      (node (ref SW7) (pin 2))
      (node (ref D7) (pin 2)))
    (net (code 135) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref SW7) (pin 3)))
    (net (code 136) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref SW6) (pin 2)))
    (net (code 137) (name "Net-(R5-Pad1)")
      (node (ref SW5) (pin 3))
      (node (ref R5) (pin 1)))
    (net (code 138) (name "Net-(R9-Pad1)")
      (node (ref SW9) (pin 3))
      (node (ref R9) (pin 1)))
    (net (code 139) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref SW10) (pin 3)))
    (net (code 140) (name "Net-(D10-Pad2)")
      (node (ref SW10) (pin 2))
      (node (ref D10) (pin 2)))
    (net (code 141) (name "Net-(D9-Pad2)")
      (node (ref D9) (pin 2))
      (node (ref SW9) (pin 2)))
    (net (code 142) (name "Net-(R8-Pad1)")
      (node (ref SW8) (pin 3))
      (node (ref R8) (pin 1)))
    (net (code 143) (name "Net-(D8-Pad2)")
      (node (ref SW8) (pin 2))
      (node (ref D8) (pin 2)))
    (net (code 144) (name "Net-(D2-Pad2)")
      (node (ref SW2) (pin 2))
      (node (ref D2) (pin 2)))
    (net (code 145) (name "Net-(R2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref SW2) (pin 3)))
    (net (code 146) (name "Net-(D3-Pad2)")
      (node (ref SW3) (pin 2))
      (node (ref D3) (pin 2)))
    (net (code 147) (name "Net-(R3-Pad1)")
      (node (ref SW3) (pin 3))
      (node (ref R3) (pin 1)))
    (net (code 148) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref SW1) (pin 3)))
    (net (code 149) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref SW1) (pin 2)))
    (net (code 150) (name "Net-(D5-Pad2)")
      (node (ref SW5) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 151) (name "Net-(R4-Pad1)")
      (node (ref SW4) (pin 3))
      (node (ref R4) (pin 1)))
    (net (code 152) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref SW4) (pin 2)))
    (net (code 153) (name "Net-(D16-Pad2)")
      (node (ref SW16) (pin 2))
      (node (ref D16) (pin 2)))
    (net (code 154) (name "Net-(R16-Pad1)")
      (node (ref R16) (pin 1))
      (node (ref SW16) (pin 3)))
    (net (code 155) (name "Net-(D17-Pad2)")
      (node (ref D17) (pin 2))
      (node (ref SW17) (pin 2)))
    (net (code 156) (name "Net-(R17-Pad1)")
      (node (ref R17) (pin 1))
      (node (ref SW17) (pin 3)))
    (net (code 157) (name "Net-(R15-Pad1)")
      (node (ref R15) (pin 1))
      (node (ref SW15) (pin 3)))
    (net (code 158) (name "Net-(D15-Pad2)")
      (node (ref D15) (pin 2))
      (node (ref SW15) (pin 2)))
    (net (code 159) (name "Net-(D18-Pad2)")
      (node (ref D18) (pin 2))
      (node (ref SW18) (pin 2)))
    (net (code 160) (name "Net-(D19-Pad2)")
      (node (ref SW19) (pin 2))
      (node (ref D19) (pin 2)))
    (net (code 161) (name "Net-(R18-Pad1)")
      (node (ref SW18) (pin 3))
      (node (ref R18) (pin 1)))
    (net (code 162) (name "Net-(R14-Pad1)")
      (node (ref SW14) (pin 3))
      (node (ref R14) (pin 1)))
    (net (code 163) (name "Net-(D12-Pad2)")
      (node (ref D12) (pin 2))
      (node (ref SW12) (pin 2)))
    (net (code 164) (name "Net-(R12-Pad1)")
      (node (ref R12) (pin 1))
      (node (ref SW12) (pin 3)))
    (net (code 165) (name "Net-(R11-Pad1)")
      (node (ref R11) (pin 1))
      (node (ref SW11) (pin 3)))
    (net (code 166) (name "Net-(D11-Pad2)")
      (node (ref D11) (pin 2))
      (node (ref SW11) (pin 2)))
    (net (code 167) (name "Net-(D14-Pad2)")
      (node (ref SW14) (pin 2))
      (node (ref D14) (pin 2)))
    (net (code 168) (name "Net-(R13-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref SW13) (pin 3)))
    (net (code 169) (name "Net-(D13-Pad2)")
      (node (ref SW13) (pin 2))
      (node (ref D13) (pin 2)))
    (net (code 170) (name "Net-(D63-Pad2)")
      (node (ref D63) (pin 2))
      (node (ref SW63) (pin 2)))
    (net (code 171) (name "Net-(R63-Pad1)")
      (node (ref SW63) (pin 3))
      (node (ref R63) (pin 1)))
    (net (code 172) (name "Net-(D64-Pad2)")
      (node (ref SW64) (pin 2))
      (node (ref D64) (pin 2)))
    (net (code 173) (name "Net-(R64-Pad1)")
      (node (ref R64) (pin 1))
      (node (ref SW64) (pin 3)))
    (net (code 174) (name "Net-(R62-Pad1)")
      (node (ref R62) (pin 1))
      (node (ref SW62) (pin 3)))
    (net (code 175) (name "Net-(D62-Pad2)")
      (node (ref D62) (pin 2))
      (node (ref SW62) (pin 2)))
    (net (code 176) (name "Net-(D65-Pad2)")
      (node (ref D65) (pin 2))
      (node (ref SW65) (pin 2)))
    (net (code 177) (name "Net-(R65-Pad1)")
      (node (ref R65) (pin 1))
      (node (ref SW65) (pin 3)))
    (net (code 178) (name "Net-(R61-Pad1)")
      (node (ref SW61) (pin 3))
      (node (ref R61) (pin 1)))
    (net (code 179) (name "Net-(R58-Pad1)")
      (node (ref R58) (pin 1))
      (node (ref SW58) (pin 3)))
    (net (code 180) (name "Net-(D58-Pad2)")
      (node (ref SW58) (pin 2))
      (node (ref D58) (pin 2)))
    (net (code 181) (name "Net-(D59-Pad2)")
      (node (ref D59) (pin 2))
      (node (ref SW59) (pin 2)))
    (net (code 182) (name "Net-(R59-Pad1)")
      (node (ref SW59) (pin 3))
      (node (ref R59) (pin 1)))
    (net (code 183) (name "Net-(R57-Pad1)")
      (node (ref SW57) (pin 3))
      (node (ref R57) (pin 1)))
    (net (code 184) (name "Net-(D57-Pad2)")
      (node (ref SW57) (pin 2))
      (node (ref D57) (pin 2)))
    (net (code 185) (name "Net-(D61-Pad2)")
      (node (ref D61) (pin 2))
      (node (ref SW61) (pin 2)))
    (net (code 186) (name "Net-(R60-Pad1)")
      (node (ref R60) (pin 1))
      (node (ref SW60) (pin 3)))
    (net (code 187) (name "Net-(D60-Pad2)")
      (node (ref SW60) (pin 2))
      (node (ref D60) (pin 2)))
    (net (code 188) (name "Net-(R72-Pad1)")
      (node (ref R72) (pin 1))
      (node (ref SW72) (pin 3)))
    (net (code 189) (name "Net-(D73-Pad2)")
      (node (ref D73) (pin 2))
      (node (ref SW73) (pin 2)))
    (net (code 190) (name "Net-(R73-Pad1)")
      (node (ref SW73) (pin 3))
      (node (ref R73) (pin 1)))
    (net (code 191) (name "Net-(D72-Pad2)")
      (node (ref SW72) (pin 2))
      (node (ref D72) (pin 2)))
    (net (code 192) (name "Net-(R71-Pad1)")
      (node (ref R71) (pin 1))
      (node (ref SW71) (pin 3)))
    (net (code 193) (name "Net-(R75-Pad1)")
      (node (ref R75) (pin 1))
      (node (ref SW75) (pin 3)))
    (net (code 194) (name "Net-(D75-Pad2)")
      (node (ref D75) (pin 2))
      (node (ref SW75) (pin 2)))
    (net (code 195) (name "Net-(R74-Pad1)")
      (node (ref SW74) (pin 3))
      (node (ref R74) (pin 1)))
    (net (code 196) (name "Net-(D74-Pad2)")
      (node (ref D74) (pin 2))
      (node (ref SW74) (pin 2)))
    (net (code 197) (name "Net-(D69-Pad2)")
      (node (ref SW69) (pin 2))
      (node (ref D69) (pin 2)))
    (net (code 198) (name "Net-(R68-Pad1)")
      (node (ref R68) (pin 1))
      (node (ref SW68) (pin 3)))
    (net (code 199) (name "Net-(D68-Pad2)")
      (node (ref D68) (pin 2))
      (node (ref SW68) (pin 2)))
    (net (code 200) (name "Net-(R69-Pad1)")
      (node (ref SW69) (pin 3))
      (node (ref R69) (pin 1)))
    (net (code 201) (name "Net-(D71-Pad2)")
      (node (ref D71) (pin 2))
      (node (ref SW71) (pin 2)))
    (net (code 202) (name "Net-(R70-Pad1)")
      (node (ref SW70) (pin 3))
      (node (ref R70) (pin 1)))
    (net (code 203) (name "Net-(D70-Pad2)")
      (node (ref SW70) (pin 2))
      (node (ref D70) (pin 2)))
    (net (code 204) (name "Net-(D44-Pad2)")
      (node (ref D44) (pin 2))
      (node (ref SW44) (pin 2)))
    (net (code 205) (name "Net-(R44-Pad1)")
      (node (ref R44) (pin 1))
      (node (ref SW44) (pin 3)))
    (net (code 206) (name "Net-(D45-Pad2)")
      (node (ref SW45) (pin 2))
      (node (ref D45) (pin 2)))
    (net (code 207) (name "Net-(R45-Pad1)")
      (node (ref R45) (pin 1))
      (node (ref SW45) (pin 3)))
    (net (code 208) (name "Net-(R43-Pad1)")
      (node (ref SW43) (pin 3))
      (node (ref R43) (pin 1)))
    (net (code 209) (name "Net-(D43-Pad2)")
      (node (ref SW43) (pin 2))
      (node (ref D43) (pin 2)))
    (net (code 210) (name "Net-(D47-Pad2)")
      (node (ref D47) (pin 2))
      (node (ref SW47) (pin 2)))
    (net (code 211) (name "Net-(R47-Pad1)")
      (node (ref R47) (pin 1))
      (node (ref SW47) (pin 3)))
    (net (code 212) (name "Net-(R46-Pad1)")
      (node (ref R46) (pin 1))
      (node (ref SW46) (pin 3)))
    (net (code 213) (name "Net-(D46-Pad2)")
      (node (ref D46) (pin 2))
      (node (ref SW46) (pin 2)))
    (net (code 214) (name "Net-(R40-Pad1)")
      (node (ref SW40) (pin 3))
      (node (ref R40) (pin 1)))
    (net (code 215) (name "Net-(R39-Pad1)")
      (node (ref R39) (pin 1))
      (node (ref SW39) (pin 3)))
    (net (code 216) (name "Net-(D40-Pad2)")
      (node (ref SW40) (pin 2))
      (node (ref D40) (pin 2)))
    (net (code 217) (name "Net-(D39-Pad2)")
      (node (ref D39) (pin 2))
      (node (ref SW39) (pin 2)))
    (net (code 218) (name "Net-(R41-Pad1)")
      (node (ref R41) (pin 1))
      (node (ref SW41) (pin 3)))
    (net (code 219) (name "Net-(R42-Pad1)")
      (node (ref SW42) (pin 3))
      (node (ref R42) (pin 1)))
    (net (code 220) (name "Net-(D42-Pad2)")
      (node (ref SW42) (pin 2))
      (node (ref D42) (pin 2)))
    (net (code 221) (name "Net-(D41-Pad2)")
      (node (ref D41) (pin 2))
      (node (ref SW41) (pin 2)))
    (net (code 222) (name "Net-(R53-Pad1)")
      (node (ref R53) (pin 1))
      (node (ref SW53) (pin 3)))
    (net (code 223) (name "Net-(D53-Pad2)")
      (node (ref D53) (pin 2))
      (node (ref SW53) (pin 2)))
    (net (code 224) (name "Net-(D54-Pad2)")
      (node (ref D54) (pin 2))
      (node (ref SW54) (pin 2)))
    (net (code 225) (name "Net-(R52-Pad1)")
      (node (ref SW52) (pin 3))
      (node (ref R52) (pin 1)))
    (net (code 226) (name "Net-(D52-Pad2)")
      (node (ref SW52) (pin 2))
      (node (ref D52) (pin 2)))
    (net (code 227) (name "Net-(D56-Pad2)")
      (node (ref SW56) (pin 2))
      (node (ref D56) (pin 2)))
    (net (code 228) (name "Net-(R56-Pad1)")
      (node (ref R56) (pin 1))
      (node (ref SW56) (pin 3)))
    (net (code 229) (name "Net-(R55-Pad1)")
      (node (ref R55) (pin 1))
      (node (ref SW55) (pin 3)))
    (net (code 230) (name "Net-(D55-Pad2)")
      (node (ref D55) (pin 2))
      (node (ref SW55) (pin 2)))
    (net (code 231) (name "Net-(R49-Pad1)")
      (node (ref R49) (pin 1))
      (node (ref SW49) (pin 3)))
    (net (code 232) (name "Net-(D49-Pad2)")
      (node (ref D49) (pin 2))
      (node (ref SW49) (pin 2)))
    (net (code 233) (name "Net-(R48-Pad1)")
      (node (ref SW48) (pin 3))
      (node (ref R48) (pin 1)))
    (net (code 234) (name "Net-(D48-Pad2)")
      (node (ref D48) (pin 2))
      (node (ref SW48) (pin 2)))
    (net (code 235) (name "Net-(D51-Pad2)")
      (node (ref D51) (pin 2))
      (node (ref SW51) (pin 2)))
    (net (code 236) (name "Net-(R51-Pad1)")
      (node (ref SW51) (pin 3))
      (node (ref R51) (pin 1)))
    (net (code 237) (name "Net-(R50-Pad1)")
      (node (ref R50) (pin 1))
      (node (ref SW50) (pin 3)))
    (net (code 238) (name "Net-(D50-Pad2)")
      (node (ref D50) (pin 2))
      (node (ref SW50) (pin 2)))))