(module TE_3-84953-4_1x34-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5C8E913E)
  (descr "TE FPC connector, 34 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4")
  (tags "te fpc 84953")
  (attr smd)
  (fp_text reference REF** (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TE_3-84953-4_1x34-1MP_P1.0mm_Horizontal (at 0 7.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -19.935 -0.8) (end 19.935 -0.8) (layer F.Fab) (width 0.1))
  (fp_line (start 19.935 -0.8) (end 19.935 3.71) (layer F.Fab) (width 0.1))
  (fp_line (start 19.935 3.71) (end 20.96 3.71) (layer F.Fab) (width 0.1))
  (fp_line (start 20.96 3.71) (end 20.96 4.6) (layer F.Fab) (width 0.1))
  (fp_line (start 20.96 4.6) (end -20.96 4.6) (layer F.Fab) (width 0.1))
  (fp_line (start -20.96 4.6) (end -20.96 3.71) (layer F.Fab) (width 0.1))
  (fp_line (start -20.96 3.71) (end -19.935 3.71) (layer F.Fab) (width 0.1))
  (fp_line (start -19.935 3.71) (end -19.935 -0.8) (layer F.Fab) (width 0.1))
  (fp_line (start -17 -0.8) (end -16.5 0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -16.5 0.2) (end -16 -0.8) (layer F.Fab) (width 0.1))
  (fp_line (start 19.935 4.6) (end 19.935 5.61) (layer F.Fab) (width 0.1))
  (fp_line (start 19.935 5.61) (end 20.96 5.61) (layer F.Fab) (width 0.1))
  (fp_line (start 20.96 5.61) (end 20.96 6.5) (layer F.Fab) (width 0.1))
  (fp_line (start 20.96 6.5) (end -20.96 6.5) (layer F.Fab) (width 0.1))
  (fp_line (start -20.96 6.5) (end -20.96 5.61) (layer F.Fab) (width 0.1))
  (fp_line (start -20.96 5.61) (end -19.935 5.61) (layer F.Fab) (width 0.1))
  (fp_line (start -19.935 5.61) (end -19.935 4.6) (layer F.Fab) (width 0.1))
  (fp_line (start 20.045 3.06) (end 20.045 3.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 20.045 3.6) (end 21.07 3.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 21.07 3.6) (end 21.07 4.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 21.07 4.71) (end -21.07 4.71) (layer F.SilkS) (width 0.12))
  (fp_line (start -21.07 4.71) (end -21.07 3.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -21.07 3.6) (end -20.045 3.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -20.045 3.6) (end -20.045 3.06) (layer F.SilkS) (width 0.12))
  (fp_line (start -17.89 -0.91) (end -17.065 -0.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -17.065 -0.91) (end -17.065 -2.71) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.065 -0.91) (end 17.89 -0.91) (layer F.SilkS) (width 0.12))
  (fp_line (start -21.46 -3.3) (end -21.46 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -21.46 7) (end 21.46 7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 21.46 7) (end 21.46 -3.3) (layer F.CrtYd) (width 0.05))
  (fp_line (start 21.46 -3.3) (end -21.46 -3.3) (layer F.CrtYd) (width 0.05))
  (pad 1 smd rect (at -16.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -15.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -14.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -13.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -12.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -11.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -10.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at -9.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at -8.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at -7.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at -6.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at -5.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at -4.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd rect (at -3.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 15 smd rect (at -2.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 16 smd rect (at -1.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 17 smd rect (at -0.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 18 smd rect (at 0.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 19 smd rect (at 1.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 20 smd rect (at 2.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 21 smd rect (at 3.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 22 smd rect (at 4.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 23 smd rect (at 5.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 24 smd rect (at 6.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 25 smd rect (at 7.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 26 smd rect (at 8.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 27 smd rect (at 9.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 28 smd rect (at 10.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 29 smd rect (at 11.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 30 smd rect (at 12.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 31 smd rect (at 13.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 32 smd rect (at 14.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 33 smd rect (at 15.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad 34 smd rect (at 16.5 -1.8) (size 0.61 2) (layers F.Cu F.Mask F.Paste))
  (pad MP smd rect (at -19.49 1) (size 2.68 3.6) (layers F.Cu F.Mask F.Paste))
  (pad MP smd rect (at 19.49 1) (size 2.68 3.6) (layers F.Cu F.Mask F.Paste))
  (fp_text user %R (at 0 1.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_3-84953-4_1x34-1MP_P1.0mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)