(export (version D)
  (design
    (source /home/antonlysak/KiCAD/PRO/Ki5/Ki5.sch)
    (date "Ср 26 сен 2018 21:47:01")
    (tool "Eeschema 5.0.0-rc3-6a2723a~65~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "U540 RISC-V MPU eval board")
        (company)
        (rev)
        (date)
        (source Ki5.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Freedom-U540_1/) (tstamps /5AF2BD01/)
      (title_block
        (title "Freedom U540 DDR and ChipLink")
        (company)
        (rev)
        (date "08 05 2018")
        (source Freedom-U540_1-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /Freedom-U540_2/) (tstamps /5AF2BD02/)
      (title_block
        (title "Freedom U540 IO and Power")
        (company)
        (rev)
        (date "08 05 2018")
        (source Freedom-U540_2-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /DDR4_x8_32b_1/) (tstamps /5AF2BD03/)
      (title_block
        (title "DDR4x8 32 Bits")
        (company)
        (rev)
        (date "08 05 2018")
        (source DDR4_x8_32b_1-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/)
      (title_block
        (title "DDR4x8 32 Bit and ECC")
        (company)
        (rev)
        (date "08 05 2018")
        (source DDR4_x8_32b_2_ECC-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /FT2232/) (tstamps /5AF2BD05/)
      (title_block
        (title "USB to UART and JTAG")
        (company)
        (rev)
        (date "08 05 2018")
        (source FT2232-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /Power.sch/) (tstamps /5AF2BD06/)
      (title_block
        (title "Power Supply")
        (company)
        (rev)
        (date "08 05 2018")
        (source Power-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /FMC.sch/) (tstamps /5AF2BD07/)
      (title_block
        (title "FMC Connector")
        (company)
        (rev)
        (date "08 05 2018")
        (source FMC-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /Ethernet/) (tstamps /5AF2BD08/)
      (title_block
        (title Ethernet)
        (company)
        (rev)
        (date "08 05 2018")
        (source Ethernet-SchDoc.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C127)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D019))
    (comp (ref C99)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D018))
    (comp (ref C125)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D017))
    (comp (ref RS2)
      (value 0R001)
      (footprint Resistor_SMD:R_Shunt_Vishay_WSKW0612)
      (fields
        (field (name CrossRef) 8))
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D016))
    (comp (ref R75)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D014))
    (comp (ref R76)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D013))
    (comp (ref R77)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D012))
    (comp (ref R78)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 9))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D011))
    (comp (ref RS3)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name CrossRef) 9))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D010))
    (comp (ref R70)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00F))
    (comp (ref C126)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00E))
    (comp (ref R145)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00D))
    (comp (ref R146)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00C))
    (comp (ref R147)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00B))
    (comp (ref R151)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (fields
        (field (name CrossRef) 7))
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D00A))
    (comp (ref R150)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D009))
    (comp (ref R149)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D008))
    (comp (ref R148)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 7))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D007))
    (comp (ref R153)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D006))
    (comp (ref R155)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D005))
    (comp (ref R152)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D004))
    (comp (ref C129)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D003))
    (comp (ref R154)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D002))
    (comp (ref RS5)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D001))
    (comp (ref RS4)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1D000))
    (comp (ref RS6)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFFF))
    (comp (ref C266)
      (value 2.2pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFFE))
    (comp (ref C128)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF8))
    (comp (ref R178)
      (value 75R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF6))
    (comp (ref C95)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF5))
    (comp (ref C96)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF4))
    (comp (ref C94)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF3))
    (comp (ref C97)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF2))
    (comp (ref C98)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5AF1CFF1))
    (comp (ref J15)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5B07519F))
    (comp (ref J16)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5B58BD51))
    (comp (ref J17)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5BBE05D8))
    (comp (ref J18)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5BF3AC88))
    (comp (ref U1)
      (value FU540-C000)
      (footprint Package_BGA:BGA-484_23.0x23.0mm_Layout22x22_P1.0mm)
      (datasheet https://static.dev.sifive.com/FU540-C000-v1.0.pdf)
      (libsource (lib MCU_SiFive) (part FU540-C000) (description " 64-bit RISC‑V SoC"))
      (sheetpath (names /Freedom-U540_1/) (tstamps /5AF2BD01/))
      (tstamp 5B3FDA45))
    (comp (ref R13)
      (value 2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF79))
    (comp (ref D4)
      (value Green)
      (footprint LED_SMD:LED_0603_1608Metric)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF78))
    (comp (ref C241)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF76))
    (comp (ref R160)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF75))
    (comp (ref R158)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF74))
    (comp (ref R159)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF73))
    (comp (ref C242)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF70))
    (comp (ref R161)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6F))
    (comp (ref R162)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6E))
    (comp (ref R18)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6D))
    (comp (ref C243)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6B))
    (comp (ref C244)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6A))
    (comp (ref C245)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF69))
    (comp (ref C246)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF68))
    (comp (ref C247)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF67))
    (comp (ref C248)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF66))
    (comp (ref C249)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF65))
    (comp (ref C250)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF64))
    (comp (ref C251)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF63))
    (comp (ref R19)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF62))
    (comp (ref C252)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF61))
    (comp (ref C253)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF60))
    (comp (ref C254)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5F))
    (comp (ref C255)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5E))
    (comp (ref C256)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5D))
    (comp (ref C257)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5C))
    (comp (ref C258)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5B))
    (comp (ref RS10)
      (value 0R001)
      (footprint Resistor_SMD:R_Shunt_Vishay_WSKW0612)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF5A))
    (comp (ref RS9)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF59))
    (comp (ref R182)
      (value 1M)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF52))
    (comp (ref R183)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF51))
    (comp (ref R186)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF50))
    (comp (ref R12)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF4E))
    (comp (ref C134)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF4D))
    (comp (ref R14)
      (value 2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF49))
    (comp (ref C206)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF48))
    (comp (ref C207)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF47))
    (comp (ref X1)
      (value "33.3333 MHz")
      (footprint Oscillator:Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm)
      (libsource (lib Oscillator) (part XO32) (description "HCMOS Clock Oscillator"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF46))
    (comp (ref C136)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF45))
    (comp (ref R20)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF44))
    (comp (ref C138)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF42))
    (comp (ref R21)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF40))
    (comp (ref R22)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3F))
    (comp (ref D1)
      (value Green)
      (footprint LED_SMD:LED_0603_1608Metric)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3E))
    (comp (ref R24)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3D))
    (comp (ref R25)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3C))
    (comp (ref R27)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3B))
    (comp (ref R28)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF3A))
    (comp (ref R29)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF39))
    (comp (ref R30)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF38))
    (comp (ref R46)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF36))
    (comp (ref R47)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF35))
    (comp (ref R48)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF34))
    (comp (ref D2)
      (value Green)
      (footprint LED_SMD:LED_0603_1608Metric)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF33))
    (comp (ref R49)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF32))
    (comp (ref R50)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF31))
    (comp (ref R51)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF30))
    (comp (ref R53)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2F))
    (comp (ref R54)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2E))
    (comp (ref R55)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2D))
    (comp (ref R56)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2C))
    (comp (ref R57)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2B))
    (comp (ref R58)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF2A))
    (comp (ref R52)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF29))
    (comp (ref R16)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF28))
    (comp (ref R59)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF27))
    (comp (ref C130)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF26))
    (comp (ref C132)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF25))
    (comp (ref C131)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF24))
    (comp (ref C133)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF23))
    (comp (ref X2)
      (value "1.0 MHz")
      (footprint Oscillator:Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm)
      (libsource (lib Oscillator) (part XO32) (description "HCMOS Clock Oscillator"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF22))
    (comp (ref C135)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF21))
    (comp (ref R44)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF20))
    (comp (ref R45)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF1F))
    (comp (ref D11)
      (value PGB1010603NRHF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression (TVS) diode"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF1E))
    (comp (ref R17)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF1D))
    (comp (ref R37)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) "5, 7"))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF1B))
    (comp (ref U20)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF19))
    (comp (ref U21)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF18))
    (comp (ref U23)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF17))
    (comp (ref U24)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF16))
    (comp (ref U25)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF15))
    (comp (ref U22)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF14))
    (comp (ref C153)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF13))
    (comp (ref C154)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF11))
    (comp (ref C155)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF10))
    (comp (ref C156)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0F))
    (comp (ref C157)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0E))
    (comp (ref C158)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0D))
    (comp (ref C159)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0C))
    (comp (ref C160)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0B))
    (comp (ref C161)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF0A))
    (comp (ref C162)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF09))
    (comp (ref C163)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF08))
    (comp (ref C164)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF06))
    (comp (ref C165)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF05))
    (comp (ref D10)
      (value PGB1010603NRHF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression (TVS) diode"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF03))
    (comp (ref R72)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF02))
    (comp (ref R73)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 5))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF01))
    (comp (ref R15)
      (value 47K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF00))
    (comp (ref R65)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEFF))
    (comp (ref S1)
      (value "SW DIP-6")
      (footprint Button_Switch_SMD:SW_DIP_SPSTx06_Slide_6.7x16.8mm_W8.61mm_P2.54mm_LowProfile)
      (libsource (lib Switch) (part SW_DIP_x06) (description "6x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEFD))
    (comp (ref D3)
      (value Green)
      (footprint LED_SMD:LED_0603_1608Metric)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEFC))
    (comp (ref S3)
      (value DNP)
      (footprint Button_Switch_SMD:SW_DIP_SPSTx06_Slide_6.7x16.8mm_W8.61mm_P2.54mm_LowProfile)
      (libsource (lib Switch) (part SW_DIP_x06) (description "6x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEFB))
    (comp (ref RS7)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name CrossRef) 9))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF8))
    (comp (ref R140)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF7))
    (comp (ref R139)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF6))
    (comp (ref R141)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF5))
    (comp (ref R142)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF4))
    (comp (ref R143)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF3))
    (comp (ref R144)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CEF2))
    (comp (ref C137)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 5))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF41))
    (comp (ref Y1)
      (value "33.333 MHz")
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (libsource (lib Device) (part Crystal_GND2) (description "Three pin crystal (GND on pin 2), e.g. in SMD package"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF43))
    (comp (ref D13)
      (value 1N4148WT)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet https://www.diodes.com/assets/Datasheets/ds30396.pdf)
      (libsource (lib Diode) (part 1N4148WT) (description "75V 0.15A Fast switching Diode, SOD-523"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B4DCC4F))
    (comp (ref J2)
      (value Conn_02x10_Odd_Even)
      (footprint Connector_PinSocket_2.00mm:PinSocket_2x10_P2.00mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x10_Odd_Even) (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B108FE9))
    (comp (ref J11)
      (value Conn_02x05_Odd_Even)
      (footprint Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x05_Odd_Even) (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5C3E0A76))
    (comp (ref J13)
      (value Conn_02x04_Odd_Even)
      (footprint Connector_PinHeader_1.27mm:PinHeader_2x04_P1.27mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Odd_Even) (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5CBFF7A2))
    (comp (ref J10)
      (value Micro_SD_Card_Det)
      (footprint Connector_Card:microSD_HC_Hirose_DM3D-SF)
      (datasheet https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1)
      (libsource (lib Connector) (part Micro_SD_Card_Det) (description "Micro SD Card Socket with card detection pins"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B0EFE2A))
    (comp (ref J3)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B15E646))
    (comp (ref J4)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B2473D5))
    (comp (ref J5)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B32F1AE))
    (comp (ref J6)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:MMCX_Molex_73415-1471_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B416F74))
    (comp (ref S2)
      (value SW_Push)
      (footprint Button_Switch_SMD:SW_SPST_PTS645)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5C00DD2F))
    (comp (ref RS8)
      (value 0R20)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5AF1CF6C))
    (comp (ref U12)
      (value IS25WP256D)
      (footprint Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm)
      (datasheet "http://www.issi.com/WW/pdf/IS25LP(WP)256D.pdf")
      (libsource (lib Memory_Flash) (part IS25WP256D) (description "SERIAL FLASH MEMORY WITH 166/133MHZ MULTI I/O SPI&QUAD I/O QPI DTR INTERFACE"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B2A8F2E))
    (comp (ref J1)
      (value Conn_02x20_Odd_Even)
      (footprint Connector_PinSocket_2.00mm:PinSocket_2x20_P2.00mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B15E7E7))
    (comp (ref Q1)
      (value FDG6335N)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.gneic.com/product/datasheet/FDG6335N-1122853.pdf)
      (libsource (lib Transistor_FET) (part FDG6335N) (description "0.7A Id, 20V Vds, Dual N-Channel MOSFET, 300mOhm Ron, SC-70-6"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B248BD4))
    (comp (ref Q2)
      (value FDG6335N)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.gneic.com/product/datasheet/FDG6335N-1122853.pdf)
      (libsource (lib Transistor_FET) (part FDG6335N) (description "0.7A Id, 20V Vds, Dual N-Channel MOSFET, 300mOhm Ron, SC-70-6"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5BD8365C))
    (comp (ref Q4)
      (value FDG6335N)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.gneic.com/product/datasheet/FDG6335N-1122853.pdf)
      (libsource (lib Transistor_FET) (part FDG6335N) (description "0.7A Id, 20V Vds, Dual N-Channel MOSFET, 300mOhm Ron, SC-70-6"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5C8DD6F6))
    (comp (ref U26)
      (value TPD6F003)
      (footprint Package_SON:Texas_R-PWSON-N12_EP0.4x2mm)
      (datasheet http://www.ti.com/lit/ds/symlink/tpd6f003.pdf)
      (libsource (lib Power_Protection) (part TPD6F003) (description "6 channel EMI filters with integrated ESD protection"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5CEE6126))
    (comp (ref Q6)
      (value IRLML6402)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.infineon.com/dgdl/irlml6402pbf.pdf?fileId=5546d462533600a401535668d5c2263c)
      (libsource (lib Transistor_FET) (part IRLML6402) (description "-3.7A Id, -20V Vds, P-channel MOSFET, 65mOhm Rds, SOT-23"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5D5E4545))
    (comp (ref J14)
      (value Conn_02x11_Odd_Even)
      (footprint Connector_PinHeader_1.27mm:PinHeader_2x11_P1.27mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x11_Odd_Even) (description "Generic connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /Freedom-U540_2/) (tstamps /5AF2BD02/))
      (tstamp 5B5B670B))
    (comp (ref R1)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1AC))
    (comp (ref C7)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1AB))
    (comp (ref C8)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1AA))
    (comp (ref C15)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A9))
    (comp (ref C14)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A8))
    (comp (ref C16)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A7))
    (comp (ref C27)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A6))
    (comp (ref C26)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A5))
    (comp (ref C28)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A4))
    (comp (ref C35)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A3))
    (comp (ref C34)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A2))
    (comp (ref R2)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A1))
    (comp (ref C36)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D1A0))
    (comp (ref C1)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19F))
    (comp (ref C2)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19E))
    (comp (ref C3)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19D))
    (comp (ref C4)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19C))
    (comp (ref C5)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19B))
    (comp (ref C9)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D19A))
    (comp (ref C10)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D199))
    (comp (ref C11)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D198))
    (comp (ref C12)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D197))
    (comp (ref R4)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D196))
    (comp (ref C13)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D195))
    (comp (ref C21)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D194))
    (comp (ref C22)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D193))
    (comp (ref C23)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D192))
    (comp (ref C24)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D191))
    (comp (ref C25)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D190))
    (comp (ref C29)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18F))
    (comp (ref C30)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18E))
    (comp (ref C31)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18D))
    (comp (ref C32)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18C))
    (comp (ref R3)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18B))
    (comp (ref C33)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D18A))
    (comp (ref U11)
      (value TPS51200DRC)
      (footprint Package_SON:Texas_S-PVSON-N10)
      (libsource (lib Regulator_Linear) (part TPS51200DRC) (description "Sink and Source DDR Termination Regulator, VSON-10"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D189))
    (comp (ref C90)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D188))
    (comp (ref R10)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D187))
    (comp (ref R11)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D186))
    (comp (ref C66)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D185))
    (comp (ref C68)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D184))
    (comp (ref C70)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D183))
    (comp (ref C91)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D182))
    (comp (ref C92)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D181))
    (comp (ref C17)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D180))
    (comp (ref C93)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17F))
    (comp (ref C88)
      (value 1nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 9))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17E))
    (comp (ref RS1)
      (value 0R001)
      (footprint Resistor_SMD:R_Shunt_Vishay_WSKW0612)
      (libsource (lib Device) (part R_Shunt) (description "Shunt Resistor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17D))
    (comp (ref R164)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17C))
    (comp (ref R166)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17B))
    (comp (ref R168)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D17A))
    (comp (ref C259)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D179))
    (comp (ref C260)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D178))
    (comp (ref C261)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D177))
    (comp (ref C262)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D176))
    (comp (ref C37)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D175))
    (comp (ref C263)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D174))
    (comp (ref C264)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D173))
    (comp (ref R163)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D172))
    (comp (ref R165)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D171))
    (comp (ref R167)
      (value 49R9)
      (footprint Resistor_SMD:R_Array_Convex_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D170))
    (comp (ref R170)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16F))
    (comp (ref R171)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16E))
    (comp (ref C265)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16D))
    (comp (ref U5)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16C))
    (comp (ref U4)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16B))
    (comp (ref C19)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D16A))
    (comp (ref U3)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D169))
    (comp (ref U2)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (fields
        (field (name CrossRef) "1, 4"))
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D168))
    (comp (ref C269)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D167))
    (comp (ref C270)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D166))
    (comp (ref C240)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D165))
    (comp (ref C268)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D164))
    (comp (ref C38)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D163))
    (comp (ref C40)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D162))
    (comp (ref C18)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D161))
    (comp (ref C20)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) "1, 4"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D160))
    (comp (ref C39)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15F))
    (comp (ref R184)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15E))
    (comp (ref RS11)
      (value 0R02)
      (footprint Resistor_SMD:R_0603_1608Metric)
      (fields
        (field (name CrossRef) 9))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15D))
    (comp (ref C284)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15C))
    (comp (ref R169)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15B))
    (comp (ref R179)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D15A))
    (comp (ref R180)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D159))
    (comp (ref R181)
      (value 49R9)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D158))
    (comp (ref C6)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_1/) (tstamps /5AF2BD03/))
      (tstamp 5AF1D157))
    (comp (ref R7)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11F))
    (comp (ref C89)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11E))
    (comp (ref C47)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11D))
    (comp (ref C46)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11C))
    (comp (ref C48)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11B))
    (comp (ref C55)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D11A))
    (comp (ref C54)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D119))
    (comp (ref C56)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D118))
    (comp (ref C63)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D117))
    (comp (ref C62)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D116))
    (comp (ref C64)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D115))
    (comp (ref R9)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D114))
    (comp (ref C85)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D113))
    (comp (ref C84)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D112))
    (comp (ref C86)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D111))
    (comp (ref C77)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D110))
    (comp (ref C76)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10F))
    (comp (ref C78)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10E))
    (comp (ref C71)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10D))
    (comp (ref C72)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10C))
    (comp (ref C73)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10B))
    (comp (ref C74)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D10A))
    (comp (ref R8)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D109))
    (comp (ref C75)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D108))
    (comp (ref C79)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D107))
    (comp (ref C80)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D106))
    (comp (ref C81)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D105))
    (comp (ref C82)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D104))
    (comp (ref C83)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D103))
    (comp (ref C41)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D102))
    (comp (ref C42)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D101))
    (comp (ref C43)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D100))
    (comp (ref C44)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FF))
    (comp (ref R6)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FE))
    (comp (ref C45)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FD))
    (comp (ref C49)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FC))
    (comp (ref C50)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FB))
    (comp (ref C51)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0FA))
    (comp (ref C52)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F9))
    (comp (ref C53)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F8))
    (comp (ref C57)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F7))
    (comp (ref C58)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F6))
    (comp (ref C59)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F5))
    (comp (ref C60)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F4))
    (comp (ref R5)
      (value 240R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F3))
    (comp (ref C61)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F2))
    (comp (ref U10)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F1))
    (comp (ref U9)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0F0))
    (comp (ref U8)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0EF))
    (comp (ref U7)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0EE))
    (comp (ref U6)
      (value H5AN8G8NAFR-UH)
      (footprint Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm)
      (libsource (lib Memory_RAM) (part H5AN8G8NAFR-UHC) (description "8Gb CMOS Double Data Rate IV Synchronous RAM"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0ED))
    (comp (ref C271)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0EC))
    (comp (ref C272)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0EB))
    (comp (ref C273)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0EA))
    (comp (ref C274)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E9))
    (comp (ref C69)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E8))
    (comp (ref C275)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E7))
    (comp (ref C276)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E6))
    (comp (ref C277)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E5))
    (comp (ref C278)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E4))
    (comp (ref C279)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E3))
    (comp (ref C280)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) "1, 3"))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E2))
    (comp (ref C65)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E1))
    (comp (ref C87)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0E0))
    (comp (ref C67)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /DDR4_x8_32b_2_ECC/) (tstamps /55AF2BD04/))
      (tstamp 5AF1D0DF))
    (comp (ref U13)
      (value FT2232HL)
      (footprint Package_QFP:LQFP-64_10x10mm_P0.5mm)
      (libsource (lib Interface_USB) (part FT2232H) (description "FT2232Hx, Hi Speed Double Channel USB UART/FIFO, LQFP/QFN-64"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEB1))
    (comp (ref C109)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEB0))
    (comp (ref C110)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAF))
    (comp (ref C113)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAE))
    (comp (ref R34)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAD))
    (comp (ref D5)
      (value PGB1010603NRHF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression (TVS) diode"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAC))
    (comp (ref D6)
      (value PGB1010603NRHF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression (TVS) diode"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAB))
    (comp (ref R33)
      (value 12K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name ClassName) DIFF90))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEAA))
    (comp (ref R23)
      (value 12K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA9))
    (comp (ref Y2)
      (value "12 MHz")
      (footprint Crystal:Crystal_SMD_Abracon_ABM8G-4Pin_3.2x2.5mm)
      (libsource (lib Device) (part Crystal_GND2) (description "Three pin crystal (GND on pin 2), e.g. in SMD package"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA8))
    (comp (ref C100)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA7))
    (comp (ref C108)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA5))
    (comp (ref C112)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA4))
    (comp (ref C111)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA3))
    (comp (ref FB1)
      (value 120R)
      (footprint Inductor_SMD:L_0402_1005Metric)
      (libsource (lib Device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA2))
    (comp (ref FB2)
      (value 120R)
      (footprint Inductor_SMD:L_0402_1005Metric)
      (libsource (lib Device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA1))
    (comp (ref U28)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CEA0))
    (comp (ref C167)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9F))
    (comp (ref C166)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9E))
    (comp (ref U29)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9D))
    (comp (ref C169)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9C))
    (comp (ref C102)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9B))
    (comp (ref C168)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE9A))
    (comp (ref U30)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE99))
    (comp (ref U31)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE98))
    (comp (ref U32)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE97))
    (comp (ref U33)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (fields
        (field (name CrossRef) "2, 7"))
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE96))
    (comp (ref R26)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE95))
    (comp (ref R31)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE94))
    (comp (ref R32)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE93))
    (comp (ref R74)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE91))
    (comp (ref C103)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE90))
    (comp (ref C171)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8F))
    (comp (ref C170)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8E))
    (comp (ref C175)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8D))
    (comp (ref C174)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8C))
    (comp (ref C177)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8B))
    (comp (ref C176)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE8A))
    (comp (ref C173)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE89))
    (comp (ref C172)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE88))
    (comp (ref C114)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE87))
    (comp (ref C115)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE86))
    (comp (ref C104)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE85))
    (comp (ref C105)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE84))
    (comp (ref C106)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE83))
    (comp (ref C107)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE82))
    (comp (ref C101)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5AF1CE81))
    (comp (ref J7)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Molex_47346-0001)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /FT2232/) (tstamps /5AF2BD05/))
      (tstamp 5B159F0F))
    (comp (ref L3)
      (value 2.2uH)
      (footprint Inductor_SMD:L_Wuerth_MAPI-2512)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE43))
    (comp (ref R36)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE42))
    (comp (ref C117)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE41))
    (comp (ref D7)
      (value DB2W40300L)
      (footprint Diode_SMD:D_SOD-123F)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE40))
    (comp (ref U16)
      (value TLV62095RGTR)
      (footprint Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm)
      (libsource (lib Regulator_Switching) (part TLV62095RGTx) (description "High efficiency step-down converter"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE3E))
    (comp (ref C139)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE3D))
    (comp (ref C142)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE3C))
    (comp (ref C143)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE3B))
    (comp (ref C140)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE3A))
    (comp (ref C141)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE39))
    (comp (ref C122)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE38))
    (comp (ref R61)
      (value 160K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE37))
    (comp (ref L4)
      (value 0.47uH)
      (footprint Inductor_SMD:L_Wuerth_MAPI-2510)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE36))
    (comp (ref U17)
      (value LP5907MFX-1.8/NOPB)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (libsource (lib Regulator_Linear) (part LP5907MFX-1.8) (description "250-mA Ultra-Low-Noise Low-IQ LDO"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE35))
    (comp (ref C145)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE34))
    (comp (ref C144)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE33))
    (comp (ref L5)
      (value 1.0uH)
      (footprint Inductor_SMD:L_Bourns_SRN6045TA)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE32))
    (comp (ref C146)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE31))
    (comp (ref U27)
      (value TPS62133RGTT)
      (footprint Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm)
      (libsource (lib Regulator_Switching) (part TPS62133) (description "3A Step-Down Converter with DCS-Control, Fixed 5.0V Output Voltage, 3-17V Input Voltage, QFN-16"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE2D))
    (comp (ref U18)
      (value TPS51363)
      (footprint Package_DFN_QFN:Texas_R-VFQFN-28-1EP_3.5x4.5mm_P0.4mm_EP2.1x3.1mm)
      (libsource (lib Regulator_Switching) (part TPS51363) (description "High-voltage input, synchronous converter with integrated FET"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE2A))
    (comp (ref C151)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE29))
    (comp (ref C152)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE28))
    (comp (ref R69)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE27))
    (comp (ref R71)
      (value 82K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE26))
    (comp (ref C147)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE25))
    (comp (ref R63)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE24))
    (comp (ref R64)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE23))
    (comp (ref C119)
      (value 33nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE22))
    (comp (ref R68)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE21))
    (comp (ref R66)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE20))
    (comp (ref U19)
      (value LM3880MFE-1AA/NOPB)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (libsource (lib Power_Supervisor) (part LM3880) (description "Simple Power Sequencer, SOT-23-6"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE1F))
    (comp (ref R43)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE1E))
    (comp (ref R67)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE1C))
    (comp (ref C148)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE1B))
    (comp (ref D12)
      (value PGB1010603NRHF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression (TVS) diode"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE1A))
    (comp (ref C149)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE18))
    (comp (ref C118)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE17))
    (comp (ref C219)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE16))
    (comp (ref R117)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE15))
    (comp (ref C220)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE14))
    (comp (ref U15)
      (value TLV62084DSGx)
      (footprint Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm)
      (libsource (lib Regulator_Switching) (part TLV62080DSGx) (description "High-efficiency Step-down Converter"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE13))
    (comp (ref C124)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE12))
    (comp (ref R40)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE11))
    (comp (ref R41)
      (value 33.2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE10))
    (comp (ref R42)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE0F))
    (comp (ref R62)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE0E))
    (comp (ref L1)
      (value 1.0uH)
      (footprint Inductor_SMD:L_Wuerth_MAPI-2512)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE0C))
    (comp (ref C150)
      (value 220uF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-7343-20_Kemet-V)
      (fields
        (field (name CrossRef) 7))
      (libsource (lib Device) (part CP1) (description "Polarised capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE0B))
    (comp (ref D9)
      (value Green)
      (footprint LED_SMD:LED_0603_1608Metric)
      (libsource (lib Device) (part LED) (description "LED generic"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE0A))
    (comp (ref R60)
      (value 80.6K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE09))
    (comp (ref U50)
      (value TLV62080DSGx)
      (footprint Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm)
      (libsource (lib Regulator_Switching) (part TLV62080DSGx) (description "High-efficiency Step-down Converter"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE08))
    (comp (ref L6)
      (value 2.2uH)
      (footprint Inductor_SMD:L_Wuerth_MAPI-2512)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE06))
    (comp (ref C281)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE05))
    (comp (ref R156)
      (value 33.2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE04))
    (comp (ref R138)
      (value 154K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE03))
    (comp (ref U14)
      (value TLV62080DSGx)
      (footprint Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm)
      (libsource (lib Regulator_Switching) (part TLV62080DSGx) (description "High-efficiency Step-down Converter"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE02))
    (comp (ref C116)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE01))
    (comp (ref C218)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE00))
    (comp (ref L2)
      (value 2.2uH)
      (footprint Inductor_SMD:L_Wuerth_MAPI-2512)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDFF))
    (comp (ref C121)
      (value 22uF)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDFE))
    (comp (ref R39)
      (value 33.2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDFD))
    (comp (ref R38)
      (value 210K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDFC))
    (comp (ref R177)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDFB))
    (comp (ref D8)
      (value SMF12A)
      (footprint Diode_SMD:D_SOD-123F)
      (libsource (lib Device) (part D_Zener) (description "Zener Diode"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDF8))
    (comp (ref R35)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CDF7))
    (comp (ref J8)
      (value Jack-DC)
      (footprint Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Jack-DC) (description "DC Barrel Jack"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B01DE3C))
    (comp (ref M1)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B01EBC6))
    (comp (ref M2)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B04B658))
    (comp (ref M3)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B061797))
    (comp (ref M4)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B07786F))
    (comp (ref M5)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B08D8D6))
    (comp (ref M6)
      (value Mounting_Hole_PAD)
      (footprint MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B0A39A4))
    (comp (ref J19)
      (value Fan_Tacho)
      (footprint Connector:FanPinHeader_1x03_P2.54mm_Vertical)
      (datasheet http://www.hardwarecanucks.com/forum/attachments/new-builds/16287d1330775095-help-chassis-power-fan-connectors-motherboard-asus_p8z68.jpg)
      (libsource (lib Motor) (part Fan_Tacho) (description "Fan, tacho output, 3-pin connector"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5B1D9917))
    (comp (ref S4)
      (value SW_Push_SPDT)
      (footprint Button_Switch_THT:SW_NKK_BB15AH)
      (libsource (lib Switch) (part SW_Push_SPDT) (description "Momentary Switch, single pole double throw"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5C541404))
    (comp (ref Q5)
      (value FDG6335N)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.gneic.com/product/datasheet/FDG6335N-1122853.pdf)
      (libsource (lib Transistor_FET) (part FDG6335N) (description "0.7A Id, 20V Vds, Dual N-Channel MOSFET, 300mOhm Ron, SC-70-6"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5CD93B12))
    (comp (ref C120)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Power.sch/) (tstamps /5AF2BD06/))
      (tstamp 5AF1CE07))
    (comp (ref R172)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5AF1D039))
    (comp (ref R173)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5AF1D038))
    (comp (ref R174)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 6))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5AF1D037))
    (comp (ref C267)
      (value DNP)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5AF1D036))
    (comp (ref R175)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5AF1D034))
    (comp (ref J9)
      (value ASP-134602-01)
      (footprint Connector_Samtec:Samtec_FMC_ASP-134602-01_10x40_P1.27mm_Vertical)
      (datasheet http://suddendocs.samtec.com/prints/asp-134602-01-mkt.pdf)
      (libsource (lib Connector) (part ASP-134602-01) (description "FPGA Mezzanine Card Terminal Connector"))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5B259F82))
    (comp (ref U49)
      (value M24C02-WMN)
      (footprint Package_SO:TSSOP-8_4.4x3mm_P0.65mm)
      (datasheet http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf)
      (libsource (lib Memory_EEPROM) (part M24C02-WDW) (description "2 Kb serial I2c bus EEPROM, TSSOP-8"))
      (sheetpath (names /FMC.sch/) (tstamps /5AF2BD07/))
      (tstamp 5B3501AC))
    (comp (ref Y3)
      (value "25 MHz")
      (footprint Crystal:Crystal_SMD_SeikoEpson_FA238-4Pin_3.2x2.5mm)
      (libsource (lib Device) (part Crystal_GND2) (description "Three pin crystal (GND on pin 2), e.g. in SMD package"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D0A4))
    (comp (ref C203)
      (value "1000pF, 2KV")
      (footprint Capacitor_SMD:C_1206_3216Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D0A3))
    (comp (ref C202)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D0A2))
    (comp (ref C201)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D0A1))
    (comp (ref C200)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D0A0))
    (comp (ref C199)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09F))
    (comp (ref R84)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09E))
    (comp (ref R86)
      (value 330R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09D))
    (comp (ref R79)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09C))
    (comp (ref R91)
      (value 33R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09B))
    (comp (ref C205)
      (value 10nF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D09A))
    (comp (ref C197)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D099))
    (comp (ref R93)
      (value 2K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D098))
    (comp (ref R92)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D094))
    (comp (ref R96)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D093))
    (comp (ref R94)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D092))
    (comp (ref R95)
      (value 0R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D091))
    (comp (ref R97)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D090))
    (comp (ref C190)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08F))
    (comp (ref C198)
      (value 18pF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08E))
    (comp (ref C185)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08D))
    (comp (ref C191)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08C))
    (comp (ref C189)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08B))
    (comp (ref C188)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D08A))
    (comp (ref C187)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D089))
    (comp (ref C192)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D088))
    (comp (ref C186)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D087))
    (comp (ref C196)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D086))
    (comp (ref C195)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D085))
    (comp (ref C194)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D084))
    (comp (ref R83)
      (value 1M)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D083))
    (comp (ref C193)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D082))
    (comp (ref FB4)
      (value 120R)
      (footprint Inductor_SMD:L_0402_1005Metric)
      (libsource (lib Device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D081))
    (comp (ref C178)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07F))
    (comp (ref C179)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07E))
    (comp (ref C180)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07D))
    (comp (ref C184)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07C))
    (comp (ref C183)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07B))
    (comp (ref C182)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D07A))
    (comp (ref C181)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name ClassName) DIFF100))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D079))
    (comp (ref R87)
      (value 75R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D078))
    (comp (ref J12)
      (value RJHSE5384)
      (footprint Connector_RJ:RJ45_Amphenol_RJHSE538X)
      (fields
        (field (name ClassName) DIFF100))
      (libsource (lib Connector) (part 8P8C_LED_Shielded) (description "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D077))
    (comp (ref R81)
      (value 39R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D076))
    (comp (ref R85)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D074))
    (comp (ref R82)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D073))
    (comp (ref R80)
      (value 33R)
      (footprint Resistor_SMD:R_Array_Concave_4x0402)
      (libsource (lib Device) (part R_Pack04) (description "4 Resistor network, parallel topology, DIP package"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D072))
    (comp (ref R98)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D071))
    (comp (ref R99)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D070))
    (comp (ref R100)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06F))
    (comp (ref R101)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06E))
    (comp (ref R88)
      (value 75R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06D))
    (comp (ref R102)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06C))
    (comp (ref R103)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06B))
    (comp (ref R104)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D06A))
    (comp (ref R105)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D069))
    (comp (ref R106)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D068))
    (comp (ref R107)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D067))
    (comp (ref R108)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D066))
    (comp (ref R109)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D065))
    (comp (ref R110)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D064))
    (comp (ref R111)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D063))
    (comp (ref R89)
      (value 75R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D062))
    (comp (ref R112)
      (value DNP)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D061))
    (comp (ref C211)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D060))
    (comp (ref C210)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05F))
    (comp (ref C209)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05E))
    (comp (ref U35)
      (value MIC5353-2.5YMT-TR)
      (footprint Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf)
      (libsource (lib Regulator_Linear) (part MIC5353-2.5YMT) (description "High-performance, single-output,  ultra-low  LDO regulator"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05D))
    (comp (ref U36)
      (value NCP133AMX100TCG)
      (footprint Package_DFN_QFN:DFN-6-1EP_1.2x1.2mm_P0.4mm_EP0.3x0.94mm)
      (datasheet http://www.onsemi.com/pub/Collateral/NCP133-D.PDF)
      (libsource (lib Regulator_Linear) (part NCP133AMX100TCG) (description "500  mA  VLDO  equipped  with  NMOS  pass transistor  and  a  separate  bias  supply  voltage"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05C))
    (comp (ref C214)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05B))
    (comp (ref C212)
      (value 1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D05A))
    (comp (ref C213)
      (value 4.7uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D059))
    (comp (ref R115)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D058))
    (comp (ref R90)
      (value 75R)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D057))
    (comp (ref R113)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D056))
    (comp (ref R114)
      (value 4.7K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D055))
    (comp (ref U37)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D054))
    (comp (ref U38)
      (value SN74AUP1T34DCKR)
      (footprint Package_TO_SOT_SMD:SOT-353_SC-70-5)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Logic_LevelTranslator) (part SN74AUP1T34DCK) (description "1-Bit Unidirectional Voltage-Level Translator, SC-70"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D053))
    (comp (ref R116)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D052))
    (comp (ref C208)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D051))
    (comp (ref C215)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (fields
        (field (name CrossRef) 2))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D050))
    (comp (ref C216)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D04F))
    (comp (ref C217)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D04E))
    (comp (ref T1)
      (value TG111-MSC13LF)
      (footprint Transformer_SMD:Transformer_Ethernet_HALO_TG111-MSC13)
      (datasheet https://www.haloelectronics.com/pdf/discrete-genesus.pdf)
      (libsource (lib Transformer) (part TG111-MSC13LF) (description "Single Port Gigabit Ethernet Transformers"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D04D))
    (comp (ref C204)
      (value "1000pF, 2KV")
      (footprint Capacitor_SMD:C_1206_3216Metric)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D04C))
    (comp (ref FB3)
      (value 120R)
      (footprint Inductor_SMD:L_0402_1005Metric)
      (libsource (lib Device) (part Ferrite_Bead) (description "Ferrite bead"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D080))
    (comp (ref TP4)
      (value Test_Point)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 6099C83E))
    (comp (ref TP5)
      (value Test_Point)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 6099CA9F))
    (comp (ref TP6)
      (value Test_Point)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 6099CD2B))
    (comp (ref IC1)
      (value VSC8541XMV-01)
      (footprint Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP5.2x5.2mm)
      (fields
        (field (name CrossRef) 1))
      (libsource (lib Interface_Ethernet) (part VSC8541XMV-0x) (description "Single Port Gigabit Ethernet Copper PHY with GMII/RGMII/MII/RMII Interfaces"))
      (sheetpath (names /Ethernet/) (tstamps /5AF2BD08/))
      (tstamp 5AF1D075)))
  (libparts
    (libpart (lib Connector) (part 8P8C_LED_Shielded)
      (aliases
        (alias RJ45_LED_Shielded))
      (description "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded")
      (docs ~)
      (footprints
        (fp 8P8C*)
        (fp RJ45*))
      (fields
        (field (name Reference) J)
        (field (name Value) 8P8C_LED_Shielded))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num SH) (name ~) (type passive))))
    (libpart (lib Connector) (part ASP-134602-01)
      (description "FPGA Mezzanine Card Terminal Connector")
      (docs http://suddendocs.samtec.com/prints/asp-134602-01-mkt.pdf)
      (footprints
        (fp *FMC*ASP*134602*01*10x40*))
      (fields
        (field (name Reference) J)
        (field (name Value) ASP-134602-01)
        (field (name Footprint) Connector_Samtec:Samtec_FMC_ASP-134602-01_10x40_P1.27mm_Vertical))
      (pins
        (pin (num A1) (name Pin_1) (type passive))
        (pin (num A2) (name Pin_2) (type passive))
        (pin (num A3) (name Pin_3) (type passive))
        (pin (num A4) (name Pin_4) (type passive))
        (pin (num A5) (name Pin_5) (type passive))
        (pin (num A6) (name Pin_6) (type passive))
        (pin (num A7) (name Pin_7) (type passive))
        (pin (num A8) (name Pin_8) (type passive))
        (pin (num A9) (name Pin_9) (type passive))
        (pin (num A10) (name Pin_10) (type passive))
        (pin (num A11) (name Pin_11) (type passive))
        (pin (num A12) (name Pin_12) (type passive))
        (pin (num A13) (name Pin_13) (type passive))
        (pin (num A14) (name Pin_14) (type passive))
        (pin (num A15) (name Pin_15) (type passive))
        (pin (num A16) (name Pin_16) (type passive))
        (pin (num A17) (name Pin_17) (type passive))
        (pin (num A18) (name Pin_18) (type passive))
        (pin (num A19) (name Pin_19) (type passive))
        (pin (num A20) (name Pin_20) (type passive))
        (pin (num A21) (name Pin_21) (type passive))
        (pin (num A22) (name Pin_22) (type passive))
        (pin (num A23) (name Pin_23) (type passive))
        (pin (num A24) (name Pin_24) (type passive))
        (pin (num A25) (name Pin_25) (type passive))
        (pin (num A26) (name Pin_26) (type passive))
        (pin (num A27) (name Pin_27) (type passive))
        (pin (num A28) (name Pin_28) (type passive))
        (pin (num A29) (name Pin_29) (type passive))
        (pin (num A30) (name Pin_30) (type passive))
        (pin (num A31) (name Pin_31) (type passive))
        (pin (num A32) (name Pin_32) (type passive))
        (pin (num A33) (name Pin_33) (type passive))
        (pin (num A34) (name Pin_34) (type passive))
        (pin (num A35) (name Pin_35) (type passive))
        (pin (num A36) (name Pin_36) (type passive))
        (pin (num A37) (name Pin_37) (type passive))
        (pin (num A38) (name Pin_38) (type passive))
        (pin (num A39) (name Pin_39) (type passive))
        (pin (num A40) (name Pin_40) (type passive))
        (pin (num B1) (name Pin_1) (type passive))
        (pin (num B2) (name Pin_2) (type passive))
        (pin (num B3) (name Pin_3) (type passive))
        (pin (num B4) (name Pin_4) (type passive))
        (pin (num B5) (name Pin_5) (type passive))
        (pin (num B6) (name Pin_6) (type passive))
        (pin (num B7) (name Pin_7) (type passive))
        (pin (num B8) (name Pin_8) (type passive))
        (pin (num B9) (name Pin_9) (type passive))
        (pin (num B10) (name Pin_10) (type passive))
        (pin (num B11) (name Pin_11) (type passive))
        (pin (num B12) (name Pin_12) (type passive))
        (pin (num B13) (name Pin_13) (type passive))
        (pin (num B14) (name Pin_14) (type passive))
        (pin (num B15) (name Pin_15) (type passive))
        (pin (num B16) (name Pin_16) (type passive))
        (pin (num B17) (name Pin_17) (type passive))
        (pin (num B18) (name Pin_18) (type passive))
        (pin (num B19) (name Pin_19) (type passive))
        (pin (num B20) (name Pin_20) (type passive))
        (pin (num B21) (name Pin_21) (type passive))
        (pin (num B22) (name Pin_22) (type passive))
        (pin (num B23) (name Pin_23) (type passive))
        (pin (num B24) (name Pin_24) (type passive))
        (pin (num B25) (name Pin_25) (type passive))
        (pin (num B26) (name Pin_26) (type passive))
        (pin (num B27) (name Pin_27) (type passive))
        (pin (num B28) (name Pin_28) (type passive))
        (pin (num B29) (name Pin_29) (type passive))
        (pin (num B30) (name Pin_30) (type passive))
        (pin (num B31) (name Pin_31) (type passive))
        (pin (num B32) (name Pin_32) (type passive))
        (pin (num B33) (name Pin_33) (type passive))
        (pin (num B34) (name Pin_34) (type passive))
        (pin (num B35) (name Pin_35) (type passive))
        (pin (num B36) (name Pin_36) (type passive))
        (pin (num B37) (name Pin_37) (type passive))
        (pin (num B38) (name Pin_38) (type passive))
        (pin (num B39) (name Pin_39) (type passive))
        (pin (num B40) (name Pin_40) (type passive))
        (pin (num C1) (name Pin_1) (type passive))
        (pin (num C2) (name Pin_2) (type passive))
        (pin (num C3) (name Pin_3) (type passive))
        (pin (num C4) (name Pin_4) (type passive))
        (pin (num C5) (name Pin_5) (type passive))
        (pin (num C6) (name Pin_6) (type passive))
        (pin (num C7) (name Pin_7) (type passive))
        (pin (num C8) (name Pin_8) (type passive))
        (pin (num C9) (name Pin_9) (type passive))
        (pin (num C10) (name Pin_10) (type passive))
        (pin (num C11) (name Pin_11) (type passive))
        (pin (num C12) (name Pin_12) (type passive))
        (pin (num C13) (name Pin_13) (type passive))
        (pin (num C14) (name Pin_14) (type passive))
        (pin (num C15) (name Pin_15) (type passive))
        (pin (num C16) (name Pin_16) (type passive))
        (pin (num C17) (name Pin_17) (type passive))
        (pin (num C18) (name Pin_18) (type passive))
        (pin (num C19) (name Pin_19) (type passive))
        (pin (num C20) (name Pin_20) (type passive))
        (pin (num C21) (name Pin_21) (type passive))
        (pin (num C22) (name Pin_22) (type passive))
        (pin (num C23) (name Pin_23) (type passive))
        (pin (num C24) (name Pin_24) (type passive))
        (pin (num C25) (name Pin_25) (type passive))
        (pin (num C26) (name Pin_26) (type passive))
        (pin (num C27) (name Pin_27) (type passive))
        (pin (num C28) (name Pin_28) (type passive))
        (pin (num C29) (name Pin_29) (type passive))
        (pin (num C30) (name Pin_30) (type passive))
        (pin (num C31) (name Pin_31) (type passive))
        (pin (num C32) (name Pin_32) (type passive))
        (pin (num C33) (name Pin_33) (type passive))
        (pin (num C34) (name Pin_34) (type passive))
        (pin (num C35) (name Pin_35) (type passive))
        (pin (num C36) (name Pin_36) (type passive))
        (pin (num C37) (name Pin_37) (type passive))
        (pin (num C38) (name Pin_38) (type passive))
        (pin (num C39) (name Pin_39) (type passive))
        (pin (num C40) (name Pin_40) (type passive))
        (pin (num D1) (name Pin_1) (type passive))
        (pin (num D2) (name Pin_2) (type passive))
        (pin (num D3) (name Pin_3) (type passive))
        (pin (num D4) (name Pin_4) (type passive))
        (pin (num D5) (name Pin_5) (type passive))
        (pin (num D6) (name Pin_6) (type passive))
        (pin (num D7) (name Pin_7) (type passive))
        (pin (num D8) (name Pin_8) (type passive))
        (pin (num D9) (name Pin_9) (type passive))
        (pin (num D10) (name Pin_10) (type passive))
        (pin (num D11) (name Pin_11) (type passive))
        (pin (num D12) (name Pin_12) (type passive))
        (pin (num D13) (name Pin_13) (type passive))
        (pin (num D14) (name Pin_14) (type passive))
        (pin (num D15) (name Pin_15) (type passive))
        (pin (num D16) (name Pin_16) (type passive))
        (pin (num D17) (name Pin_17) (type passive))
        (pin (num D18) (name Pin_18) (type passive))
        (pin (num D19) (name Pin_19) (type passive))
        (pin (num D20) (name Pin_20) (type passive))
        (pin (num D21) (name Pin_21) (type passive))
        (pin (num D22) (name Pin_22) (type passive))
        (pin (num D23) (name Pin_23) (type passive))
        (pin (num D24) (name Pin_24) (type passive))
        (pin (num D25) (name Pin_25) (type passive))
        (pin (num D26) (name Pin_26) (type passive))
        (pin (num D27) (name Pin_27) (type passive))
        (pin (num D28) (name Pin_28) (type passive))
        (pin (num D29) (name Pin_29) (type passive))
        (pin (num D30) (name Pin_30) (type passive))
        (pin (num D31) (name Pin_31) (type passive))
        (pin (num D32) (name Pin_32) (type passive))
        (pin (num D33) (name Pin_33) (type passive))
        (pin (num D34) (name Pin_34) (type passive))
        (pin (num D35) (name Pin_35) (type passive))
        (pin (num D36) (name Pin_36) (type passive))
        (pin (num D37) (name Pin_37) (type passive))
        (pin (num D38) (name Pin_38) (type passive))
        (pin (num D39) (name Pin_39) (type passive))
        (pin (num D40) (name Pin_40) (type passive))
        (pin (num E1) (name Pin_1) (type passive))
        (pin (num E2) (name Pin_2) (type passive))
        (pin (num E3) (name Pin_3) (type passive))
        (pin (num E4) (name Pin_4) (type passive))
        (pin (num E5) (name Pin_5) (type passive))
        (pin (num E6) (name Pin_6) (type passive))
        (pin (num E7) (name Pin_7) (type passive))
        (pin (num E8) (name Pin_8) (type passive))
        (pin (num E9) (name Pin_9) (type passive))
        (pin (num E10) (name Pin_10) (type passive))
        (pin (num E11) (name Pin_11) (type passive))
        (pin (num E12) (name Pin_12) (type passive))
        (pin (num E13) (name Pin_13) (type passive))
        (pin (num E14) (name Pin_14) (type passive))
        (pin (num E15) (name Pin_15) (type passive))
        (pin (num E16) (name Pin_16) (type passive))
        (pin (num E17) (name Pin_17) (type passive))
        (pin (num E18) (name Pin_18) (type passive))
        (pin (num E19) (name Pin_19) (type passive))
        (pin (num E20) (name Pin_20) (type passive))
        (pin (num E21) (name Pin_21) (type passive))
        (pin (num E22) (name Pin_22) (type passive))
        (pin (num E23) (name Pin_23) (type passive))
        (pin (num E24) (name Pin_24) (type passive))
        (pin (num E25) (name Pin_25) (type passive))
        (pin (num E26) (name Pin_26) (type passive))
        (pin (num E27) (name Pin_27) (type passive))
        (pin (num E28) (name Pin_28) (type passive))
        (pin (num E29) (name Pin_29) (type passive))
        (pin (num E30) (name Pin_30) (type passive))
        (pin (num E31) (name Pin_31) (type passive))
        (pin (num E32) (name Pin_32) (type passive))
        (pin (num E33) (name Pin_33) (type passive))
        (pin (num E34) (name Pin_34) (type passive))
        (pin (num E35) (name Pin_35) (type passive))
        (pin (num E36) (name Pin_36) (type passive))
        (pin (num E37) (name Pin_37) (type passive))
        (pin (num E38) (name Pin_38) (type passive))
        (pin (num E39) (name Pin_39) (type passive))
        (pin (num E40) (name Pin_40) (type passive))
        (pin (num F1) (name Pin_1) (type passive))
        (pin (num F2) (name Pin_2) (type passive))
        (pin (num F3) (name Pin_3) (type passive))
        (pin (num F4) (name Pin_4) (type passive))
        (pin (num F5) (name Pin_5) (type passive))
        (pin (num F6) (name Pin_6) (type passive))
        (pin (num F7) (name Pin_7) (type passive))
        (pin (num F8) (name Pin_8) (type passive))
        (pin (num F9) (name Pin_9) (type passive))
        (pin (num F10) (name Pin_10) (type passive))
        (pin (num F11) (name Pin_11) (type passive))
        (pin (num F12) (name Pin_12) (type passive))
        (pin (num F13) (name Pin_13) (type passive))
        (pin (num F14) (name Pin_14) (type passive))
        (pin (num F15) (name Pin_15) (type passive))
        (pin (num F16) (name Pin_16) (type passive))
        (pin (num F17) (name Pin_17) (type passive))
        (pin (num F18) (name Pin_18) (type passive))
        (pin (num F19) (name Pin_19) (type passive))
        (pin (num F20) (name Pin_20) (type passive))
        (pin (num F21) (name Pin_21) (type passive))
        (pin (num F22) (name Pin_22) (type passive))
        (pin (num F23) (name Pin_23) (type passive))
        (pin (num F24) (name Pin_24) (type passive))
        (pin (num F25) (name Pin_25) (type passive))
        (pin (num F26) (name Pin_26) (type passive))
        (pin (num F27) (name Pin_27) (type passive))
        (pin (num F28) (name Pin_28) (type passive))
        (pin (num F29) (name Pin_29) (type passive))
        (pin (num F30) (name Pin_30) (type passive))
        (pin (num F31) (name Pin_31) (type passive))
        (pin (num F32) (name Pin_32) (type passive))
        (pin (num F33) (name Pin_33) (type passive))
        (pin (num F34) (name Pin_34) (type passive))
        (pin (num F35) (name Pin_35) (type passive))
        (pin (num F36) (name Pin_36) (type passive))
        (pin (num F37) (name Pin_37) (type passive))
        (pin (num F38) (name Pin_38) (type passive))
        (pin (num F39) (name Pin_39) (type passive))
        (pin (num F40) (name Pin_40) (type passive))
        (pin (num G1) (name Pin_1) (type passive))
        (pin (num G2) (name Pin_2) (type passive))
        (pin (num G3) (name Pin_3) (type passive))
        (pin (num G4) (name Pin_4) (type passive))
        (pin (num G5) (name Pin_5) (type passive))
        (pin (num G6) (name Pin_6) (type passive))
        (pin (num G7) (name Pin_7) (type passive))
        (pin (num G8) (name Pin_8) (type passive))
        (pin (num G9) (name Pin_9) (type passive))
        (pin (num G10) (name Pin_10) (type passive))
        (pin (num G11) (name Pin_11) (type passive))
        (pin (num G12) (name Pin_12) (type passive))
        (pin (num G13) (name Pin_13) (type passive))
        (pin (num G14) (name Pin_14) (type passive))
        (pin (num G15) (name Pin_15) (type passive))
        (pin (num G16) (name Pin_16) (type passive))
        (pin (num G17) (name Pin_17) (type passive))
        (pin (num G18) (name Pin_18) (type passive))
        (pin (num G19) (name Pin_19) (type passive))
        (pin (num G20) (name Pin_20) (type passive))
        (pin (num G21) (name Pin_21) (type passive))
        (pin (num G22) (name Pin_22) (type passive))
        (pin (num G23) (name Pin_23) (type passive))
        (pin (num G24) (name Pin_24) (type passive))
        (pin (num G25) (name Pin_25) (type passive))
        (pin (num G26) (name Pin_26) (type passive))
        (pin (num G27) (name Pin_27) (type passive))
        (pin (num G28) (name Pin_28) (type passive))
        (pin (num G29) (name Pin_29) (type passive))
        (pin (num G30) (name Pin_30) (type passive))
        (pin (num G31) (name Pin_31) (type passive))
        (pin (num G32) (name Pin_32) (type passive))
        (pin (num G33) (name Pin_33) (type passive))
        (pin (num G34) (name Pin_34) (type passive))
        (pin (num G35) (name Pin_35) (type passive))
        (pin (num G36) (name Pin_36) (type passive))
        (pin (num G37) (name Pin_37) (type passive))
        (pin (num G38) (name Pin_38) (type passive))
        (pin (num G39) (name Pin_39) (type passive))
        (pin (num G40) (name Pin_40) (type passive))
        (pin (num H1) (name Pin_1) (type passive))
        (pin (num H2) (name Pin_2) (type passive))
        (pin (num H3) (name Pin_3) (type passive))
        (pin (num H4) (name Pin_4) (type passive))
        (pin (num H5) (name Pin_5) (type passive))
        (pin (num H6) (name Pin_6) (type passive))
        (pin (num H7) (name Pin_7) (type passive))
        (pin (num H8) (name Pin_8) (type passive))
        (pin (num H9) (name Pin_9) (type passive))
        (pin (num H10) (name Pin_10) (type passive))
        (pin (num H11) (name Pin_11) (type passive))
        (pin (num H12) (name Pin_12) (type passive))
        (pin (num H13) (name Pin_13) (type passive))
        (pin (num H14) (name Pin_14) (type passive))
        (pin (num H15) (name Pin_15) (type passive))
        (pin (num H16) (name Pin_16) (type passive))
        (pin (num H17) (name Pin_17) (type passive))
        (pin (num H18) (name Pin_18) (type passive))
        (pin (num H19) (name Pin_19) (type passive))
        (pin (num H20) (name Pin_20) (type passive))
        (pin (num H21) (name Pin_21) (type passive))
        (pin (num H22) (name Pin_22) (type passive))
        (pin (num H23) (name Pin_23) (type passive))
        (pin (num H24) (name Pin_24) (type passive))
        (pin (num H25) (name Pin_25) (type passive))
        (pin (num H26) (name Pin_26) (type passive))
        (pin (num H27) (name Pin_27) (type passive))
        (pin (num H28) (name Pin_28) (type passive))
        (pin (num H29) (name Pin_29) (type passive))
        (pin (num H30) (name Pin_30) (type passive))
        (pin (num H31) (name Pin_31) (type passive))
        (pin (num H32) (name Pin_32) (type passive))
        (pin (num H33) (name Pin_33) (type passive))
        (pin (num H34) (name Pin_34) (type passive))
        (pin (num H35) (name Pin_35) (type passive))
        (pin (num H36) (name Pin_36) (type passive))
        (pin (num H37) (name Pin_37) (type passive))
        (pin (num H38) (name Pin_38) (type passive))
        (pin (num H39) (name Pin_39) (type passive))
        (pin (num H40) (name Pin_40) (type passive))
        (pin (num J1) (name Pin_1) (type passive))
        (pin (num J2) (name Pin_2) (type passive))
        (pin (num J3) (name Pin_3) (type passive))
        (pin (num J4) (name Pin_4) (type passive))
        (pin (num J5) (name Pin_5) (type passive))
        (pin (num J6) (name Pin_6) (type passive))
        (pin (num J7) (name Pin_7) (type passive))
        (pin (num J8) (name Pin_8) (type passive))
        (pin (num J9) (name Pin_9) (type passive))
        (pin (num J10) (name Pin_10) (type passive))
        (pin (num J11) (name Pin_11) (type passive))
        (pin (num J12) (name Pin_12) (type passive))
        (pin (num J13) (name Pin_13) (type passive))
        (pin (num J14) (name Pin_14) (type passive))
        (pin (num J15) (name Pin_15) (type passive))
        (pin (num J16) (name Pin_16) (type passive))
        (pin (num J17) (name Pin_17) (type passive))
        (pin (num J18) (name Pin_18) (type passive))
        (pin (num J19) (name Pin_19) (type passive))
        (pin (num J20) (name Pin_20) (type passive))
        (pin (num J21) (name Pin_21) (type passive))
        (pin (num J22) (name Pin_22) (type passive))
        (pin (num J23) (name Pin_23) (type passive))
        (pin (num J24) (name Pin_24) (type passive))
        (pin (num J25) (name Pin_25) (type passive))
        (pin (num J26) (name Pin_26) (type passive))
        (pin (num J27) (name Pin_27) (type passive))
        (pin (num J28) (name Pin_28) (type passive))
        (pin (num J29) (name Pin_29) (type passive))
        (pin (num J30) (name Pin_30) (type passive))
        (pin (num J31) (name Pin_31) (type passive))
        (pin (num J32) (name Pin_32) (type passive))
        (pin (num J33) (name Pin_33) (type passive))
        (pin (num J34) (name Pin_34) (type passive))
        (pin (num J35) (name Pin_35) (type passive))
        (pin (num J36) (name Pin_36) (type passive))
        (pin (num J37) (name Pin_37) (type passive))
        (pin (num J38) (name Pin_38) (type passive))
        (pin (num J39) (name Pin_39) (type passive))
        (pin (num J40) (name Pin_40) (type passive))
        (pin (num K1) (name Pin_1) (type passive))
        (pin (num K2) (name Pin_2) (type passive))
        (pin (num K3) (name Pin_3) (type passive))
        (pin (num K4) (name Pin_4) (type passive))
        (pin (num K5) (name Pin_5) (type passive))
        (pin (num K6) (name Pin_6) (type passive))
        (pin (num K7) (name Pin_7) (type passive))
        (pin (num K8) (name Pin_8) (type passive))
        (pin (num K9) (name Pin_9) (type passive))
        (pin (num K10) (name Pin_10) (type passive))
        (pin (num K11) (name Pin_11) (type passive))
        (pin (num K12) (name Pin_12) (type passive))
        (pin (num K13) (name Pin_13) (type passive))
        (pin (num K14) (name Pin_14) (type passive))
        (pin (num K15) (name Pin_15) (type passive))
        (pin (num K16) (name Pin_16) (type passive))
        (pin (num K17) (name Pin_17) (type passive))
        (pin (num K18) (name Pin_18) (type passive))
        (pin (num K19) (name Pin_19) (type passive))
        (pin (num K20) (name Pin_20) (type passive))
        (pin (num K21) (name Pin_21) (type passive))
        (pin (num K22) (name Pin_22) (type passive))
        (pin (num K23) (name Pin_23) (type passive))
        (pin (num K24) (name Pin_24) (type passive))
        (pin (num K25) (name Pin_25) (type passive))
        (pin (num K26) (name Pin_26) (type passive))
        (pin (num K27) (name Pin_27) (type passive))
        (pin (num K28) (name Pin_28) (type passive))
        (pin (num K29) (name Pin_29) (type passive))
        (pin (num K30) (name Pin_30) (type passive))
        (pin (num K31) (name Pin_31) (type passive))
        (pin (num K32) (name Pin_32) (type passive))
        (pin (num K33) (name Pin_33) (type passive))
        (pin (num K34) (name Pin_34) (type passive))
        (pin (num K35) (name Pin_35) (type passive))
        (pin (num K36) (name Pin_36) (type passive))
        (pin (num K37) (name Pin_37) (type passive))
        (pin (num K38) (name Pin_38) (type passive))
        (pin (num K39) (name Pin_39) (type passive))
        (pin (num K40) (name Pin_40) (type passive))))
    (libpart (lib Connector) (part Barrel_Jack)
      (aliases
        (alias Jack-DC))
      (description "DC Barrel Jack")
      (docs ~)
      (footprints
        (fp BarrelJack*))
      (fields
        (field (name Reference) J)
        (field (name Value) Barrel_Jack))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Connector) (part Micro_SD_Card_Det)
      (aliases
        (alias Micro_SD_Card_Det_Hirose_DM3AT))
      (description "Micro SD Card Socket with card detection pins")
      (docs https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1)
      (footprints
        (fp microSD*))
      (fields
        (field (name Reference) J)
        (field (name Value) Micro_SD_Card_Det))
      (pins
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type input))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type input))
        (pin (num 8) (name DAT1) (type input))
        (pin (num 9) (name DET_B) (type passive))
        (pin (num 10) (name DET_A) (type passive))
        (pin (num 11) (name SHIELD) (type passive))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x04_Odd_Even)
      (description "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x04_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x05_Odd_Even)
      (description "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x05_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x10_Odd_Even)
      (description "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x10_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x11_Odd_Even)
      (description "Generic connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x11_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP1)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_GND2)
      (description "Three pin crystal (GND on pin 2), e.g. in SMD package")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_TVS)
      (description "Bidirectional transient-voltage-suppression (TVS) diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_TVS))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Device) (part D_Zener)
      (description "Zener Diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Zener))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead)
      (description "Ferrite bead")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "LED generic")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Pack04)
      (description "4 Resistor network, parallel topology, DIP package")
      (docs ~)
      (footprints
        (fp DIP*)
        (fp SOIC*))
      (fields
        (field (name Reference) RN)
        (field (name Value) R_Pack04))
      (pins
        (pin (num 1) (name R1.1) (type passive))
        (pin (num 2) (name R2.1) (type passive))
        (pin (num 3) (name R3.1) (type passive))
        (pin (num 4) (name R4.1) (type passive))
        (pin (num 5) (name R4.2) (type passive))
        (pin (num 6) (name R3.2) (type passive))
        (pin (num 7) (name R2.2) (type passive))
        (pin (num 8) (name R1.2) (type passive))))
    (libpart (lib Device) (part R_Shunt)
      (description "Shunt Resistor")
      (docs ~)
      (footprints
        (fp R_*Shunt*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Shunt))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Diode) (part 1N4148WT)
      (aliases
        (alias 1N4448WT)
        (alias 1N914WT))
      (description "75V 0.15A Fast switching Diode, SOD-523")
      (docs https://www.diodes.com/assets/Datasheets/ds30396.pdf)
      (footprints
        (fp D*SOD?523*))
      (fields
        (field (name Reference) D)
        (field (name Value) 1N4148WT)
        (field (name Footprint) Diode_SMD:D_SOD-523))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Interface_Ethernet) (part VSC8541XMV-0x)
      (description "Single Port Gigabit Ethernet Copper PHY with GMII/RGMII/MII/RMII Interfaces")
      (docs https://www.mouser.com/ds/2/523/Microsemi_VSC8541-01_Datasheet_10496_V40-1148034.pdf)
      (footprints
        (fp QFN?68*1EP*8x8mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) VSC8541XMV-0x))
      (pins
        (pin (num 1) (name REF_REXT) (type passive))
        (pin (num 2) (name VDD25A1) (type power_in))
        (pin (num 3) (name P0_D3N) (type passive))
        (pin (num 4) (name P0_D3P) (type passive))
        (pin (num 5) (name VDD1A1) (type power_in))
        (pin (num 6) (name P0_D2N) (type passive))
        (pin (num 7) (name P0_D2P) (type passive))
        (pin (num 8) (name VDD25A2) (type power_in))
        (pin (num 9) (name P0_D1N) (type passive))
        (pin (num 10) (name P0_D1P) (type passive))
        (pin (num 11) (name VDD25A3) (type power_in))
        (pin (num 12) (name P0_D0N) (type passive))
        (pin (num 13) (name P0_D0P) (type passive))
        (pin (num 14) (name VDD1A2) (type power_in))
        (pin (num 15) (name THERMDA) (type passive))
        (pin (num 16) (name THERMDC_VSS) (type passive))
        (pin (num 17) (name VDD11) (type power_in))
        (pin (num 18) (name COL) (type BiDi))
        (pin (num 19) (name CRS) (type BiDi))
        (pin (num 20) (name RXD7) (type BiDi))
        (pin (num 21) (name RXD6) (type BiDi))
        (pin (num 22) (name VDDMAC1) (type power_in))
        (pin (num 23) (name RXD5) (type BiDi))
        (pin (num 24) (name RXD4) (type BiDi))
        (pin (num 25) (name RXD3) (type BiDi))
        (pin (num 26) (name RXD2) (type BiDi))
        (pin (num 27) (name RXD1) (type BiDi))
        (pin (num 28) (name VDDMAC2) (type power_in))
        (pin (num 29) (name RXD0) (type BiDi))
        (pin (num 30) (name RX_DV/RX_CTL) (type BiDi))
        (pin (num 31) (name RX_ER) (type BiDi))
        (pin (num 32) (name RX_CLK) (type BiDi))
        (pin (num 33) (name TX_EN/TX_CTL) (type input))
        (pin (num 34) (name VDD12) (type power_in))
        (pin (num 35) (name TX_ER) (type input))
        (pin (num 36) (name MII_TXCLK) (type output))
        (pin (num 37) (name GTX_CLK) (type input))
        (pin (num 38) (name TXD0) (type input))
        (pin (num 39) (name VDDMAC3) (type power_in))
        (pin (num 40) (name TXD1) (type input))
        (pin (num 41) (name TXD2) (type input))
        (pin (num 42) (name TXD3) (type input))
        (pin (num 43) (name TXD4) (type input))
        (pin (num 44) (name VDDMAC4) (type power_in))
        (pin (num 45) (name TXD5) (type input))
        (pin (num 46) (name TXD6) (type input))
        (pin (num 47) (name TXD7) (type input))
        (pin (num 48) (name MDC) (type input))
        (pin (num 49) (name VDDMDIO) (type power_in))
        (pin (num 50) (name MDIO) (type BiDi))
        (pin (num 51) (name MDINT) (type output))
        (pin (num 52) (name FASTLINK_FAIL) (type output))
        (pin (num 53) (name NRESET) (type input))
        (pin (num 54) (name CLKOUT) (type output))
        (pin (num 55) (name RCVRD_CLK) (type output))
        (pin (num 56) (name COMA_MODE) (type input))
        (pin (num 57) (name CLK_SQUELCH_IN) (type input))
        (pin (num 58) (name VDDIO) (type power_in))
        (pin (num 59) (name LED1) (type output))
        (pin (num 60) (name LED0) (type output))
        (pin (num 61) (name REFCLK_SEL_1) (type input))
        (pin (num 62) (name REFCLK_SEL_0) (type input))
        (pin (num 63) (name XTAL1) (type input))
        (pin (num 64) (name XTAL2) (type output))
        (pin (num 65) (name RESERVED_1) (type passive))
        (pin (num 66) (name RESERVED_0) (type passive))
        (pin (num 67) (name REF_FILT) (type passive))
        (pin (num 68) (name VDD1A3) (type power_in))
        (pin (num 69) (name P_GND) (type power_in))))
    (libpart (lib Interface_USB) (part FT2232H)
      (description "FT2232Hx, Hi Speed Double Channel USB UART/FIFO, LQFP/QFN-64")
      (docs http://www.ftdichip.com/Products/ICs/FT2232H.html)
      (footprints
        (fp QFN*)
        (fp LQFP*))
      (fields
        (field (name Reference) U)
        (field (name Value) FT2232H))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name OSCI) (type input))
        (pin (num 3) (name OSCO) (type output))
        (pin (num 4) (name VPHY) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name REF) (type output))
        (pin (num 7) (name DM) (type BiDi))
        (pin (num 8) (name DP) (type BiDi))
        (pin (num 9) (name VPLL) (type input))
        (pin (num 10) (name AGND) (type power_in))
        (pin (num 11) (name GND) (type power_in))
        (pin (num 12) (name VCORE) (type power_in))
        (pin (num 13) (name TEST) (type input))
        (pin (num 14) (name ~RESET) (type input))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name ADBUS0) (type BiDi))
        (pin (num 17) (name ADBUS1) (type BiDi))
        (pin (num 18) (name ADBUS2) (type BiDi))
        (pin (num 19) (name ADBUS3) (type BiDi))
        (pin (num 20) (name VCCIO) (type power_in))
        (pin (num 21) (name ADBUS4) (type BiDi))
        (pin (num 22) (name ADBUS5) (type BiDi))
        (pin (num 23) (name ADBUS6) (type BiDi))
        (pin (num 24) (name ADBUS7) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name ACBUS0) (type BiDi))
        (pin (num 27) (name ACBUS1) (type BiDi))
        (pin (num 28) (name ACBUS2) (type BiDi))
        (pin (num 29) (name ACBUS3) (type BiDi))
        (pin (num 30) (name ACBUS4) (type BiDi))
        (pin (num 31) (name VCCIO) (type power_in))
        (pin (num 32) (name ACBUS5) (type BiDi))
        (pin (num 33) (name ACBUS6) (type BiDi))
        (pin (num 34) (name ACBUS7) (type BiDi))
        (pin (num 35) (name GND) (type power_in))
        (pin (num 36) (name ~SUSPEND) (type output))
        (pin (num 37) (name VCORE) (type power_in))
        (pin (num 38) (name BDBUS0) (type BiDi))
        (pin (num 39) (name BDBUS1) (type BiDi))
        (pin (num 40) (name BDBUS2) (type BiDi))
        (pin (num 41) (name BDBUS3) (type BiDi))
        (pin (num 42) (name VCCIO) (type power_in))
        (pin (num 43) (name BDBUS4) (type BiDi))
        (pin (num 44) (name BDBUS5) (type BiDi))
        (pin (num 45) (name BDBUS6) (type BiDi))
        (pin (num 46) (name BDBUS7) (type BiDi))
        (pin (num 47) (name GND) (type power_in))
        (pin (num 48) (name BCBUS0) (type BiDi))
        (pin (num 49) (name VREGOUT) (type power_out))
        (pin (num 50) (name VREGIN) (type power_in))
        (pin (num 51) (name GND) (type power_in))
        (pin (num 52) (name BCBUS1) (type BiDi))
        (pin (num 53) (name BCBUS2) (type BiDi))
        (pin (num 54) (name BCBUS3) (type BiDi))
        (pin (num 55) (name BCBUS4) (type BiDi))
        (pin (num 56) (name VCCIO) (type power_in))
        (pin (num 57) (name BCBUS5) (type BiDi))
        (pin (num 58) (name BCBUS6) (type BiDi))
        (pin (num 59) (name BCBUS7) (type BiDi))
        (pin (num 60) (name ~PWREN) (type output))
        (pin (num 61) (name EEDATA) (type BiDi))
        (pin (num 62) (name EECLK) (type output))
        (pin (num 63) (name EECS) (type output))
        (pin (num 64) (name VCORE) (type power_in))))
    (libpart (lib Logic_LevelTranslator) (part SN74AUP1T34DCK)
      (description "1-Bit Unidirectional Voltage-Level Translator, SC-70")
      (docs http://www.ti.com/lit/ds/symlink/sn74aup1t34.pdf)
      (footprints
        (fp SOT?353*SC?70?5*))
      (fields
        (field (name Reference) U)
        (field (name Value) SN74AUP1T34DCK)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-353_SC-70-5))
      (pins
        (pin (num 1) (name VCCA) (type power_in))
        (pin (num 2) (name A) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name B) (type 3state))
        (pin (num 5) (name VCCB) (type power_in))))
    (libpart (lib MCU_SiFive) (part FU540-C000)
      (description " 64-bit RISC‑V SoC")
      (docs https://static.dev.sifive.com/FU540-C000-v1.0.pdf)
      (footprints
        (fp BGA?484*23.0x23.0mm*P1.0mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) FU540-C000))
      (pins
        (pin (num A1) (name VSS) (type power_in))
        (pin (num A2) (name VSS) (type power_in))
        (pin (num A3) (name VSS) (type power_in))
        (pin (num A4) (name IO_DDR_MEM_DATA[18]) (type BiDi))
        (pin (num A5) (name IO_DDR_MEM_DATA[19]) (type BiDi))
        (pin (num A6) (name IO_DDR_MEM_DQS_P[2]) (type BiDi))
        (pin (num A7) (name IO_DDR_MEM_DQS_M[2]) (type BiDi))
        (pin (num A8) (name IO_GEMGXL_0_RXD_5) (type input))
        (pin (num A9) (name VSS) (type power_in))
        (pin (num A10) (name IO_GEMGXL_0_RXD_2) (type input))
        (pin (num A11) (name IO_GEMGXL_0_RX_DV) (type input))
        (pin (num A12) (name IO_GEMGXL_0_RXD_0) (type input))
        (pin (num A13) (name IO_GEMGXL_0_COL) (type input))
        (pin (num A14) (name VSS) (type power_in))
        (pin (num A15) (name HFXOSCIN) (type passive))
        (pin (num A16) (name IO_PRCI_RSVD0) (type passive))
        (pin (num A17) (name IO_PRCI_PORESET_N) (type input))
        (pin (num A18) (name VSS) (type power_in))
        (pin (num A19) (name IO_MSEL_MSEL_0) (type input))
        (pin (num A20) (name IO_MSEL_MSEL_2) (type input))
        (pin (num A21) (name IO_GPIO_0_PINS_9) (type BiDi))
        (pin (num A22) (name VSS) (type power_in))
        (pin (num AA1) (name IO_DDR_MEM_DATA[41]) (type BiDi))
        (pin (num AA2) (name VSS) (type power_in))
        (pin (num AA3) (name IO_DDR_MEM_DATA[45]) (type BiDi))
        (pin (num AA4) (name IO_DDR_MEM_DATA[47]) (type BiDi))
        (pin (num AA5) (name IO_DDR_MEM_ODT[0]) (type output))
        (pin (num AA6) (name IO_DDR_MEM_CKE[1]) (type output))
        (pin (num AA7) (name IO_DDR_MEM_DQS_M[6]) (type BiDi))
        (pin (num AA8) (name IO_DDR_MEM_DQS_P[7]) (type BiDi))
        (pin (num AA9) (name IO_DDR_MEM_DATA[62]) (type BiDi))
        (pin (num AA10) (name IO_DDR_MEM_DATA[61]) (type BiDi))
        (pin (num AA11) (name IO_DDR_MEM_DATA[63]) (type BiDi))
        (pin (num AA12) (name IO_DDR_MEM_DATA[58]) (type BiDi))
        (pin (num AA13) (name IO_DDR_MEM_DATA[56]) (type BiDi))
        (pin (num AA14) (name IO_UART_1_RXD) (type input))
        (pin (num AA15) (name IO_UART_1_TXD) (type output))
        (pin (num AA16) (name IO_QSPI_2_DQ_0) (type BiDi))
        (pin (num AA17) (name VDD) (type power_in))
        (pin (num AA18) (name IO_CHIPLINK_0_B2C_DATA_2) (type input))
        (pin (num AA19) (name IO_CHIPLINK_0_B2C_DATA_8) (type input))
        (pin (num AA20) (name IO_CHIPLINK_0_B2C_DATA_23) (type input))
        (pin (num AA21) (name IO_CHIPLINK_0_B2C_DATA_29) (type input))
        (pin (num AA22) (name IO_CHIPLINK_0_B2C_CLK) (type input))
        (pin (num AB1) (name VSS) (type power_in))
        (pin (num AB2) (name IO_DDR_MEM_DATA[44]) (type BiDi))
        (pin (num AB3) (name IO_DDR_MEM_DATA[46]) (type BiDi))
        (pin (num AB4) (name VSS) (type power_in))
        (pin (num AB5) (name IO_DDR_MEM_ODT[1]) (type output))
        (pin (num AB6) (name IO_DDR_MEM_CKE[0]) (type output))
        (pin (num AB7) (name VSS) (type power_in))
        (pin (num AB8) (name IO_DDR_MEM_DATA[57]) (type BiDi))
        (pin (num AB9) (name IO_DDR_MEM_DATA[59]) (type BiDi))
        (pin (num AB10) (name VSS) (type power_in))
        (pin (num AB11) (name IO_DDR_MEM_DATA[60]) (type BiDi))
        (pin (num AB12) (name IO_DDR_MEM_DM[7]) (type BiDi))
        (pin (num AB13) (name VSS) (type power_in))
        (pin (num AB14) (name IO_QSPI_2_CS_0) (type output))
        (pin (num AB15) (name IO_QSPI_2_DQ_1) (type BiDi))
        (pin (num AB16) (name IO_QSPI_2_DQ_2) (type BiDi))
        (pin (num AB17) (name VSS) (type power_in))
        (pin (num AB18) (name IO_CHIPLINK_0_B2C_DATA_1) (type input))
        (pin (num AB19) (name IO_CHIPLINK_0_B2C_DATA_13) (type input))
        (pin (num AB20) (name IO_CHIPLINK_0_B2C_DATA_22) (type input))
        (pin (num AB21) (name IO_CHIPLINK_0_B2C_DATA_26) (type input))
        (pin (num AB22) (name VSS) (type power_in))
        (pin (num B1) (name IO_DDR_MEM_DATA[1]) (type BiDi))
        (pin (num B2) (name IO_DDR_MEM_DATA[17]) (type BiDi))
        (pin (num B3) (name IO_DDR_MEM_DATA[22]) (type BiDi))
        (pin (num B4) (name IO_DDR_MEM_DATA[16]) (type BiDi))
        (pin (num B5) (name IO_DDR_MEM_DATA[20]) (type BiDi))
        (pin (num B6) (name IO_DDR_MEM_DATA[23]) (type BiDi))
        (pin (num B7) (name IO_GEMGXL_0_TX_EN) (type output))
        (pin (num B8) (name IO_GEMGXL_0_TXD_6) (type output))
        (pin (num B9) (name VDD) (type power_in))
        (pin (num B10) (name IO_GEMGXL_0_RXD_1) (type input))
        (pin (num B11) (name IO_GEMGXL_0_RX_ER) (type input))
        (pin (num B12) (name IO_GEMGXL_0_TXD_0) (type output))
        (pin (num B13) (name IO_GEMGXL_0_MDC) (type output))
        (pin (num B14) (name VDD) (type power_in))
        (pin (num B15) (name HFXOSCOUT) (type passive))
        (pin (num B16) (name IO_PRCI_RTCXALTCLKIN) (type passive))
        (pin (num B17) (name IO_PRCI_RSVD6) (type passive))
        (pin (num B18) (name VDD) (type power_in))
        (pin (num B19) (name IO_MSEL_MSEL_3) (type input))
        (pin (num B20) (name IO_GPIO_0_PINS_11) (type BiDi))
        (pin (num B21) (name IO_GPIO_0_PINS_12) (type BiDi))
        (pin (num B22) (name IO_GPIO_0_PINS_14) (type BiDi))
        (pin (num C1) (name IO_DDR_MEM_DATA[4]) (type BiDi))
        (pin (num C2) (name IO_DDR_MEM_DATA[29]) (type BiDi))
        (pin (num C3) (name IO_DDR_MEM_DATA[27]) (type BiDi))
        (pin (num C4) (name IO_DDR_MEM_DATA[24]) (type BiDi))
        (pin (num C5) (name IO_DDR_MEM_DATA[21]) (type BiDi))
        (pin (num C6) (name IO_DDR_MEM_DM[2]) (type BiDi))
        (pin (num C7) (name IO_DDR_MEM_DATA[31]) (type BiDi))
        (pin (num C8) (name IO_GEMGXL_0_TX_CLK) (type input))
        (pin (num C9) (name IO_GEMGXL_0_RXD_6) (type input))
        (pin (num C10) (name IO_GEMGXL_0_TXD_4) (type output))
        (pin (num C11) (name IO_GEMGXL_0_TXD_1) (type output))
        (pin (num C12) (name IO_GEMGXL_0_MDIO) (type BiDi))
        (pin (num C13) (name IO_GEMGXL_0_CRS) (type input))
        (pin (num C14) (name IO_PRCI_RSVD15) (type passive))
        (pin (num C15) (name IO_PRCI_HFXSEL) (type input))
        (pin (num C16) (name IO_PRCI_RSVD4) (type passive))
        (pin (num C17) (name IO_PRCI_ERESET_N) (type input))
        (pin (num C18) (name IO_MSEL_MSEL_1) (type input))
        (pin (num C19) (name IO_JTAG_TDI) (type input))
        (pin (num C20) (name IO_GPIO_0_PINS_7) (type BiDi))
        (pin (num C21) (name IO_GPIO_0_PINS_2) (type BiDi))
        (pin (num C22) (name IO_GPIO_0_PINS_1) (type BiDi))
        (pin (num D1) (name VSS) (type power_in))
        (pin (num D2) (name IO_DDR_MEM_DATA[0]) (type BiDi))
        (pin (num D3) (name IO_DDR_MEM_DATA[30]) (type BiDi))
        (pin (num D4) (name IO_DDR_MEM_DATA[25]) (type BiDi))
        (pin (num D5) (name IO_DDR_MEM_DM[3]) (type BiDi))
        (pin (num D6) (name IO_DDR_MEM_DATA[26]) (type BiDi))
        (pin (num D7) (name IO_DDR_MEM_DQS_M[3]) (type BiDi))
        (pin (num D8) (name IO_DDR_RSVD1) (type passive))
        (pin (num D9) (name IO_GEMGXL_0_TXD_7) (type output))
        (pin (num D10) (name IO_GEMGXL_0_TXD_5) (type output))
        (pin (num D11) (name IO_GEMGXL_0_TXD_2) (type output))
        (pin (num D12) (name VSS) (type power_in))
        (pin (num D13) (name IO_PRCI_RSVD1) (type passive))
        (pin (num D14) (name IO_PRCI_RSVD11) (type passive))
        (pin (num D15) (name IO_PRCI_RTCXSEL) (type input))
        (pin (num D16) (name IO_PRCI_RSVD3) (type passive))
        (pin (num D17) (name IO_PRCI_RSVD10) (type passive))
        (pin (num D18) (name IO_JTAG_TCK) (type input))
        (pin (num D19) (name IO_GPIO_0_PINS_8) (type BiDi))
        (pin (num D20) (name IO_GPIO_0_PINS_5) (type BiDi))
        (pin (num D21) (name IO_GPIO_0_PINS_3) (type BiDi))
        (pin (num D22) (name IO_PWM_1_PWM_0) (type BiDi))
        (pin (num E1) (name IO_DDR_MEM_DATA[6]) (type BiDi))
        (pin (num E2) (name IO_DDR_MEM_DATA[3]) (type BiDi))
        (pin (num E3) (name VDD) (type power_in))
        (pin (num E4) (name VSS) (type power_in))
        (pin (num E5) (name IO_DDR_MEM_DM[0]) (type BiDi))
        (pin (num E6) (name IO_DDR_MEM_DATA[28]) (type BiDi))
        (pin (num E7) (name IO_DDR_MEM_DQS_P[3]) (type BiDi))
        (pin (num E8) (name IO_DDR_RSVD0) (type passive))
        (pin (num E9) (name IO_GEMGXL_0_RXD_7) (type input))
        (pin (num E10) (name IO_GEMGXL_0_RXD_4) (type input))
        (pin (num E11) (name IO_GEMGXL_0_RXD_3) (type input))
        (pin (num E12) (name IO_GEMGXL_0_GTX_CLK) (type input))
        (pin (num E13) (name IO_PRCI_RSVD2) (type passive))
        (pin (num E14) (name IO_PRCI_RSVD12) (type passive))
        (pin (num E15) (name IO_PRCI_RSVD5) (type passive))
        (pin (num E16) (name IO_PRCI_RSVD9) (type passive))
        (pin (num E17) (name IO_JTAG_TDO) (type output))
        (pin (num E18) (name IO_GPIO_0_PINS_4) (type BiDi))
        (pin (num E19) (name IO_GPIO_0_PINS_13) (type BiDi))
        (pin (num E20) (name IO_GPIO_0_PINS_6) (type BiDi))
        (pin (num E21) (name VDD) (type power_in))
        (pin (num E22) (name VSS) (type power_in))
        (pin (num F1) (name IO_DDR_MEM_DATA[9]) (type BiDi))
        (pin (num F2) (name IO_DDR_MEM_DQS_P[0]) (type BiDi))
        (pin (num F3) (name IO_DDR_MEM_DQS_M[0]) (type BiDi))
        (pin (num F4) (name IO_DDR_MEM_DATA[2]) (type BiDi))
        (pin (num F5) (name IO_DDR_MEM_DATA[10]) (type BiDi))
        (pin (num F6) (name IO_DDR_CAL_0) (type passive))
        (pin (num F7) (name VSS) (type power_in))
        (pin (num F8) (name IO_DDR_RSVD2) (type passive))
        (pin (num F9) (name IO_DDR_RSVD3) (type passive))
        (pin (num F10) (name IO_GEMGXL_0_TX_ER) (type output))
        (pin (num F11) (name IO_GEMGXL_0_TXD_3) (type output))
        (pin (num F12) (name IO_GEMGXL_0_RX_CLK) (type input))
        (pin (num F13) (name IO_PRCI_RSVD14) (type passive))
        (pin (num F14) (name IO_PRCI_RSVD13) (type passive))
        (pin (num F15) (name IO_PRCI_HFXCLKIN) (type input))
        (pin (num F16) (name IO_JTAG_TMS) (type input))
        (pin (num F17) (name IO_GPIO_0_PINS_0) (type BiDi))
        (pin (num F18) (name IO_GPIO_0_PINS_10) (type BiDi))
        (pin (num F19) (name IO_PWM_1_PWM_3) (type BiDi))
        (pin (num F20) (name IO_PWM_0_PWM_2) (type BiDi))
        (pin (num F21) (name IO_PWM_0_PWM_1) (type BiDi))
        (pin (num F22) (name IO_QSPI_1_DQ_2) (type BiDi))
        (pin (num G1) (name IO_DDR_MEM_DATA[11]) (type BiDi))
        (pin (num G2) (name VSS) (type power_in))
        (pin (num G3) (name IO_DDR_MEM_DATA[7]) (type BiDi))
        (pin (num G4) (name IO_DDR_MEM_DATA[5]) (type BiDi))
        (pin (num G5) (name IO_DDR_MEM_DM[1]) (type BiDi))
        (pin (num G6) (name VSS) (type power_in))
        (pin (num G7) (name DDR_VDDQ) (type power_in))
        (pin (num G8) (name VSS) (type power_in))
        (pin (num G9) (name VDD) (type power_in))
        (pin (num G10) (name VSS) (type power_in))
        (pin (num G11) (name VDD) (type power_in))
        (pin (num G12) (name VSS) (type power_in))
        (pin (num G13) (name IO_PRCI_RSVD7) (type passive))
        (pin (num G14) (name OTP_VDD) (type input))
        (pin (num G15) (name VDD) (type power_in))
        (pin (num G16) (name VSS) (type power_in))
        (pin (num G17) (name IO_GPIO_0_PINS_15) (type BiDi))
        (pin (num G18) (name IO_PWM_1_PWM_2) (type BiDi))
        (pin (num G19) (name IO_PWM_0_PWM_0) (type BiDi))
        (pin (num G20) (name IO_PWM_0_PWM_3) (type BiDi))
        (pin (num G21) (name IO_QSPI_1_CS_1) (type output))
        (pin (num G22) (name IO_QSPI_1_DQ_0) (type BiDi))
        (pin (num H1) (name IO_DDR_MEM_DATA[12]) (type BiDi))
        (pin (num H2) (name IO_DDR_MEM_DQS_P[1]) (type BiDi))
        (pin (num H3) (name IO_DDR_MEM_DQS_M[1]) (type BiDi))
        (pin (num H4) (name IO_DDR_MEM_DATA[8]) (type BiDi))
        (pin (num H5) (name IO_DDR_MEM_ECC_DATA[0]) (type BiDi))
        (pin (num H6) (name DDR_VDDQ) (type power_in))
        (pin (num H7) (name VSS) (type power_in))
        (pin (num H8) (name VDD) (type power_in))
        (pin (num H9) (name VSS) (type power_in))
        (pin (num H10) (name VDD) (type power_in))
        (pin (num H11) (name GIVSS) (type passive))
        (pin (num H12) (name VDD) (type power_in))
        (pin (num H13) (name IO_PRCI_RSVD8) (type passive))
        (pin (num H14) (name VDD) (type power_in))
        (pin (num H15) (name VSS) (type power_in))
        (pin (num H16) (name VDD) (type power_in))
        (pin (num H17) (name IO_PWM_1_PWM_1) (type BiDi))
        (pin (num H18) (name IO_QSPI_1_SCK) (type output))
        (pin (num H19) (name IO_QSPI_1_CS_2) (type output))
        (pin (num H20) (name IO_QSPI_0_DQ_3) (type BiDi))
        (pin (num H21) (name IO_QSPI_0_DQ_0) (type BiDi))
        (pin (num H22) (name IO_QSPI_0_DQ_1) (type BiDi))
        (pin (num J1) (name VSS) (type power_in))
        (pin (num J2) (name IO_DDR_MEM_DATA[14]) (type BiDi))
        (pin (num J3) (name IO_DDR_MEM_DATA[13]) (type BiDi))
        (pin (num J4) (name IO_DDR_MEM_DATA[15]) (type BiDi))
        (pin (num J5) (name IO_DDR_MEM_ECC_DM) (type BiDi))
        (pin (num J6) (name VSS) (type power_in))
        (pin (num J7) (name DDR_VDDQ) (type power_in))
        (pin (num J8) (name VSS) (type power_in))
        (pin (num J9) (name VDD) (type power_in))
        (pin (num J10) (name VSS) (type power_in))
        (pin (num J11) (name GIVDD) (type power_in))
        (pin (num J12) (name GEMGXLPLL_AVSS) (type power_in))
        (pin (num J13) (name DDRPLL_AVSS) (type passive))
        (pin (num J14) (name COREPLL_AVSS) (type input))
        (pin (num J15) (name VDD) (type power_in))
        (pin (num J16) (name VSS) (type power_in))
        (pin (num J17) (name IO_QSPI_1_DQ_3) (type BiDi))
        (pin (num J18) (name IO_QSPI_1_DQ_1) (type BiDi))
        (pin (num J19) (name IO_QSPI_0_CS_0) (type output))
        (pin (num J20) (name IO_QSPI_1_CS_3) (type output))
        (pin (num J21) (name IO_QSPI_0_DQ_2) (type BiDi))
        (pin (num J22) (name VSS) (type power_in))
        (pin (num K1) (name IO_DDR_MEM_ECC_DATA[1]) (type BiDi))
        (pin (num K2) (name IO_DDR_MEM_ECC_DQS_P) (type BiDi))
        (pin (num K3) (name IO_DDR_MEM_ECC_DQS_M) (type BiDi))
        (pin (num K4) (name IO_DDR_MEM_ECC_DATA[2]) (type BiDi))
        (pin (num K5) (name IO_DDR_MEM_CLK) (type output))
        (pin (num K6) (name DDR_VDDQ) (type power_in))
        (pin (num K7) (name VSS) (type power_in))
        (pin (num K8) (name VDD) (type power_in))
        (pin (num K9) (name VSS) (type power_in))
        (pin (num K10) (name VDD) (type power_in))
        (pin (num K11) (name VSS) (type power_in))
        (pin (num K12) (name GEMGXLPLL_AVDD) (type power_in))
        (pin (num K13) (name DDRPLL_AVDD) (type power_in))
        (pin (num K14) (name COREPLL_AVDD) (type input))
        (pin (num K15) (name IVSS) (type passive))
        (pin (num K16) (name IVDD) (type power_in))
        (pin (num K17) (name IO_QSPI_1_CS_0) (type output))
        (pin (num K18) (name IO_QSPI_0_SCK) (type output))
        (pin (num K19) (name IO_CHIPLINK_0_C2B_DATA_28) (type output))
        (pin (num K20) (name IO_CHIPLINK_0_C2B_DATA_24) (type output))
        (pin (num K21) (name VDD) (type power_in))
        (pin (num K22) (name IO_CHIPLINK_0_C2B_DATA_26) (type output))
        (pin (num L1) (name IO_DDR_MEM_ECC_DATA[4]) (type BiDi))
        (pin (num L2) (name IO_DDR_MEM_ECC_DATA[3]) (type BiDi))
        (pin (num L3) (name IO_DDR_MEM_ECC_DATA[7]) (type BiDi))
        (pin (num L4) (name IO_DDR_MEM_ECC_DATA[5]) (type BiDi))
        (pin (num L5) (name IO_DDR_MEM_CLK_N) (type output))
        (pin (num L6) (name VSS) (type power_in))
        (pin (num L7) (name DDR_VDDQ) (type power_in))
        (pin (num L8) (name VSS) (type power_in))
        (pin (num L9) (name DDR_VDDPLL) (type power_in))
        (pin (num L10) (name VSS) (type power_in))
        (pin (num L11) (name VDD) (type power_in))
        (pin (num L12) (name VSS) (type power_in))
        (pin (num L13) (name VDD) (type power_in))
        (pin (num L14) (name VSS) (type power_in))
        (pin (num L15) (name IVSS) (type passive))
        (pin (num L16) (name IVDD) (type power_in))
        (pin (num L17) (name IO_CHIPLINK_0_C2B_DATA_31) (type output))
        (pin (num L18) (name IO_CHIPLINK_0_C2B_DATA_30) (type output))
        (pin (num L19) (name IO_CHIPLINK_0_C2B_DATA_27) (type output))
        (pin (num L20) (name IO_CHIPLINK_0_C2B_DATA_20) (type output))
        (pin (num L21) (name IO_CHIPLINK_0_C2B_DATA_18) (type output))
        (pin (num L22) (name IO_CHIPLINK_0_C2B_DATA_29) (type output))
        (pin (num M1) (name IO_DDR_MEM_ECC_DATA[6]) (type BiDi))
        (pin (num M2) (name IO_DDR_MEM_RAS_N) (type output))
        (pin (num M3) (name IO_DDR_MEM_CAS_N) (type output))
        (pin (num M4) (name IO_DDR_MEM_BANK[0]) (type output))
        (pin (num M5) (name IO_DDR_MEM_BANK[2]) (type output))
        (pin (num M6) (name DDR_VDDQ) (type power_in))
        (pin (num M7) (name VSS) (type power_in))
        (pin (num M8) (name VDD) (type power_in))
        (pin (num M9) (name DDR_VDDPLL) (type power_in))
        (pin (num M10) (name VDD) (type power_in))
        (pin (num M11) (name VSS) (type power_in))
        (pin (num M12) (name VDD) (type power_in))
        (pin (num M13) (name VSS) (type power_in))
        (pin (num M14) (name VDD) (type power_in))
        (pin (num M15) (name IVSS) (type passive))
        (pin (num M16) (name IVDD) (type power_in))
        (pin (num M17) (name IO_CHIPLINK_0_C2B_DATA_15) (type output))
        (pin (num M18) (name IO_CHIPLINK_0_C2B_DATA_19) (type output))
        (pin (num M19) (name IO_CHIPLINK_0_C2B_DATA_23) (type output))
        (pin (num M20) (name IO_CHIPLINK_0_C2B_DATA_12) (type output))
        (pin (num M21) (name IO_CHIPLINK_0_C2B_DATA_25) (type output))
        (pin (num M22) (name IO_CHIPLINK_0_C2B_DATA_22) (type output))
        (pin (num N1) (name IO_DDR_MEM_WE_N) (type output))
        (pin (num N2) (name IO_DDR_MEM_BANK[1]) (type output))
        (pin (num N3) (name IO_DDR_MEM_ADDRESS[0]) (type output))
        (pin (num N4) (name IO_DDR_MEM_ADDRESS[2]) (type output))
        (pin (num N5) (name IO_DDR_MEM_ADDRESS[5]) (type output))
        (pin (num N6) (name VSS) (type power_in))
        (pin (num N7) (name DDR_VDDQ) (type power_in))
        (pin (num N8) (name VSS) (type power_in))
        (pin (num N9) (name VDD) (type power_in))
        (pin (num N10) (name VSS) (type power_in))
        (pin (num N11) (name VDD) (type power_in))
        (pin (num N12) (name VSS) (type power_in))
        (pin (num N13) (name VDD) (type power_in))
        (pin (num N14) (name VSS) (type power_in))
        (pin (num N15) (name IVSS) (type passive))
        (pin (num N16) (name IVDD) (type power_in))
        (pin (num N17) (name IO_CHIPLINK_0_C2B_SEND) (type output))
        (pin (num N18) (name IO_CHIPLINK_0_C2B_DATA_2) (type output))
        (pin (num N19) (name IO_CHIPLINK_0_C2B_DATA_6) (type output))
        (pin (num N20) (name IO_CHIPLINK_0_C2B_DATA_21) (type output))
        (pin (num N21) (name IO_CHIPLINK_0_C2B_DATA_16) (type output))
        (pin (num N22) (name IO_CHIPLINK_0_C2B_DATA_14) (type output))
        (pin (num P1) (name VSS) (type power_in))
        (pin (num P2) (name VDD) (type power_in))
        (pin (num P3) (name IO_DDR_MEM_ADDRESS[3]) (type output))
        (pin (num P4) (name IO_DDR_MEM_ADDRESS[6]) (type output))
        (pin (num P5) (name IO_DDR_MEM_ADDRESS[12]) (type output))
        (pin (num P6) (name DDR_VDDQ) (type power_in))
        (pin (num P7) (name VSS) (type power_in))
        (pin (num P8) (name VDD) (type power_in))
        (pin (num P9) (name VSS) (type power_in))
        (pin (num P10) (name VDD) (type power_in))
        (pin (num P11) (name VSS) (type power_in))
        (pin (num P12) (name VDD) (type power_in))
        (pin (num P13) (name VSS) (type power_in))
        (pin (num P14) (name VDD) (type power_in))
        (pin (num P15) (name VSS) (type power_in))
        (pin (num P16) (name VDD) (type power_in))
        (pin (num P17) (name IO_CHIPLINK_0_B2C_RST) (type input))
        (pin (num P18) (name IO_CHIPLINK_0_B2C_DATA_21) (type input))
        (pin (num P19) (name IO_CHIPLINK_0_C2B_CLK) (type output))
        (pin (num P20) (name IO_CHIPLINK_0_C2B_DATA_4) (type output))
        (pin (num P21) (name VDD) (type power_in))
        (pin (num P22) (name VSS) (type power_in))
        (pin (num R1) (name IO_DDR_MEM_ADDRESS[1]) (type output))
        (pin (num R2) (name IO_DDR_MEM_ADDRESS[7]) (type output))
        (pin (num R3) (name IO_DDR_MEM_ADDRESS[8]) (type output))
        (pin (num R4) (name IO_DDR_MEM_ADDRESS[11]) (type output))
        (pin (num R5) (name IO_DDR_MEM_DATA[32]) (type BiDi))
        (pin (num R6) (name VSS) (type power_in))
        (pin (num R7) (name DDR_VDDQ) (type power_in))
        (pin (num R8) (name VSS) (type power_in))
        (pin (num R9) (name VDD) (type power_in))
        (pin (num R10) (name VSS) (type power_in))
        (pin (num R11) (name VDD) (type power_in))
        (pin (num R12) (name VSS) (type power_in))
        (pin (num R13) (name VDD) (type power_in))
        (pin (num R14) (name VSS) (type power_in))
        (pin (num R15) (name VDD) (type power_in))
        (pin (num R16) (name VSS) (type power_in))
        (pin (num R17) (name IO_CHIPLINK_0_B2C_DATA_24) (type input))
        (pin (num R18) (name IO_CHIPLINK_0_B2C_DATA_17) (type input))
        (pin (num R19) (name IO_CHIPLINK_0_C2B_DATA_1) (type output))
        (pin (num R20) (name IO_CHIPLINK_0_C2B_DATA_3) (type output))
        (pin (num R21) (name IO_CHIPLINK_0_C2B_DATA_8) (type output))
        (pin (num R22) (name IO_CHIPLINK_0_C2B_DATA_17) (type output))
        (pin (num T1) (name IO_DDR_MEM_ADDRESS[4]) (type output))
        (pin (num T2) (name IO_DDR_MEM_ADDRESS[13]) (type output))
        (pin (num T3) (name IO_DDR_MEM_ADDRESS[9]) (type output))
        (pin (num T4) (name IO_DDR_MEM_DATA[34]) (type BiDi))
        (pin (num T5) (name IO_DDR_MEM_DM[4]) (type BiDi))
        (pin (num T6) (name DDR_VDDQ) (type power_in))
        (pin (num T7) (name VSS) (type power_in))
        (pin (num T8) (name VDD) (type power_in))
        (pin (num T9) (name VSS) (type power_in))
        (pin (num T10) (name VDD) (type power_in))
        (pin (num T11) (name VSS) (type power_in))
        (pin (num T12) (name VDD) (type power_in))
        (pin (num T13) (name VSS) (type power_in))
        (pin (num T14) (name VDD) (type power_in))
        (pin (num T15) (name VSS) (type power_in))
        (pin (num T16) (name VDD) (type power_in))
        (pin (num T17) (name VSS) (type power_in))
        (pin (num T18) (name IO_CHIPLINK_0_B2C_DATA_19) (type input))
        (pin (num T19) (name IO_CHIPLINK_0_C2B_DATA_0) (type output))
        (pin (num T20) (name IO_CHIPLINK_0_C2B_RST) (type output))
        (pin (num T21) (name IO_CHIPLINK_0_C2B_DATA_13) (type output))
        (pin (num T22) (name IO_CHIPLINK_0_C2B_DATA_10) (type output))
        (pin (num U1) (name IO_DDR_MEM_ADDRESS[10]) (type output))
        (pin (num U2) (name IO_DDR_MEM_PARITY_IN) (type output))
        (pin (num U3) (name IO_DDR_MEM_ADDRESS[14]) (type output))
        (pin (num U4) (name IO_DDR_MEM_DQS_M[4]) (type BiDi))
        (pin (num U5) (name IO_DDR_MEM_DATA[39]) (type BiDi))
        (pin (num U6) (name VSS) (type power_in))
        (pin (num U7) (name DDR_VDDQCK) (type power_in))
        (pin (num U8) (name VSS) (type power_in))
        (pin (num U9) (name VDD) (type power_in))
        (pin (num U10) (name VSS) (type power_in))
        (pin (num U11) (name VDD) (type power_in))
        (pin (num U12) (name VSS) (type power_in))
        (pin (num U13) (name VDD) (type power_in))
        (pin (num U14) (name VSS) (type power_in))
        (pin (num U15) (name VDD) (type power_in))
        (pin (num U16) (name VSS) (type power_in))
        (pin (num U17) (name IO_CHIPLINK_0_B2C_DATA_20) (type input))
        (pin (num U18) (name IO_CHIPLINK_0_B2C_DATA_14) (type input))
        (pin (num U19) (name IO_CHIPLINK_0_B2C_DATA_18) (type input))
        (pin (num U20) (name IO_CHIPLINK_0_C2B_DATA_5) (type output))
        (pin (num U21) (name IO_CHIPLINK_0_C2B_DATA_11) (type output))
        (pin (num U22) (name IO_CHIPLINK_0_C2B_DATA_7) (type output))
        (pin (num V1) (name VSS) (type power_in))
        (pin (num V2) (name IO_DDR_MEM_DATA[35]) (type BiDi))
        (pin (num V3) (name IO_DDR_MEM_ADDRESS[15]) (type output))
        (pin (num V4) (name IO_DDR_MEM_DQS_P[4]) (type BiDi))
        (pin (num V5) (name IO_DDR_MEM_DATA[40]) (type BiDi))
        (pin (num V6) (name VDD) (type power_in))
        (pin (num V7) (name VSS) (type power_in))
        (pin (num V8) (name VDD) (type power_in))
        (pin (num V9) (name VSS) (type power_in))
        (pin (num V10) (name VDD) (type power_in))
        (pin (num V11) (name VSS) (type power_in))
        (pin (num V12) (name VDD) (type power_in))
        (pin (num V13) (name VSS) (type power_in))
        (pin (num V14) (name VDD) (type power_in))
        (pin (num V15) (name VSS) (type power_in))
        (pin (num V16) (name IO_CHIPLINK_0_B2C_DATA_12) (type input))
        (pin (num V17) (name IO_CHIPLINK_0_B2C_DATA_16) (type input))
        (pin (num V18) (name IO_CHIPLINK_0_B2C_DATA_9) (type input))
        (pin (num V19) (name IO_CHIPLINK_0_B2C_DATA_15) (type input))
        (pin (num V20) (name IO_CHIPLINK_0_B2C_DATA_25) (type input))
        (pin (num V21) (name VDD) (type power_in))
        (pin (num V22) (name VSS) (type power_in))
        (pin (num W1) (name IO_DDR_MEM_DATA[33]) (type BiDi))
        (pin (num W2) (name IO_DDR_MEM_DATA[38]) (type BiDi))
        (pin (num W3) (name IO_DDR_MEM_DATA[37]) (type BiDi))
        (pin (num W4) (name IO_DDR_MEM_DQS_M[5]) (type BiDi))
        (pin (num W5) (name IO_DDR_MEM_DM[5]) (type BiDi))
        (pin (num W6) (name IO_DDR_MEM_ERROR_N) (type input))
        (pin (num W7) (name IO_DDR_MEM_CS_N[1]) (type output))
        (pin (num W8) (name IO_DDR_MEM_DATA[51]) (type BiDi))
        (pin (num W9) (name IO_DDR_MEM_DATA[55]) (type BiDi))
        (pin (num W10) (name IO_DDR_MEM_DM[6]) (type BiDi))
        (pin (num W11) (name IO_DDR_MEM_DATA[49]) (type BiDi))
        (pin (num W12) (name IO_DDR_MEM_DATA[54]) (type BiDi))
        (pin (num W13) (name IO_I2C_0_SDA) (type BiDi))
        (pin (num W14) (name IO_UART_0_RXD) (type input))
        (pin (num W15) (name IO_QSPI_2_SCK) (type output))
        (pin (num W16) (name IO_CHIPLINK_0_B2C_DATA_4) (type input))
        (pin (num W17) (name IO_CHIPLINK_0_B2C_DATA_3) (type input))
        (pin (num W18) (name IO_CHIPLINK_0_B2C_DATA_5) (type input))
        (pin (num W19) (name IO_CHIPLINK_0_B2C_DATA_11) (type input))
        (pin (num W20) (name IO_CHIPLINK_0_B2C_DATA_28) (type input))
        (pin (num W21) (name IO_CHIPLINK_0_B2C_SEND) (type input))
        (pin (num W22) (name IO_CHIPLINK_0_C2B_DATA_9) (type output))
        (pin (num Y1) (name IO_DDR_MEM_DATA[36]) (type BiDi))
        (pin (num Y2) (name IO_DDR_MEM_DATA[43]) (type BiDi))
        (pin (num Y3) (name IO_DDR_MEM_DATA[42]) (type BiDi))
        (pin (num Y4) (name IO_DDR_MEM_DQS_P[5]) (type BiDi))
        (pin (num Y5) (name IO_DDR_MEM_RESET_N) (type output))
        (pin (num Y6) (name IO_DDR_MEM_CS_N[0]) (type output))
        (pin (num Y7) (name IO_DDR_MEM_DQS_P[6]) (type BiDi))
        (pin (num Y8) (name IO_DDR_MEM_DQS_M[7]) (type BiDi))
        (pin (num Y9) (name IO_DDR_MEM_DATA[53]) (type BiDi))
        (pin (num Y10) (name IO_DDR_MEM_DATA[52]) (type BiDi))
        (pin (num Y11) (name IO_DDR_MEM_DATA[50]) (type BiDi))
        (pin (num Y12) (name IO_DDR_MEM_DATA[48]) (type BiDi))
        (pin (num Y13) (name IO_UART_0_TXD) (type output))
        (pin (num Y14) (name IO_I2C_0_SCL) (type BiDi))
        (pin (num Y15) (name IO_QSPI_2_DQ_3) (type BiDi))
        (pin (num Y16) (name IO_CHIPLINK_0_B2C_DATA_0) (type input))
        (pin (num Y17) (name IO_CHIPLINK_0_B2C_DATA_7) (type input))
        (pin (num Y18) (name IO_CHIPLINK_0_B2C_DATA_6) (type input))
        (pin (num Y19) (name IO_CHIPLINK_0_B2C_DATA_10) (type input))
        (pin (num Y20) (name IO_CHIPLINK_0_B2C_DATA_27) (type input))
        (pin (num Y21) (name IO_CHIPLINK_0_B2C_DATA_31) (type input))
        (pin (num Y22) (name IO_CHIPLINK_0_B2C_DATA_30) (type input))))
    (libpart (lib Mechanical) (part MountingHole_Pad)
      (description "Mounting Hole with connection")
      (docs ~)
      (footprints
        (fp MountingHole*Pad*))
      (fields
        (field (name Reference) MH)
        (field (name Value) MountingHole_Pad))
      (pins
        (pin (num 1) (name 1) (type input))))
    (libpart (lib Memory_EEPROM) (part M24C02-WDW)
      (aliases
        (alias M24C02-WMN))
      (description "2 Kb serial I2c bus EEPROM, TSSOP-8")
      (docs http://www.st.com/content/ccc/resource/technical/document/datasheet/b0/d8/50/40/5a/85/49/6f/DM00071904.pdf/files/DM00071904.pdf/jcr:content/translations/en.DM00071904.pdf)
      (footprints
        (fp *TSSOP-8*4.4x3mm*P0.65mm*)
        (fp *SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) M24C02-WDW))
      (pins
        (pin (num 1) (name E0) (type input))
        (pin (num 2) (name E1) (type input))
        (pin (num 3) (name E2) (type input))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name SDA) (type BiDi))
        (pin (num 6) (name SCL) (type input))
        (pin (num 7) (name ~WC) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Memory_Flash) (part IS25WP256D)
      (description "SERIAL FLASH MEMORY WITH 166/133MHZ MULTI I/O SPI&QUAD I/O QPI DTR INTERFACE")
      (docs "http://www.issi.com/WW/pdf/IS25LP(WP)256D.pdf")
      (footprints
        (fp SOIC?16W*7.5x10.3mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) IS25WP256D))
      (pins
        (pin (num 1) (name HOLD#/IO3) (type BiDi))
        (pin (num 2) (name VCC) (type power_in))
        (pin (num 3) (name RST#/NC) (type passive))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name NC) (type NotConnected))
        (pin (num 7) (name CS#) (type input))
        (pin (num 8) (name MISO/IO1) (type BiDi))
        (pin (num 9) (name WP#/IO2) (type BiDi))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name NC) (type NotConnected))
        (pin (num 13) (name NC) (type NotConnected))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name MOSI/IO0) (type BiDi))
        (pin (num 16) (name SCK) (type input))))
    (libpart (lib Memory_RAM) (part H5AN8G8NAFR-UHC)
      (description "8Gb CMOS Double Data Rate IV Synchronous RAM")
      (docs https://www.skhynix.com/product/filedata/fileDownload.do?seq=7687)
      (footprints
        (fp FBGA*7.5x11mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) H5AN8G8NAFR-UHC)
        (field (name Footprint) Package_BGA:FBGA-78_7.5x11mm_Layout2x3x13_P0.8mm))
      (pins
        (pin (num A1) (name VDD) (type power_in))
        (pin (num A2) (name VSSQ) (type power_in))
        (pin (num A3) (name NC) (type NotConnected))
        (pin (num A7) (name ~DM/DBI) (type BiDi))
        (pin (num A8) (name VSSQ) (type passive))
        (pin (num A9) (name VSS) (type power_in))
        (pin (num B1) (name VPP) (type power_in))
        (pin (num B2) (name VDDQ) (type power_in))
        (pin (num B3) (name DQS_c) (type BiDi))
        (pin (num B7) (name DQ1) (type BiDi))
        (pin (num B8) (name VDDQ) (type passive))
        (pin (num B9) (name ZQ) (type passive))
        (pin (num C1) (name VDDQ) (type passive))
        (pin (num C2) (name DQ0) (type BiDi))
        (pin (num C3) (name DQS_t) (type BiDi))
        (pin (num C7) (name VDD) (type passive))
        (pin (num C8) (name VSS) (type passive))
        (pin (num C9) (name VDDQ) (type passive))
        (pin (num D1) (name VSSQ) (type passive))
        (pin (num D2) (name DQ4) (type BiDi))
        (pin (num D3) (name DQ2) (type BiDi))
        (pin (num D7) (name DQ3) (type BiDi))
        (pin (num D8) (name DQ5) (type BiDi))
        (pin (num D9) (name VSSQ) (type passive))
        (pin (num E1) (name VSS) (type passive))
        (pin (num E2) (name VDDQ) (type passive))
        (pin (num E3) (name DQ6) (type BiDi))
        (pin (num E7) (name DQ7) (type BiDi))
        (pin (num E8) (name VDDQ) (type passive))
        (pin (num E9) (name VSS) (type passive))
        (pin (num F1) (name VDD) (type passive))
        (pin (num F2) (name NC/C2/ODT1) (type passive))
        (pin (num F3) (name ODT) (type input))
        (pin (num F7) (name CK_t) (type input))
        (pin (num F8) (name CK_c) (type input))
        (pin (num F9) (name VDD) (type passive))
        (pin (num G1) (name VSS) (type passive))
        (pin (num G2) (name NC/C0/CKE1) (type passive))
        (pin (num G3) (name CKE) (type input))
        (pin (num G7) (name ~CS) (type input))
        (pin (num G8) (name NC/~CS1) (type passive))
        (pin (num G9) (name TEN) (type input))
        (pin (num H1) (name VDD) (type passive))
        (pin (num H2) (name A14/~WE) (type input))
        (pin (num H3) (name ~ACT) (type input))
        (pin (num H7) (name A15/~CAS) (type input))
        (pin (num H8) (name A16/~RAS) (type input))
        (pin (num H9) (name VSS) (type passive))
        (pin (num J1) (name VREFCA) (type passive))
        (pin (num J2) (name BG0) (type input))
        (pin (num J3) (name A10/AP) (type input))
        (pin (num J7) (name A12/~BC) (type input))
        (pin (num J8) (name BG1) (type input))
        (pin (num J9) (name VDD) (type passive))
        (pin (num K1) (name VSS) (type passive))
        (pin (num K2) (name BA0) (type input))
        (pin (num K3) (name A4) (type input))
        (pin (num K7) (name A3) (type input))
        (pin (num K8) (name BA1) (type input))
        (pin (num K9) (name VSS) (type passive))
        (pin (num L1) (name ~RESET) (type input))
        (pin (num L2) (name A6) (type input))
        (pin (num L3) (name A0) (type input))
        (pin (num L7) (name A1) (type input))
        (pin (num L8) (name A5) (type input))
        (pin (num L9) (name ~ALERT) (type openCol))
        (pin (num M1) (name VDD) (type passive))
        (pin (num M2) (name A8) (type input))
        (pin (num M3) (name A2) (type input))
        (pin (num M7) (name A9) (type input))
        (pin (num M8) (name A7) (type input))
        (pin (num M9) (name VPP) (type passive))
        (pin (num N1) (name VSS) (type passive))
        (pin (num N2) (name A11) (type input))
        (pin (num N3) (name PAR) (type input))
        (pin (num N7) (name A17/NC) (type passive))
        (pin (num N8) (name A13) (type input))
        (pin (num N9) (name VDD) (type passive))))
    (libpart (lib Motor) (part Fan_Tacho)
      (aliases
        (alias Fan_3pin)
        (alias Fan_PC_Chassis))
      (description "Fan, tacho output, 3-pin connector")
      (docs http://www.hardwarecanucks.com/forum/attachments/new-builds/16287d1330775095-help-chassis-power-fan-connectors-motherboard-asus_p8z68.jpg)
      (footprints
        (fp FanPinHeader*P2.54mm*Vertical*)
        (fp PinHeader*P2.54mm*Vertical*)
        (fp TerminalBlock*))
      (fields
        (field (name Reference) M)
        (field (name Value) Fan_Tacho))
      (pins
        (pin (num 1) (name Tacho) (type passive))
        (pin (num 2) (name +) (type passive))
        (pin (num 3) (name -) (type passive))))
    (libpart (lib Oscillator) (part XO32)
      (description "HCMOS Clock Oscillator")
      (docs http://cdn-reichelt.de/documents/datenblatt/B400/XO32.pdf)
      (footprints
        (fp Oscillator*SMD*EuroQuartz*XO32*3.2x2.5mm*))
      (fields
        (field (name Reference) X)
        (field (name Value) XO32)
        (field (name Footprint) Oscillator:Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name V+) (type power_in))))
    (libpart (lib Power_Protection) (part TPD6F003)
      (description "6 channel EMI filters with integrated ESD protection")
      (docs http://www.ti.com/lit/ds/symlink/tpd6f003.pdf)
      (footprints
        (fp *WSON*EP0.4x2mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPD6F003)
        (field (name Footprint) Package_SON:Texas_R-PWSON-N12_EP0.4x2mm))
      (pins
        (pin (num 1) (name Ch1_In) (type passive))
        (pin (num 2) (name Ch2_In) (type passive))
        (pin (num 3) (name Ch3_In) (type passive))
        (pin (num 4) (name Ch4_In) (type passive))
        (pin (num 5) (name Ch5_In) (type passive))
        (pin (num 6) (name Ch6_In) (type passive))
        (pin (num 7) (name Ch6_Out) (type passive))
        (pin (num 8) (name Ch5_Out) (type passive))
        (pin (num 9) (name Ch4_Out) (type passive))
        (pin (num 10) (name Ch3_Out) (type passive))
        (pin (num 11) (name Ch2_Out) (type passive))
        (pin (num 12) (name Ch1_Out) (type passive))
        (pin (num 13) (name GND) (type power_in))))
    (libpart (lib Power_Supervisor) (part LM3880)
      (description "Simple Power Sequencer, SOT-23-6")
      (docs http://www.ti.com/lit/ds/symlink/lm3880.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM3880)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name FLAG3) (type openCol))
        (pin (num 5) (name FLAG2) (type openCol))
        (pin (num 6) (name FLAG1) (type openCol))))
    (libpart (lib Regulator_Linear) (part LP5907MFX-1.8)
      (description "250-mA Ultra-Low-Noise Low-IQ LDO")
      (docs http://www.ti.com/lit/ds/symlink/lp5907.pdf)
      (footprints
        (fp *SOT?23?5*))
      (fields
        (field (name Reference) U)
        (field (name Value) LP5907MFX-1.8)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name OUT) (type power_out))))
    (libpart (lib Regulator_Linear) (part MIC5353-2.5YMT)
      (aliases
        (alias MIC5353-1.8YMT)
        (alias MIC5353-2.6YMT)
        (alias MIC5353-2.8YMT)
        (alias MIC5353-3.0YMT)
        (alias MIC5353-3.3YMT))
      (description "High-performance, single-output,  ultra-low  LDO regulator")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/mic5353.pdf)
      (footprints
        (fp MLF?6?1EP*1.6x1.6mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MIC5353-2.5YMT)
        (field (name Footprint) Package_DFN_QFN:MLF-6-1EP_1.6x1.6mm_P0.5mm_EP0.5x1.26mm))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VIN) (type power_in))
        (pin (num 4) (name VOUT) (type power_out))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name BYP) (type passive))
        (pin (num 7) (name GND) (type passive))))
    (libpart (lib Regulator_Linear) (part NCP133AMX100TCG)
      (description "500  mA  VLDO  equipped  with  NMOS  pass transistor  and  a  separate  bias  supply  voltage")
      (docs http://www.onsemi.com/pub/Collateral/NCP133-D.PDF)
      (footprints
        (fp DFN?6?1EP*1.2x1.2mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) NCP133AMX100TCG))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name ADJ/NC) (type passive))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name BIAS) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name IN) (type power_in))
        (pin (num 7) (name GND) (type passive))))
    (libpart (lib Regulator_Linear) (part TPS51200DRC)
      (description "Sink and Source DDR Termination Regulator, VSON-10")
      (docs http://www.ti.com/lit/ds/symlink/tps51200.pdf)
      (footprints
        (fp *VSON?10?1EP?3x3mm?P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS51200DRC)
        (field (name Footprint) Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm))
      (pins
        (pin (num 1) (name REFIN) (type input))
        (pin (num 2) (name VLDOIN) (type power_in))
        (pin (num 3) (name VO) (type power_out))
        (pin (num 4) (name GND) (type passive))
        (pin (num 5) (name VOSNS) (type input))
        (pin (num 6) (name REFOUT) (type output))
        (pin (num 7) (name EN) (type input))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name PGOOD) (type openCol))
        (pin (num 10) (name VIN) (type power_in))
        (pin (num 11) (name GND) (type passive))))
    (libpart (lib Regulator_Switching) (part TLV62080DSGx)
      (aliases
        (alias TLV62084DSGx)
        (alias TLV62084ADSGx))
      (description "High-efficiency Step-down Converter")
      (docs http://www.ti.com/lit/ds/symlink/tlv62080.pdf)
      (footprints
        (fp *WSON?8?1EP*2x2mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TLV62080DSGx)
        (field (name Footprint) Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name FB) (type input))
        (pin (num 5) (name VOS) (type input))
        (pin (num 6) (name PG) (type openCol))
        (pin (num 7) (name SW) (type power_out))
        (pin (num 8) (name VIN) (type power_in))
        (pin (num 9) (name GND) (type passive))))
    (libpart (lib Regulator_Switching) (part TLV62095RGTx)
      (description "High efficiency step-down converter")
      (docs http://www.ti.com/lit/ds/symlink/tlv62095.pdf)
      (footprints
        (fp *QFN?16?1EP*3x3mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TLV62095RGTx)
        (field (name Footprint) Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm))
      (pins
        (pin (num 1) (name SW) (type power_out))
        (pin (num 2) (name SW) (type power_out))
        (pin (num 3) (name DEF) (type input))
        (pin (num 4) (name PG) (type 3state))
        (pin (num 5) (name FB) (type input))
        (pin (num 6) (name AGND) (type power_in))
        (pin (num 7) (name CP) (type passive))
        (pin (num 8) (name CN) (type passive))
        (pin (num 9) (name SS) (type input))
        (pin (num 10) (name AVIN) (type power_in))
        (pin (num 11) (name PVIN) (type power_in))
        (pin (num 12) (name PVIN) (type power_in))
        (pin (num 13) (name EN) (type input))
        (pin (num 14) (name PGND) (type power_in))
        (pin (num 15) (name PGND) (type power_in))
        (pin (num 16) (name VOS) (type input))
        (pin (num 17) (name AGND) (type power_in))))
    (libpart (lib Regulator_Switching) (part TPS51363)
      (description "High-voltage input, synchronous converter with integrated FET")
      (docs http://www.ti.com/lit/ds/symlink/tps51363.pdf)
      (footprints
        (fp Texas?R?VFQFN?28?1EP*3.5x4.5mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS51363))
      (pins
        (pin (num 1) (name PGOOD) (type openCol))
        (pin (num 2) (name NU) (type NotConnected))
        (pin (num 3) (name MODE) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name BST) (type input))
        (pin (num 6) (name SW) (type power_out))
        (pin (num 7) (name SW) (type passive))
        (pin (num 8) (name SW) (type passive))
        (pin (num 9) (name SW) (type passive))
        (pin (num 10) (name PGND) (type power_in))
        (pin (num 11) (name PGND) (type passive))
        (pin (num 12) (name PGND) (type passive))
        (pin (num 13) (name PGND) (type passive))
        (pin (num 14) (name PGND) (type passive))
        (pin (num 15) (name VIN) (type power_in))
        (pin (num 16) (name VIN) (type passive))
        (pin (num 17) (name VIN) (type passive))
        (pin (num 18) (name V5) (type power_in))
        (pin (num 19) (name GND) (type power_in))
        (pin (num 20) (name TRIP) (type input))
        (pin (num 21) (name SLEW) (type output))
        (pin (num 22) (name VSNS) (type input))
        (pin (num 23) (name GSNS) (type output))
        (pin (num 24) (name REFIN2) (type input))
        (pin (num 25) (name REFIN) (type input))
        (pin (num 26) (name VREF) (type output))
        (pin (num 27) (name NU) (type NotConnected))
        (pin (num 28) (name EN) (type input))
        (pin (num 29) (name EP) (type power_in))))
    (libpart (lib Regulator_Switching) (part TPS62130)
      (aliases
        (alias TPS62130A)
        (alias TPS62131)
        (alias TPS62132)
        (alias TPS62133)
        (alias TPS62150)
        (alias TPS62150A)
        (alias TPS62151)
        (alias TPS62152)
        (alias TPS62153)
        (alias TPS62140)
        (alias TPS62140A)
        (alias TPS62141)
        (alias TPS62142)
        (alias TPS62143))
      (description "3A Step-Down Converter with DCS-Control, Adjustable Output Voltage, 3-17V Input Voltage, QFN-16")
      (docs http://www.ti.com/lit/ds/symlink/tps62130.pdf)
      (footprints
        (fp QFN*3x3mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS62130)
        (field (name Footprint) Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm))
      (pins
        (pin (num 1) (name SW) (type output))
        (pin (num 2) (name SW) (type passive))
        (pin (num 3) (name SW) (type passive))
        (pin (num 4) (name PG) (type openCol))
        (pin (num 5) (name FB) (type input))
        (pin (num 6) (name AGND) (type power_in))
        (pin (num 7) (name FSW) (type input))
        (pin (num 8) (name DEF) (type input))
        (pin (num 9) (name SS/TR) (type input))
        (pin (num 10) (name AVIN) (type power_in))
        (pin (num 11) (name PVIN) (type power_in))
        (pin (num 12) (name PVIN) (type passive))
        (pin (num 13) (name EN) (type input))
        (pin (num 14) (name VOS) (type input))
        (pin (num 15) (name PGND) (type power_in))
        (pin (num 16) (name PGND) (type passive))
        (pin (num 17) (name EP) (type power_in))))
    (libpart (lib Switch) (part SW_DIP_x06)
      (description "6x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
      (footprints
        (fp SW?DIP?x6*))
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_DIP_x06))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Switch) (part SW_Push_SPDT)
      (description "Momentary Switch, single pole double throw")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push_SPDT))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transformer) (part TG111-MSC13LF)
      (description "Single Port Gigabit Ethernet Transformers")
      (docs https://www.haloelectronics.com/pdf/discrete-genesus.pdf)
      (footprints
        (fp Transformer*Ethernet*HALO*TG111*))
      (fields
        (field (name Reference) TR)
        (field (name Value) TG111-MSC13LF)
        (field (name Footprint) Transformer_SMD:Transformer_Ethernet_HALO_TG111-MSC13))
      (pins
        (pin (num 1) (name TCT1) (type passive))
        (pin (num 2) (name TD1+) (type passive))
        (pin (num 3) (name TD1-) (type passive))
        (pin (num 4) (name TCT2) (type passive))
        (pin (num 5) (name TD2+) (type passive))
        (pin (num 6) (name TD2-) (type passive))
        (pin (num 7) (name TCT3) (type passive))
        (pin (num 8) (name TD3+) (type passive))
        (pin (num 9) (name TD3-) (type passive))
        (pin (num 10) (name TCT4) (type passive))
        (pin (num 11) (name TD4+) (type passive))
        (pin (num 12) (name TD4-) (type passive))
        (pin (num 13) (name MX4-) (type passive))
        (pin (num 14) (name MX4+) (type passive))
        (pin (num 15) (name MCT4) (type passive))
        (pin (num 16) (name MTX3-) (type passive))
        (pin (num 17) (name MTX3+) (type passive))
        (pin (num 18) (name MCT3) (type passive))
        (pin (num 19) (name MTX2-) (type passive))
        (pin (num 20) (name MTX2+) (type passive))
        (pin (num 21) (name MCT2) (type passive))
        (pin (num 22) (name MTX1-) (type passive))
        (pin (num 23) (name MTX1+) (type passive))
        (pin (num 24) (name MTC1) (type passive))))
    (libpart (lib Transistor_FET) (part FDG1024NZ)
      (aliases
        (alias FDG6335N))
      (description "1.2A Id, 20V Vds, Dual N-Channel MOSFET, 175mOhm Ron, SC-70-6")
      (docs http://www.fairchildsemi.com/ds/FD/FDG1024NZ.pdf)
      (footprints
        (fp *SC?70*))
      (fields
        (field (name Reference) Q)
        (field (name Value) FDG1024NZ)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-363_SC-70-6))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name G) (type passive))
        (pin (num 3) (name D) (type passive))
        (pin (num 4) (name S) (type passive))
        (pin (num 5) (name G) (type passive))
        (pin (num 6) (name D) (type passive))))
    (libpart (lib Transistor_FET) (part TP0610T)
      (aliases
        (alias VP0610T)
        (alias BSS84)
        (alias NTR2101P)
        (alias BSS83P)
        (alias Si2319CDS)
        (alias IRLML6402))
      (description "-0.18A Id, -60V Vds, P-Channel MOSFET, SOT-23-3")
      (docs http://www.vishay.com/docs/70209/70209.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) TP0610T)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Diode)
      (uri /usr/share/kicad/library/Diode.lib))
    (library (logical Interface_Ethernet)
      (uri /usr/share/kicad/library/Interface_Ethernet.lib))
    (library (logical Interface_USB)
      (uri /usr/share/kicad/library/Interface_USB.lib))
    (library (logical Logic_LevelTranslator)
      (uri /usr/share/kicad/library/Logic_LevelTranslator.lib))
    (library (logical MCU_SiFive)
      (uri /usr/share/kicad/library/MCU_SiFive.lib))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical Memory_EEPROM)
      (uri /usr/share/kicad/library/Memory_EEPROM.lib))
    (library (logical Memory_Flash)
      (uri /usr/share/kicad/library/Memory_Flash.lib))
    (library (logical Memory_RAM)
      (uri /usr/share/kicad/library/Memory_RAM.lib))
    (library (logical Motor)
      (uri /usr/share/kicad/library/Motor.lib))
    (library (logical Oscillator)
      (uri /usr/share/kicad/library/Oscillator.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical Power_Supervisor)
      (uri /usr/share/kicad/library/Power_Supervisor.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical Regulator_Switching)
      (uri /usr/share/kicad/library/Regulator_Switching.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Transformer)
      (uri /usr/share/kicad/library/Transformer.lib))
    (library (logical Transistor_FET)
      (uri /usr/share/kicad/library/Transistor_FET.lib)))
  (nets
    (net (code 10) (name /Freedom-U540_1/CHIPLINK_TX_DAT1_R)
      (node (ref R154) (pin 3))
      (node (ref U1) (pin R19)))
    (net (code 11) (name /Freedom-U540_1/CHIPLINK_TX_DAT3_R)
      (node (ref U1) (pin R20))
      (node (ref R154) (pin 2)))
    (net (code 12) (name /Freedom-U540_1/CHIPLINK_TX_DAT0_R)
      (node (ref U1) (pin T19))
      (node (ref R154) (pin 1)))
    (net (code 13) (name /Freedom-U540_1/CHIPLINK_TX_DAT12_R)
      (node (ref U1) (pin M20))
      (node (ref R152) (pin 4)))
    (net (code 14) (name /Freedom-U540_1/CHIPLINK_TX_DAT6_R)
      (node (ref R152) (pin 3))
      (node (ref U1) (pin N19)))
    (net (code 15) (name /Freedom-U540_1/CHIPLINK_TX_DAT2_R)
      (node (ref R152) (pin 2))
      (node (ref U1) (pin N18)))
    (net (code 16) (name /Freedom-U540_1/CHIPLINK_TX_DAT21_R)
      (node (ref R152) (pin 1))
      (node (ref U1) (pin N20)))
    (net (code 17) (name /Freedom-U540_1/CHIPLINK_TX_DAT4_R)
      (node (ref R154) (pin 4))
      (node (ref U1) (pin P20)))
    (net (code 18) (name /Freedom-U540_1/CHIPLINK_TX_DAT19_R)
      (node (ref R155) (pin 4))
      (node (ref U1) (pin M18)))
    (net (code 19) (name /Freedom-U540_1/CHIPLINK_TX_DAT20_R)
      (node (ref U1) (pin L20))
      (node (ref R155) (pin 3)))
    (net (code 20) (name /Freedom-U540_1/CHIPLINK_TX_DAT23_R)
      (node (ref U1) (pin M19))
      (node (ref R155) (pin 2)))
    (net (code 21) (name /Freedom-U540_1/CHIPLINK_TX_DAT15_R)
      (node (ref U1) (pin M17))
      (node (ref R155) (pin 1)))
    (net (code 22) (name /Freedom-U540_1/CHIPLINK_TX_DAT28_R)
      (node (ref U1) (pin K19))
      (node (ref R153) (pin 4)))
    (net (code 23) (name VCCQ)
      (node (ref U1) (pin U7))
      (node (ref C99) (pin 1))
      (node (ref C125) (pin 1))
      (node (ref RS2) (pin 4))
      (node (ref U1) (pin R7))
      (node (ref U1) (pin H6))
      (node (ref U1) (pin G7))
      (node (ref U1) (pin J7))
      (node (ref C98) (pin 1))
      (node (ref C97) (pin 1))
      (node (ref C94) (pin 1))
      (node (ref C96) (pin 1))
      (node (ref C95) (pin 1))
      (node (ref U1) (pin L7))
      (node (ref U1) (pin M6))
      (node (ref U1) (pin K6))
      (node (ref U1) (pin N7))
      (node (ref R178) (pin 2))
      (node (ref U1) (pin P6))
      (node (ref U1) (pin T6)))
    (net (code 24) (name "Net-(R70-Pad2)")
      (node (ref R70) (pin 2))
      (node (ref U1) (pin F6)))
    (net (code 25) (name /Freedom-U540_1/CHIPLINK_TX_DAT30_R)
      (node (ref R153) (pin 3))
      (node (ref U1) (pin L18)))
    (net (code 26) (name /Freedom-U540_1/GEMGXL_TXD2_R)
      (node (ref U1) (pin D11))
      (node (ref R75) (pin 6)))
    (net (code 27) (name /Freedom-U540_1/GEMGXL_TXD0_R)
      (node (ref R75) (pin 8))
      (node (ref U1) (pin B12)))
    (net (code 28) (name /Freedom-U540_1/CHIPLINK_TX_DAT27_R)
      (node (ref U1) (pin L19))
      (node (ref R153) (pin 2)))
    (net (code 29) (name /Freedom-U540_1/CHIPLINK_TX_DAT31_R)
      (node (ref R153) (pin 1))
      (node (ref U1) (pin L17)))
    (net (code 30) (name /Freedom-U540_1/GEMGXL_TXD6_R)
      (node (ref R76) (pin 6))
      (node (ref U1) (pin B8)))
    (net (code 31) (name /Freedom-U540_1/GEMGXL_TXD5_R)
      (node (ref U1) (pin D10))
      (node (ref R76) (pin 7)))
    (net (code 32) (name /Freedom-U540_1/GEMGXL_TXD4_R)
      (node (ref R76) (pin 8))
      (node (ref U1) (pin C10)))
    (net (code 33) (name /Freedom-U540_1/GEMGXL_TXD1_R)
      (node (ref R75) (pin 7))
      (node (ref U1) (pin C11)))
    (net (code 34) (name /Freedom-U540_1/GEMGXL_TXD3_R)
      (node (ref U1) (pin F11))
      (node (ref R75) (pin 5)))
    (net (code 35) (name /Freedom-U540_1/GEMGXL_TXD7_R)
      (node (ref U1) (pin D9))
      (node (ref R76) (pin 5)))
    (net (code 36) (name /Freedom-U540_1/CHIPLINK_TX_CLK_R)
      (node (ref U1) (pin P19))
      (node (ref R148) (pin 2)))
    (net (code 37) (name /Freedom-U540_1/CHIPLINK_TX_SEND_R)
      (node (ref U1) (pin N17))
      (node (ref R149) (pin 2)))
    (net (code 38) (name /Freedom-U540_1/CHIPLINK_TX_RST_R)
      (node (ref R150) (pin 2))
      (node (ref U1) (pin T20)))
    (net (code 39) (name /Freedom-U540_1/GEMGXL_TX_ER_R)
      (node (ref R78) (pin 1))
      (node (ref U1) (pin F10)))
    (net (code 40) (name /Freedom-U540_1/GEMGXL_TX_EN_R)
      (node (ref R77) (pin 1))
      (node (ref U1) (pin B7)))
    (net (code 41) (name /Freedom-U540_1/CHIPLINK_TX_DAT5_R)
      (node (ref U1) (pin U20))
      (node (ref R151) (pin 3)))
    (net (code 42) (name /Freedom-U540_1/CHIPLINK_TX_DAT29_R)
      (node (ref U1) (pin L22))
      (node (ref R145) (pin 3)))
    (net (code 43) (name /Freedom-U540_1/CHIPLINK_TX_DAT26_R)
      (node (ref U1) (pin K22))
      (node (ref R145) (pin 1)))
    (net (code 44) (name /Freedom-U540_1/CHIPLINK_TX_DAT25_R)
      (node (ref R146) (pin 2))
      (node (ref U1) (pin M21)))
    (net (code 45) (name /Freedom-U540_1/CHIPLINK_TX_DAT24_R)
      (node (ref U1) (pin K20))
      (node (ref R145) (pin 2)))
    (net (code 46) (name /Freedom-U540_1/CHIPLINK_TX_DAT22_R)
      (node (ref U1) (pin M22))
      (node (ref R146) (pin 1)))
    (net (code 47) (name /Freedom-U540_1/CHIPLINK_TX_DAT18_R)
      (node (ref U1) (pin L21))
      (node (ref R145) (pin 4)))
    (net (code 48) (name /Freedom-U540_1/CHIPLINK_TX_DAT17_R)
      (node (ref U1) (pin R22))
      (node (ref R147) (pin 1)))
    (net (code 49) (name /Freedom-U540_1/CHIPLINK_TX_DAT16_R)
      (node (ref U1) (pin N21))
      (node (ref R146) (pin 4)))
    (net (code 50) (name /Freedom-U540_1/CHIPLINK_TX_DAT14_R)
      (node (ref U1) (pin N22))
      (node (ref R146) (pin 3)))
    (net (code 51) (name /Freedom-U540_1/CHIPLINK_TX_DAT13_R)
      (node (ref R147) (pin 4))
      (node (ref U1) (pin T21)))
    (net (code 52) (name /Freedom-U540_1/CHIPLINK_TX_DAT11_R)
      (node (ref U1) (pin U21))
      (node (ref R151) (pin 2)))
    (net (code 53) (name /Freedom-U540_1/CHIPLINK_TX_DAT10_R)
      (node (ref U1) (pin T22))
      (node (ref R147) (pin 3)))
    (net (code 54) (name /Freedom-U540_1/CHIPLINK_TX_DAT9_R)
      (node (ref U1) (pin W22))
      (node (ref R151) (pin 4)))
    (net (code 55) (name /Freedom-U540_1/CHIPLINK_TX_DAT8_R)
      (node (ref R147) (pin 2))
      (node (ref U1) (pin R21)))
    (net (code 56) (name /Freedom-U540_1/CHIPLINK_TX_DAT7_R)
      (node (ref U1) (pin U22))
      (node (ref R151) (pin 1)))
    (net (code 57) (name VDD_DDRPLL_P)
      (node (ref RS10) (pin 4))
      (node (ref L5) (pin 2))
      (node (ref J14) (pin 13))
      (node (ref RS3) (pin 2))
      (node (ref C150) (pin 1)))
    (net (code 58) (name VMEM)
      (node (ref L4) (pin 2))
      (node (ref RS1) (pin 4))
      (node (ref R60) (pin 2))
      (node (ref RS2) (pin 1))
      (node (ref C140) (pin 2))
      (node (ref C141) (pin 2))
      (node (ref U16) (pin 16)))
    (net (code 59) (name VDD_GIVDD_N)
      (node (ref C128) (pin 1))
      (node (ref J14) (pin 18))
      (node (ref RS5) (pin 2))
      (node (ref U1) (pin J11)))
    (net (code 60) (name VDD_GEMGXLPLL_N)
      (node (ref C129) (pin 1))
      (node (ref U1) (pin K12))
      (node (ref J14) (pin 20))
      (node (ref RS6) (pin 1)))
    (net (code 61) (name DDR_DQ0)
      (node (ref U1) (pin D2))
      (node (ref U2) (pin D3)))
    (net (code 62) (name VDD_DDRPLL_N)
      (node (ref U1) (pin M9))
      (node (ref U1) (pin L9))
      (node (ref J14) (pin 14))
      (node (ref C126) (pin 1))
      (node (ref RS3) (pin 1)))
    (net (code 63) (name AVDD_DDRPLL_N)
      (node (ref C127) (pin 1))
      (node (ref J14) (pin 16))
      (node (ref U1) (pin K13))
      (node (ref RS4) (pin 2)))
    (net (code 64) (name DDR_DQ1)
      (node (ref U1) (pin B1))
      (node (ref U2) (pin D2)))
    (net (code 65) (name CHIPLINK_RX_SEND)
      (node (ref U1) (pin W21))
      (node (ref J9) (pin G36)))
    (net (code 66) (name CHIPLINK_RX_RST)
      (node (ref J9) (pin G37))
      (node (ref U1) (pin P17)))
    (net (code 67) (name CHIPLINK_RX_CLK)
      (node (ref J9) (pin G2))
      (node (ref U1) (pin AA22)))
    (net (code 68) (name AGND)
      (node (ref U1) (pin G10))
      (node (ref U1) (pin F7))
      (node (ref U1) (pin L10))
      (node (ref U1) (pin G8))
      (node (ref U1) (pin G6))
      (node (ref U1) (pin G12))
      (node (ref U1) (pin G16))
      (node (ref U1) (pin G2))
      (node (ref U1) (pin L15))
      (node (ref U1) (pin H7))
      (node (ref J1) (pin 2))
      (node (ref U1) (pin E4))
      (node (ref U1) (pin A1))
      (node (ref U1) (pin A14))
      (node (ref U1) (pin A18))
      (node (ref U1) (pin A2))
      (node (ref U1) (pin A22))
      (node (ref U1) (pin A3))
      (node (ref U1) (pin K9))
      (node (ref U1) (pin H9))
      (node (ref U1) (pin J1))
      (node (ref U1) (pin J10))
      (node (ref U1) (pin J16))
      (node (ref U1) (pin J22))
      (node (ref U1) (pin J6))
      (node (ref U1) (pin J8))
      (node (ref U1) (pin K11))
      (node (ref U1) (pin K7))
      (node (ref U1) (pin K15))
      (node (ref U1) (pin L12))
      (node (ref U1) (pin H15))
      (node (ref U1) (pin J14))
      (node (ref C267) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J9) (pin B14))
      (node (ref J9) (pin A9))
      (node (ref J9) (pin B10))
      (node (ref J9) (pin B11))
      (node (ref J9) (pin B15))
      (node (ref J9) (pin B31))
      (node (ref J9) (pin B34))
      (node (ref J9) (pin B26))
      (node (ref J9) (pin B38))
      (node (ref J9) (pin B39))
      (node (ref J9) (pin B6))
      (node (ref J9) (pin B7))
      (node (ref J4) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref J9) (pin B23))
      (node (ref J3) (pin 2))
      (node (ref J9) (pin B22))
      (node (ref J9) (pin B2))
      (node (ref J1) (pin 39))
      (node (ref J9) (pin B19))
      (node (ref J10) (pin 6))
      (node (ref J10) (pin 11))
      (node (ref J10) (pin 10))
      (node (ref J9) (pin A32))
      (node (ref U1) (pin D1))
      (node (ref J9) (pin A28))
      (node (ref J9) (pin A29))
      (node (ref U1) (pin A9))
      (node (ref U1) (pin AB4))
      (node (ref U1) (pin D12))
      (node (ref J9) (pin A33))
      (node (ref J9) (pin A36))
      (node (ref J9) (pin A37))
      (node (ref J9) (pin A4))
      (node (ref J9) (pin A40))
      (node (ref J9) (pin A5))
      (node (ref U1) (pin AB22))
      (node (ref U1) (pin AB17))
      (node (ref U12) (pin 10))
      (node (ref U1) (pin N15))
      (node (ref J9) (pin B18))
      (node (ref J9) (pin A17))
      (node (ref U1) (pin M15))
      (node (ref U1) (pin E22))
      (node (ref U1) (pin T7))
      (node (ref S2) (pin 1))
      (node (ref J9) (pin A24))
      (node (ref J9) (pin A25))
      (node (ref J9) (pin B35))
      (node (ref J9) (pin B27))
      (node (ref J9) (pin B3))
      (node (ref J9) (pin B30))
      (node (ref J1) (pin 40))
      (node (ref J9) (pin A1))
      (node (ref J9) (pin A12))
      (node (ref J9) (pin A13))
      (node (ref J9) (pin A16))
      (node (ref J9) (pin A8))
      (node (ref J9) (pin A20))
      (node (ref U1) (pin AB13))
      (node (ref U1) (pin AB10))
      (node (ref U1) (pin AB1))
      (node (ref U1) (pin AA2))
      (node (ref J9) (pin A21))
      (node (ref U1) (pin AB7))
      (node (ref C137) (pin 1))
      (node (ref Y1) (pin 2))
      (node (ref S1) (pin 11))
      (node (ref S3) (pin 11))
      (node (ref S3) (pin 12))
      (node (ref S1) (pin 10))
      (node (ref S1) (pin 7))
      (node (ref S1) (pin 8))
      (node (ref S1) (pin 9))
      (node (ref S1) (pin 12))
      (node (ref J9) (pin D3))
      (node (ref U1) (pin V7))
      (node (ref J9) (pin D28))
      (node (ref U1) (pin V9))
      (node (ref Q1) (pin 1))
      (node (ref J9) (pin E17))
      (node (ref J9) (pin E23))
      (node (ref J9) (pin E20))
      (node (ref Q1) (pin 4))
      (node (ref J9) (pin E14))
      (node (ref J9) (pin E11))
      (node (ref J9) (pin E1))
      (node (ref U1) (pin V22))
      (node (ref J9) (pin C5))
      (node (ref J9) (pin C40))
      (node (ref J9) (pin C4))
      (node (ref J9) (pin C38))
      (node (ref J9) (pin C36))
      (node (ref J9) (pin C8))
      (node (ref J9) (pin C33))
      (node (ref J9) (pin C32))
      (node (ref J9) (pin C29))
      (node (ref J9) (pin C28))
      (node (ref J9) (pin D25))
      (node (ref Q2) (pin 1))
      (node (ref Q2) (pin 4))
      (node (ref S3) (pin 10))
      (node (ref Q4) (pin 4))
      (node (ref J9) (pin D7))
      (node (ref J9) (pin D6))
      (node (ref J9) (pin D39))
      (node (ref U1) (pin V15))
      (node (ref J9) (pin D37))
      (node (ref U18) (pin 10))
      (node (ref U27) (pin 17))
      (node (ref U27) (pin 5))
      (node (ref U27) (pin 6))
      (node (ref U27) (pin 8))
      (node (ref U27) (pin 16))
      (node (ref U18) (pin 11))
      (node (ref C121) (pin 1))
      (node (ref C135) (pin 1))
      (node (ref C220) (pin 1))
      (node (ref C218) (pin 1))
      (node (ref U14) (pin 2))
      (node (ref U14) (pin 3))
      (node (ref U14) (pin 9))
      (node (ref D11) (pin 1))
      (node (ref R58) (pin 2))
      (node (ref R54) (pin 2))
      (node (ref C116) (pin 1))
      (node (ref R55) (pin 2))
      (node (ref R56) (pin 2))
      (node (ref R39) (pin 2))
      (node (ref R57) (pin 2))
      (node (ref U50) (pin 2))
      (node (ref U50) (pin 3))
      (node (ref U50) (pin 9))
      (node (ref C281) (pin 1))
      (node (ref R156) (pin 2))
      (node (ref U27) (pin 7))
      (node (ref R59) (pin 2))
      (node (ref U27) (pin 15))
      (node (ref C144) (pin 2))
      (node (ref C152) (pin 1))
      (node (ref R71) (pin 1))
      (node (ref C147) (pin 1))
      (node (ref C151) (pin 2))
      (node (ref C119) (pin 1))
      (node (ref C145) (pin 2))
      (node (ref U19) (pin 2))
      (node (ref U18) (pin 19))
      (node (ref U18) (pin 23))
      (node (ref U16) (pin 6))
      (node (ref U18) (pin 29))
      (node (ref S3) (pin 7))
      (node (ref S3) (pin 8))
      (node (ref S3) (pin 9))
      (node (ref U18) (pin 14))
      (node (ref U18) (pin 12))
      (node (ref U18) (pin 13))
      (node (ref J9) (pin D22))
      (node (ref R61) (pin 1))
      (node (ref U17) (pin 2))
      (node (ref J9) (pin C21))
      (node (ref J9) (pin C20))
      (node (ref J9) (pin C16))
      (node (ref J9) (pin C13))
      (node (ref J9) (pin C12))
      (node (ref J9) (pin C1))
      (node (ref J14) (pin 21))
      (node (ref J14) (pin 22))
      (node (ref J9) (pin C24))
      (node (ref J9) (pin E4))
      (node (ref J9) (pin G11))
      (node (ref U1) (pin P13))
      (node (ref J9) (pin G1))
      (node (ref U1) (pin N6))
      (node (ref J9) (pin F9))
      (node (ref J9) (pin E35))
      (node (ref J9) (pin E5))
      (node (ref U1) (pin P22))
      (node (ref U1) (pin P7))
      (node (ref J9) (pin E40))
      (node (ref U1) (pin P9))
      (node (ref U1) (pin R10))
      (node (ref U1) (pin P11))
      (node (ref J9) (pin E38))
      (node (ref U1) (pin L14))
      (node (ref U1) (pin L6))
      (node (ref U1) (pin L8))
      (node (ref J9) (pin E8))
      (node (ref U1) (pin M11))
      (node (ref J9) (pin E32))
      (node (ref U1) (pin M13))
      (node (ref J9) (pin E29))
      (node (ref U1) (pin M7))
      (node (ref J9) (pin F24))
      (node (ref J9) (pin F33))
      (node (ref J9) (pin D2))
      (node (ref J9) (pin D19))
      (node (ref J9) (pin E26))
      (node (ref J9) (pin D16))
      (node (ref J9) (pin D13))
      (node (ref J9) (pin D10))
      (node (ref J9) (pin C9))
      (node (ref J9) (pin F6))
      (node (ref J9) (pin F39))
      (node (ref J9) (pin F36))
      (node (ref U1) (pin N10))
      (node (ref J9) (pin F30))
      (node (ref J9) (pin F3))
      (node (ref U26) (pin 13))
      (node (ref J9) (pin F27))
      (node (ref J9) (pin G17))
      (node (ref J9) (pin G23))
      (node (ref J9) (pin G20))
      (node (ref U1) (pin P15))
      (node (ref U1) (pin N8))
      (node (ref U1) (pin P1))
      (node (ref J9) (pin G14))
      (node (ref U1) (pin T15))
      (node (ref U1) (pin R14))
      (node (ref U1) (pin R16))
      (node (ref U1) (pin R6))
      (node (ref U1) (pin R8))
      (node (ref U1) (pin T11))
      (node (ref U1) (pin T13))
      (node (ref U1) (pin R12))
      (node (ref U1) (pin T17))
      (node (ref J9) (pin C17))
      (node (ref J9) (pin C25))
      (node (ref U1) (pin U14))
      (node (ref J9) (pin F21))
      (node (ref U1) (pin N12))
      (node (ref J9) (pin F2))
      (node (ref U1) (pin N14))
      (node (ref U1) (pin U16))
      (node (ref J9) (pin F18))
      (node (ref U1) (pin T9))
      (node (ref U1) (pin U10))
      (node (ref J9) (pin F15))
      (node (ref U1) (pin U12))
      (node (ref J9) (pin F12))
      (node (ref U1) (pin U6))
      (node (ref U1) (pin U8))
      (node (ref U1) (pin V1))
      (node (ref U1) (pin V11))
      (node (ref U1) (pin V13))
      (node (ref C138) (pin 1))
      (node (ref J9) (pin G26))
      (node (ref U2) (pin A2))
      (node (ref U3) (pin N1))
      (node (ref U2) (pin A8))
      (node (ref U2) (pin A9))
      (node (ref J9) (pin G38))
      (node (ref C257) (pin 2))
      (node (ref C258) (pin 2))
      (node (ref J9) (pin G32))
      (node (ref J9) (pin G29))
      (node (ref J9) (pin H18))
      (node (ref J9) (pin H24))
      (node (ref J9) (pin H21))
      (node (ref J9) (pin H2))
      (node (ref C241) (pin 2))
      (node (ref C242) (pin 1))
      (node (ref J9) (pin H36))
      (node (ref C134) (pin 1))
      (node (ref J9) (pin J23))
      (node (ref C243) (pin 2))
      (node (ref J9) (pin J20))
      (node (ref C245) (pin 2))
      (node (ref J9) (pin H27))
      (node (ref C246) (pin 2))
      (node (ref J9) (pin J17))
      (node (ref C247) (pin 2))
      (node (ref J9) (pin J14))
      (node (ref C248) (pin 2))
      (node (ref J9) (pin J11))
      (node (ref J9) (pin G35))
      (node (ref J9) (pin G8))
      (node (ref J9) (pin G5))
      (node (ref C206) (pin 1))
      (node (ref C207) (pin 1))
      (node (ref X1) (pin 2))
      (node (ref J9) (pin G40))
      (node (ref J9) (pin G4))
      (node (ref C136) (pin 1))
      (node (ref J9) (pin H39))
      (node (ref C252) (pin 2))
      (node (ref C249) (pin 2))
      (node (ref C250) (pin 2))
      (node (ref J9) (pin H9))
      (node (ref C251) (pin 2))
      (node (ref J9) (pin H6))
      (node (ref C253) (pin 2))
      (node (ref J9) (pin J1))
      (node (ref C254) (pin 2))
      (node (ref C255) (pin 2))
      (node (ref J9) (pin H33))
      (node (ref C256) (pin 2))
      (node (ref C244) (pin 2))
      (node (ref J9) (pin H30))
      (node (ref J9) (pin H3))
      (node (ref J9) (pin J26))
      (node (ref C269) (pin 1))
      (node (ref U2) (pin G1))
      (node (ref U2) (pin N1))
      (node (ref U2) (pin K9))
      (node (ref U3) (pin K9))
      (node (ref U3) (pin K1))
      (node (ref U3) (pin C8))
      (node (ref U3) (pin D1))
      (node (ref U3) (pin D9))
      (node (ref C20) (pin 1))
      (node (ref U3) (pin G9))
      (node (ref U3) (pin H9))
      (node (ref U2) (pin C8))
      (node (ref U2) (pin D1))
      (node (ref U2) (pin D9))
      (node (ref U2) (pin E1))
      (node (ref U2) (pin E9))
      (node (ref U3) (pin E9))
      (node (ref C284) (pin 1))
      (node (ref U3) (pin G1))
      (node (ref U3) (pin E1))
      (node (ref C270) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref U2) (pin G9))
      (node (ref U2) (pin H9))
      (node (ref U2) (pin K1))
      (node (ref C39) (pin 1))
      (node (ref C40) (pin 1))
      (node (ref C18) (pin 1))
      (node (ref C240) (pin 1))
      (node (ref C268) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref C198) (pin 1))
      (node (ref C190) (pin 2))
      (node (ref R95) (pin 2))
      (node (ref R94) (pin 2))
      (node (ref R96) (pin 2))
      (node (ref R92) (pin 2))
      (node (ref C200) (pin 1))
      (node (ref C201) (pin 1))
      (node (ref C202) (pin 1))
      (node (ref C203) (pin 2))
      (node (ref C203) (pin 1))
      (node (ref Y3) (pin 2))
      (node (ref C173) (pin 1))
      (node (ref C172) (pin 1))
      (node (ref C176) (pin 1))
      (node (ref C174) (pin 1))
      (node (ref C175) (pin 1))
      (node (ref C170) (pin 1))
      (node (ref C171) (pin 1))
      (node (ref C177) (pin 1))
      (node (ref C197) (pin 1))
      (node (ref C205) (pin 2))
      (node (ref C199) (pin 1))
      (node (ref R93) (pin 1))
      (node (ref C65) (pin 1))
      (node (ref C87) (pin 1))
      (node (ref C67) (pin 1))
      (node (ref C278) (pin 1))
      (node (ref C279) (pin 1))
      (node (ref C69) (pin 1))
      (node (ref C277) (pin 1))
      (node (ref C210) (pin 1))
      (node (ref C271) (pin 1))
      (node (ref C272) (pin 1))
      (node (ref C273) (pin 1))
      (node (ref C274) (pin 1))
      (node (ref C280) (pin 1))
      (node (ref C275) (pin 1))
      (node (ref C276) (pin 1))
      (node (ref C169) (pin 1))
      (node (ref Y2) (pin 2))
      (node (ref C100) (pin 1))
      (node (ref C92) (pin 1))
      (node (ref C111) (pin 1))
      (node (ref C90) (pin 1))
      (node (ref U11) (pin 8))
      (node (ref C66) (pin 1))
      (node (ref R11) (pin 2))
      (node (ref C68) (pin 1))
      (node (ref U33) (pin 3))
      (node (ref C70) (pin 1))
      (node (ref C91) (pin 1))
      (node (ref C112) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref U11) (pin 4))
      (node (ref U32) (pin 3))
      (node (ref C93) (pin 1))
      (node (ref C23) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref C103) (pin 1))
      (node (ref U29) (pin 3))
      (node (ref C108) (pin 1))
      (node (ref C102) (pin 1))
      (node (ref J12) (pin SH))
      (node (ref C187) (pin 1))
      (node (ref C188) (pin 2))
      (node (ref C189) (pin 2))
      (node (ref C191) (pin 2))
      (node (ref C167) (pin 1))
      (node (ref C185) (pin 1))
      (node (ref C196) (pin 1))
      (node (ref C179) (pin 2))
      (node (ref C181) (pin 2))
      (node (ref C182) (pin 2))
      (node (ref C183) (pin 2))
      (node (ref C184) (pin 1))
      (node (ref C180) (pin 1))
      (node (ref C115) (pin 1))
      (node (ref C211) (pin 1))
      (node (ref C101) (pin 1))
      (node (ref C107) (pin 1))
      (node (ref C114) (pin 1))
      (node (ref C106) (pin 1))
      (node (ref C105) (pin 1))
      (node (ref C104) (pin 1))
      (node (ref U28) (pin 3))
      (node (ref C178) (pin 2))
      (node (ref C193) (pin 2))
      (node (ref C194) (pin 2))
      (node (ref C195) (pin 2))
      (node (ref C186) (pin 2))
      (node (ref C192) (pin 2))
      (node (ref R117) (pin 2))
      (node (ref C166) (pin 1))
      (node (ref C63) (pin 1))
      (node (ref C62) (pin 1))
      (node (ref C64) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref U9) (pin N1))
      (node (ref U8) (pin A2))
      (node (ref U9) (pin G9))
      (node (ref U9) (pin K9))
      (node (ref C56) (pin 1))
      (node (ref U9) (pin K1))
      (node (ref U9) (pin H9))
      (node (ref U8) (pin E9))
      (node (ref U8) (pin G1))
      (node (ref U8) (pin G9))
      (node (ref U8) (pin H9))
      (node (ref U8) (pin A8))
      (node (ref U8) (pin A9))
      (node (ref U8) (pin C8))
      (node (ref C89) (pin 1))
      (node (ref C47) (pin 1))
      (node (ref C46) (pin 1))
      (node (ref C48) (pin 1))
      (node (ref C55) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref U9) (pin D1))
      (node (ref U9) (pin D9))
      (node (ref U9) (pin E9))
      (node (ref U9) (pin E1))
      (node (ref U10) (pin N1))
      (node (ref U9) (pin A8))
      (node (ref U9) (pin A9))
      (node (ref U9) (pin A2))
      (node (ref U9) (pin C8))
      (node (ref U10) (pin K9))
      (node (ref U8) (pin D1))
      (node (ref U8) (pin D9))
      (node (ref U8) (pin E1))
      (node (ref C126) (pin 2))
      (node (ref R70) (pin 1))
      (node (ref U10) (pin H9))
      (node (ref U10) (pin K1))
      (node (ref U9) (pin G1))
      (node (ref C61) (pin 1))
      (node (ref U10) (pin D9))
      (node (ref U10) (pin E1))
      (node (ref U10) (pin E9))
      (node (ref U10) (pin G1))
      (node (ref U10) (pin G9))
      (node (ref C125) (pin 2))
      (node (ref C99) (pin 2))
      (node (ref C127) (pin 2))
      (node (ref C43) (pin 1))
      (node (ref C80) (pin 1))
      (node (ref C129) (pin 2))
      (node (ref C81) (pin 1))
      (node (ref C82) (pin 1))
      (node (ref C83) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref C42) (pin 1))
      (node (ref C44) (pin 2))
      (node (ref R6) (pin 1))
      (node (ref C85) (pin 1))
      (node (ref C84) (pin 1))
      (node (ref C97) (pin 2))
      (node (ref C94) (pin 2))
      (node (ref C96) (pin 2))
      (node (ref C95) (pin 2))
      (node (ref C86) (pin 1))
      (node (ref C79) (pin 1))
      (node (ref C128) (pin 2))
      (node (ref C98) (pin 2))
      (node (ref J17) (pin 2))
      (node (ref J16) (pin 2))
      (node (ref J15) (pin 2))
      (node (ref C50) (pin 1))
      (node (ref C49) (pin 1))
      (node (ref C51) (pin 1))
      (node (ref C52) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref C57) (pin 1))
      (node (ref C58) (pin 1))
      (node (ref C59) (pin 1))
      (node (ref C60) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref C74) (pin 1))
      (node (ref C77) (pin 1))
      (node (ref C76) (pin 1))
      (node (ref C75) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref C72) (pin 1))
      (node (ref C73) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref C78) (pin 1))
      (node (ref U10) (pin A2))
      (node (ref U10) (pin A8))
      (node (ref U10) (pin A9))
      (node (ref C45) (pin 1))
      (node (ref U10) (pin C8))
      (node (ref U10) (pin D1))
      (node (ref U6) (pin C8))
      (node (ref U6) (pin D9))
      (node (ref U1) (pin H11))
      (node (ref J18) (pin 2))
      (node (ref U1) (pin J12))
      (node (ref U6) (pin E1))
      (node (ref U13) (pin 15))
      (node (ref U7) (pin E1))
      (node (ref U8) (pin N1))
      (node (ref U7) (pin G9))
      (node (ref U7) (pin H9))
      (node (ref U7) (pin C8))
      (node (ref U7) (pin K1))
      (node (ref U7) (pin K9))
      (node (ref U7) (pin D1))
      (node (ref U7) (pin D9))
      (node (ref U8) (pin K9))
      (node (ref U7) (pin E9))
      (node (ref U7) (pin G1))
      (node (ref U6) (pin N1))
      (node (ref U6) (pin D1))
      (node (ref U7) (pin N1))
      (node (ref U6) (pin A2))
      (node (ref U6) (pin A8))
      (node (ref U1) (pin J13))
      (node (ref U6) (pin A9))
      (node (ref U6) (pin K1))
      (node (ref U6) (pin K9))
      (node (ref U6) (pin E9))
      (node (ref U6) (pin G1))
      (node (ref U6) (pin G9))
      (node (ref U6) (pin H9))
      (node (ref U7) (pin A2))
      (node (ref U7) (pin A8))
      (node (ref U7) (pin A9))
      (node (ref U8) (pin K1))
      (node (ref J7) (pin 6))
      (node (ref J7) (pin 5))
      (node (ref U13) (pin 11))
      (node (ref U13) (pin 10))
      (node (ref U13) (pin 13))
      (node (ref U13) (pin 1))
      (node (ref U5) (pin A8))
      (node (ref U5) (pin A9))
      (node (ref U5) (pin C8))
      (node (ref U5) (pin D1))
      (node (ref C19) (pin 1))
      (node (ref U3) (pin A2))
      (node (ref U3) (pin A8))
      (node (ref U3) (pin A9))
      (node (ref U4) (pin H9))
      (node (ref C30) (pin 1))
      (node (ref U4) (pin K9))
      (node (ref U4) (pin K1))
      (node (ref U5) (pin A2))
      (node (ref U5) (pin K1))
      (node (ref J2) (pin 15))
      (node (ref J2) (pin 20))
      (node (ref U5) (pin K9))
      (node (ref U5) (pin D9))
      (node (ref U5) (pin E1))
      (node (ref J13) (pin 8))
      (node (ref C120) (pin 1))
      (node (ref C265) (pin 1))
      (node (ref Q5) (pin 4))
      (node (ref C2) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref J19) (pin 3))
      (node (ref C11) (pin 1))
      (node (ref S4) (pin 3))
      (node (ref C12) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref J9) (pin J29))
      (node (ref J9) (pin K30))
      (node (ref J9) (pin K33))
      (node (ref J9) (pin K36))
      (node (ref J9) (pin K6))
      (node (ref J9) (pin K9))
      (node (ref J9) (pin K39))
      (node (ref J9) (pin H12))
      (node (ref J9) (pin H15))
      (node (ref C7) (pin 1))
      (node (ref U4) (pin G1))
      (node (ref U4) (pin G9))
      (node (ref U5) (pin N1))
      (node (ref U4) (pin A2))
      (node (ref U4) (pin A8))
      (node (ref U4) (pin D1))
      (node (ref U4) (pin C8))
      (node (ref U4) (pin A9))
      (node (ref U4) (pin E9))
      (node (ref U4) (pin N1))
      (node (ref C35) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C28) (pin 1))
      (node (ref U5) (pin E9))
      (node (ref C34) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref D8) (pin 2))
      (node (ref U4) (pin D9))
      (node (ref U4) (pin E1))
      (node (ref D10) (pin 1))
      (node (ref U21) (pin 3))
      (node (ref C117) (pin 1))
      (node (ref U23) (pin 3))
      (node (ref C162) (pin 2))
      (node (ref C163) (pin 1))
      (node (ref C164) (pin 2))
      (node (ref C165) (pin 2))
      (node (ref U16) (pin 14))
      (node (ref C154) (pin 2))
      (node (ref C155) (pin 2))
      (node (ref C156) (pin 2))
      (node (ref C157) (pin 2))
      (node (ref U22) (pin 3))
      (node (ref U24) (pin 3))
      (node (ref C158) (pin 2))
      (node (ref U16) (pin 17))
      (node (ref U20) (pin 3))
      (node (ref C153) (pin 2))
      (node (ref U16) (pin 15))
      (node (ref R29) (pin 2))
      (node (ref R41) (pin 2))
      (node (ref R27) (pin 2))
      (node (ref C150) (pin 2))
      (node (ref R28) (pin 2))
      (node (ref C149) (pin 1))
      (node (ref U15) (pin 2))
      (node (ref C148) (pin 1))
      (node (ref D12) (pin 1))
      (node (ref C132) (pin 2))
      (node (ref D9) (pin 1))
      (node (ref C131) (pin 2))
      (node (ref C118) (pin 1))
      (node (ref C133) (pin 2))
      (node (ref C219) (pin 1))
      (node (ref X2) (pin 2))
      (node (ref C130) (pin 2))
      (node (ref C159) (pin 2))
      (node (ref C122) (pin 1))
      (node (ref C160) (pin 2))
      (node (ref C161) (pin 2))
      (node (ref R30) (pin 2))
      (node (ref R53) (pin 2))
      (node (ref U15) (pin 3))
      (node (ref U15) (pin 9))
      (node (ref C124) (pin 1))
      (node (ref C139) (pin 1))
      (node (ref U5) (pin H9))
      (node (ref U5) (pin G1))
      (node (ref U5) (pin G9))
      (node (ref J11) (pin 10))
      (node (ref J11) (pin 2))
      (node (ref U25) (pin 3))
      (node (ref C143) (pin 2))
      (node (ref C140) (pin 1))
      (node (ref C141) (pin 1))
      (node (ref U35) (pin 7))
      (node (ref C216) (pin 2))
      (node (ref M3) (pin 1))
      (node (ref C217) (pin 2))
      (node (ref U36) (pin 5))
      (node (ref C209) (pin 1))
      (node (ref U13) (pin 51))
      (node (ref U35) (pin 2))
      (node (ref C88) (pin 2))
      (node (ref C215) (pin 2))
      (node (ref R33) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref U36) (pin 7))
      (node (ref D5) (pin 1))
      (node (ref C214) (pin 2))
      (node (ref C212) (pin 1))
      (node (ref C113) (pin 1))
      (node (ref C213) (pin 2))
      (node (ref C264) (pin 1))
      (node (ref C263) (pin 1))
      (node (ref M2) (pin 1))
      (node (ref M6) (pin 1))
      (node (ref M5) (pin 1))
      (node (ref M4) (pin 1))
      (node (ref C208) (pin 2))
      (node (ref U37) (pin 3))
      (node (ref U38) (pin 3))
      (node (ref M1) (pin 1))
      (node (ref R116) (pin 1))
      (node (ref J8) (pin 2))
      (node (ref C168) (pin 1))
      (node (ref U13) (pin 25))
      (node (ref C259) (pin 1))
      (node (ref U13) (pin 47))
      (node (ref U13) (pin 35))
      (node (ref C204) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref U11) (pin 11))
      (node (ref U30) (pin 3))
      (node (ref C33) (pin 1))
      (node (ref IC1) (pin 69))
      (node (ref R3) (pin 1))
      (node (ref U31) (pin 3))
      (node (ref C32) (pin 1))
      (node (ref C110) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref C109) (pin 1))
      (node (ref C262) (pin 1))
      (node (ref C261) (pin 1))
      (node (ref U13) (pin 5))
      (node (ref C260) (pin 1))
      (node (ref J9) (pin K18))
      (node (ref J9) (pin K15))
      (node (ref R1) (pin 1))
      (node (ref J9) (pin K2))
      (node (ref J9) (pin J40))
      (node (ref U49) (pin 4))
      (node (ref U49) (pin 3))
      (node (ref J9) (pin J38))
      (node (ref J9) (pin J8))
      (node (ref J9) (pin J5))
      (node (ref J9) (pin J4))
      (node (ref J9) (pin J35))
      (node (ref J9) (pin J32))
      (node (ref J9) (pin K3))
      (node (ref J9) (pin K12))
      (node (ref J9) (pin K27))
      (node (ref J9) (pin K24))
      (node (ref J9) (pin K21)))
    (net (code 69) (name VDD_DDR_SOC_N)
      (node (ref J14) (pin 4))
      (node (ref RS2) (pin 3)))
    (net (code 70) (name VDD_DDR_SOC_P)
      (node (ref J14) (pin 3))
      (node (ref RS2) (pin 2)))
    (net (code 71) (name DDR_DQS3_N)
      (node (ref U1) (pin D7))
      (node (ref U5) (pin B3)))
    (net (code 72) (name DDR_DQS3_P)
      (node (ref U5) (pin C3))
      (node (ref U1) (pin E7)))
    (net (code 73) (name DDR_DM3)
      (node (ref U5) (pin A7))
      (node (ref U1) (pin D5)))
    (net (code 74) (name DDR_DQS2_N)
      (node (ref U1) (pin A7))
      (node (ref U4) (pin B3)))
    (net (code 75) (name DDR_DQS4_N)
      (node (ref U1) (pin U4))
      (node (ref U6) (pin B3)))
    (net (code 76) (name DDR_DQS4_P)
      (node (ref U1) (pin V4))
      (node (ref U6) (pin C3)))
    (net (code 77) (name DDR_DM4)
      (node (ref U1) (pin T5))
      (node (ref U6) (pin A7)))
    (net (code 78) (name DDR_DQS2_P)
      (node (ref U1) (pin A6))
      (node (ref U4) (pin C3)))
    (net (code 79) (name DDR_DQS0_N)
      (node (ref U1) (pin F3))
      (node (ref U2) (pin B3)))
    (net (code 80) (name DDR_DQS0_P)
      (node (ref U1) (pin F2))
      (node (ref U2) (pin C3)))
    (net (code 81) (name DDR_DM0)
      (node (ref U2) (pin A7))
      (node (ref U1) (pin E5)))
    (net (code 82) (name DDR_DM2)
      (node (ref U1) (pin C6))
      (node (ref U4) (pin A7)))
    (net (code 83) (name DDR_DQS1_N)
      (node (ref U3) (pin B3))
      (node (ref U1) (pin H3)))
    (net (code 84) (name DDR_DQS1_P)
      (node (ref U3) (pin C3))
      (node (ref U1) (pin H2)))
    (net (code 85) (name DDR_DM1)
      (node (ref U1) (pin G5))
      (node (ref U3) (pin A7)))
    (net (code 86) (name DDR_DQS7_N)
      (node (ref U9) (pin B3))
      (node (ref U1) (pin Y8)))
    (net (code 87) (name DDR_DQS7_P)
      (node (ref U1) (pin AA8))
      (node (ref U9) (pin C3)))
    (net (code 88) (name DDR_DM7)
      (node (ref U1) (pin AB12))
      (node (ref U9) (pin A7)))
    (net (code 89) (name DDR_ECC_DM)
      (node (ref U10) (pin A7))
      (node (ref U1) (pin J5)))
    (net (code 90) (name DDR_ECC_DQS_N)
      (node (ref U10) (pin B3))
      (node (ref U1) (pin K3)))
    (net (code 91) (name DDR_ECC_DQS_P)
      (node (ref U1) (pin K2))
      (node (ref U10) (pin C3)))
    (net (code 92) (name DDR_DQS5_P)
      (node (ref U1) (pin Y4))
      (node (ref U7) (pin C3)))
    (net (code 93) (name DDR_DQS5_N)
      (node (ref U1) (pin W4))
      (node (ref U7) (pin B3)))
    (net (code 94) (name DDR_DM5)
      (node (ref U7) (pin A7))
      (node (ref U1) (pin W5)))
    (net (code 95) (name DDR_DQS6_N)
      (node (ref U1) (pin AA7))
      (node (ref U8) (pin B3)))
    (net (code 96) (name DDR_DQS6_P)
      (node (ref U8) (pin C3))
      (node (ref U1) (pin Y7)))
    (net (code 97) (name DDR_DM6)
      (node (ref U8) (pin A7))
      (node (ref U1) (pin W10)))
    (net (code 98) (name CHIPLINK_TX_CLK)
      (node (ref R148) (pin 1))
      (node (ref J9) (pin H4)))
    (net (code 99) (name CHIPLINK_TX_SEND)
      (node (ref J9) (pin G18))
      (node (ref R149) (pin 1)))
    (net (code 100) (name CHIPLINK_TX_RST)
      (node (ref J9) (pin G19))
      (node (ref R150) (pin 1)))
    (net (code 101) (name GEMGXL_RXD3)
      (node (ref U1) (pin E11))
      (node (ref R82) (pin 7)))
    (net (code 102) (name GEMGXL_RX_COL)
      (node (ref R85) (pin 5))
      (node (ref U1) (pin A13)))
    (net (code 103) (name GEMGXL_RX_CRS)
      (node (ref U1) (pin C13))
      (node (ref R85) (pin 6)))
    (net (code 104) (name GEMGXL_RX_ER)
      (node (ref U1) (pin B11))
      (node (ref R80) (pin 8)))
    (net (code 105) (name GEMGXL_RX_DV)
      (node (ref R80) (pin 7))
      (node (ref U1) (pin A11)))
    (net (code 106) (name GEMGXL_RXD7)
      (node (ref R85) (pin 7))
      (node (ref U1) (pin E9)))
    (net (code 107) (name GEMGXL_RXD6)
      (node (ref U1) (pin C9))
      (node (ref R85) (pin 8)))
    (net (code 108) (name GEMGXL_RXD5)
      (node (ref U1) (pin A8))
      (node (ref R82) (pin 5)))
    (net (code 109) (name GEMGXL_RXD4)
      (node (ref U1) (pin E10))
      (node (ref R82) (pin 6)))
    (net (code 110) (name GEMGXL_RXD2)
      (node (ref U1) (pin A10))
      (node (ref R82) (pin 8)))
    (net (code 111) (name GEMGXL_RXD1)
      (node (ref R80) (pin 5))
      (node (ref U1) (pin B10)))
    (net (code 112) (name GEMGXL_RXD0)
      (node (ref U1) (pin A12))
      (node (ref R80) (pin 6)))
    (net (code 113) (name GEMGXL_RX_CLK)
      (node (ref U1) (pin F12))
      (node (ref R79) (pin 2)))
    (net (code 114) (name GEMGXL_GTX_CLK)
      (node (ref R97) (pin 1))
      (node (ref IC1) (pin 37))
      (node (ref U1) (pin E12)))
    (net (code 115) (name GEMGXL_TX_CLK)
      (node (ref U1) (pin C8))
      (node (ref R91) (pin 2)))
    (net (code 116) (name GEMGXL_TXD6)
      (node (ref IC1) (pin 46))
      (node (ref R76) (pin 3)))
    (net (code 117) (name GEMGXL_TXD5)
      (node (ref R76) (pin 2))
      (node (ref IC1) (pin 45)))
    (net (code 118) (name GEMGXL_TXD4)
      (node (ref IC1) (pin 43))
      (node (ref R76) (pin 1)))
    (net (code 119) (name GEMGXL_TXD3)
      (node (ref R75) (pin 4))
      (node (ref IC1) (pin 42)))
    (net (code 120) (name GEMGXL_TXD2)
      (node (ref IC1) (pin 41))
      (node (ref R75) (pin 3)))
    (net (code 121) (name GEMGXL_TXD1)
      (node (ref IC1) (pin 40))
      (node (ref R75) (pin 2)))
    (net (code 122) (name GEMGXL_TXD0)
      (node (ref R75) (pin 1))
      (node (ref IC1) (pin 38)))
    (net (code 123) (name GEMGXL_TX_EN)
      (node (ref R77) (pin 2))
      (node (ref IC1) (pin 33)))
    (net (code 124) (name GEMGXL_TXD7)
      (node (ref IC1) (pin 47))
      (node (ref R76) (pin 4)))
    (net (code 125) (name /Freedom-U540_1/IO_DDR_RSVD3)
      (node (ref J18) (pin 1))
      (node (ref U1) (pin F9)))
    (net (code 126) (name /Freedom-U540_1/IO_DDR_RSVD1)
      (node (ref U1) (pin D8))
      (node (ref J16) (pin 1)))
    (net (code 127) (name /Freedom-U540_1/IO_DDR_RSVD2)
      (node (ref J17) (pin 1))
      (node (ref U1) (pin F8)))
    (net (code 128) (name GEMGXL_TX_ER)
      (node (ref IC1) (pin 35))
      (node (ref R78) (pin 2)))
    (net (code 129) (name /Freedom-U540_1/IO_DDR_RSVD0)
      (node (ref U1) (pin E8))
      (node (ref J15) (pin 1)))
    (net (code 130) (name /Freedom-U540_2/QSPI1_DQ1)
      (node (ref U1) (pin J18))
      (node (ref R158) (pin 1)))
    (net (code 131) (name /Freedom-U540_2/QSPI1_CS3)
      (node (ref R158) (pin 2))
      (node (ref U1) (pin J20)))
    (net (code 132) (name /Freedom-U540_2/QSPI1_CS2)
      (node (ref U1) (pin H19))
      (node (ref R159) (pin 4)))
    (net (code 133) (name /Freedom-U540_2/QSPI1_CS0)
      (node (ref U1) (pin K17))
      (node (ref R158) (pin 4)))
    (net (code 134) (name /Freedom-U540_2/QSPI1_DQ1_R)
      (node (ref J1) (pin 32))
      (node (ref R158) (pin 8)))
    (net (code 135) (name /Freedom-U540_2/QSPI1_CS3_R)
      (node (ref R158) (pin 7))
      (node (ref J2) (pin 13)))
    (net (code 136) (name /Freedom-U540_2/QSPI1_DQ3_R)
      (node (ref R158) (pin 6))
      (node (ref J2) (pin 7)))
    (net (code 137) (name /Freedom-U540_2/QSPI1_CS0_R)
      (node (ref J1) (pin 30))
      (node (ref R158) (pin 5)))
    (net (code 138) (name /Freedom-U540_2/QSPI1_CS1)
      (node (ref R159) (pin 1))
      (node (ref U1) (pin G21)))
    (net (code 139) (name /Freedom-U540_2/QSPI1_SCK)
      (node (ref R159) (pin 2))
      (node (ref U1) (pin H18)))
    (net (code 140) (name /Freedom-U540_2/QSPI1_DQ0)
      (node (ref U1) (pin G22))
      (node (ref R159) (pin 3)))
    (net (code 141) (name /Freedom-U540_2/QSPI1_DQ3)
      (node (ref R158) (pin 3))
      (node (ref U1) (pin J17)))
    (net (code 142) (name /Freedom-U540_2/QSPI1_CS1_R)
      (node (ref J2) (pin 9))
      (node (ref R159) (pin 8)))
    (net (code 143) (name /Freedom-U540_2/QSPI1_SCK_R)
      (node (ref R159) (pin 7))
      (node (ref J1) (pin 34)))
    (net (code 144) (name /Freedom-U540_2/QSPI1_DQ0_R)
      (node (ref R159) (pin 6))
      (node (ref J1) (pin 28)))
    (net (code 145) (name /Freedom-U540_2/QSPI1_CS2_R)
      (node (ref J2) (pin 11))
      (node (ref R159) (pin 5)))
    (net (code 146) (name "Net-(D1-Pad2)")
      (node (ref R16) (pin 2))
      (node (ref D1) (pin 2)))
    (net (code 147) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R17) (pin 2)))
    (net (code 148) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R18) (pin 2)))
    (net (code 149) (name "Net-(D4-Pad2)")
      (node (ref D4) (pin 2))
      (node (ref R19) (pin 2)))
    (net (code 150) (name "Net-(R183-Pad2)")
      (node (ref R183) (pin 2))
      (node (ref U1) (pin B15)))
    (net (code 151) (name "Net-(R20-Pad2)")
      (node (ref X1) (pin 1))
      (node (ref R20) (pin 2)))
    (net (code 152) (name /Freedom-U540_2/PWM0_2)
      (node (ref U1) (pin F20))
      (node (ref Q2) (pin 2))
      (node (ref J2) (pin 1)))
    (net (code 153) (name GEMGXL_RST)
      (node (ref U1) (pin B21))
      (node (ref J2) (pin 6))
      (node (ref U37) (pin 2))
      (node (ref R116) (pin 2)))
    (net (code 154) (name FASTLINK_FAIL)
      (node (ref U1) (pin E19))
      (node (ref J2) (pin 8))
      (node (ref U38) (pin 4)))
    (net (code 155) (name /Freedom-U540_2/SD_CD)
      (node (ref J10) (pin 9))
      (node (ref J2) (pin 12))
      (node (ref D10) (pin 2))
      (node (ref R72) (pin 1))
      (node (ref U1) (pin B20)))
    (net (code 156) (name /Freedom-U540_2/PWM0_3)
      (node (ref Q2) (pin 5))
      (node (ref J2) (pin 3))
      (node (ref U1) (pin G20)))
    (net (code 157) (name /Freedom-U540_2/QSPI1_DQ2_R)
      (node (ref J2) (pin 5))
      (node (ref R160) (pin 1)))
    (net (code 158) (name "Net-(J2-Pad14)")
      (node (ref J2) (pin 14)))
    (net (code 159) (name "Net-(J11-Pad8)")
      (node (ref J11) (pin 8)))
    (net (code 160) (name "Net-(J11-Pad7)")
      (node (ref J11) (pin 7)))
    (net (code 161) (name +3V3)
      (node (ref C156) (pin 1))
      (node (ref C165) (pin 1))
      (node (ref C162) (pin 1))
      (node (ref C154) (pin 1))
      (node (ref Q6) (pin 2))
      (node (ref C158) (pin 1))
      (node (ref R38) (pin 2))
      (node (ref U20) (pin 5))
      (node (ref C160) (pin 1))
      (node (ref U21) (pin 5))
      (node (ref R36) (pin 2))
      (node (ref C121) (pin 2))
      (node (ref R17) (pin 1))
      (node (ref U23) (pin 5))
      (node (ref L2) (pin 2))
      (node (ref U24) (pin 5))
      (node (ref R73) (pin 1))
      (node (ref U14) (pin 5))
      (node (ref U25) (pin 5))
      (node (ref U22) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref R161) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref U17) (pin 1))
      (node (ref C144) (pin 1))
      (node (ref C110) (pin 2))
      (node (ref U13) (pin 31))
      (node (ref U13) (pin 20))
      (node (ref U13) (pin 42))
      (node (ref C102) (pin 2))
      (node (ref U11) (pin 10))
      (node (ref U31) (pin 1))
      (node (ref R74) (pin 2))
      (node (ref C104) (pin 2))
      (node (ref U28) (pin 1))
      (node (ref C167) (pin 2))
      (node (ref R23) (pin 1))
      (node (ref C169) (pin 2))
      (node (ref U29) (pin 5))
      (node (ref FB2) (pin 2))
      (node (ref C171) (pin 2))
      (node (ref C173) (pin 2))
      (node (ref C177) (pin 2))
      (node (ref C175) (pin 2))
      (node (ref U30) (pin 1))
      (node (ref C70) (pin 2))
      (node (ref U33) (pin 1))
      (node (ref U32) (pin 5))
      (node (ref U11) (pin 7))
      (node (ref FB1) (pin 2))
      (node (ref C242) (pin 2))
      (node (ref C103) (pin 2))
      (node (ref U35) (pin 3))
      (node (ref U13) (pin 56))
      (node (ref U35) (pin 1))
      (node (ref C209) (pin 2))
      (node (ref U13) (pin 50)))
    (net (code 162) (name "Net-(R65-Pad2)")
      (node (ref U12) (pin 3))
      (node (ref R65) (pin 2)))
    (net (code 163) (name "Net-(R44-Pad1)")
      (node (ref X2) (pin 1))
      (node (ref R44) (pin 1)))
    (net (code 164) (name VDD)
      (node (ref U1) (pin V21))
      (node (ref U1) (pin P2))
      (node (ref U1) (pin V14))
      (node (ref U1) (pin N9))
      (node (ref U1) (pin P10))
      (node (ref U1) (pin M14))
      (node (ref U1) (pin P12))
      (node (ref U1) (pin P14))
      (node (ref U1) (pin P16))
      (node (ref U1) (pin H16))
      (node (ref U1) (pin P21))
      (node (ref U1) (pin P8))
      (node (ref U1) (pin V6))
      (node (ref U1) (pin L13))
      (node (ref U1) (pin M10))
      (node (ref U1) (pin H14))
      (node (ref U1) (pin M12))
      (node (ref U1) (pin V8))
      (node (ref U1) (pin H12))
      (node (ref U1) (pin H10))
      (node (ref U1) (pin G9))
      (node (ref U1) (pin J9))
      (node (ref U1) (pin J15))
      (node (ref U1) (pin H8))
      (node (ref U1) (pin K10))
      (node (ref U1) (pin K21))
      (node (ref U1) (pin U11))
      (node (ref U1) (pin K8))
      (node (ref U1) (pin L11))
      (node (ref U1) (pin G11))
      (node (ref U1) (pin G15))
      (node (ref U1) (pin E3))
      (node (ref U1) (pin T8))
      (node (ref U1) (pin N13))
      (node (ref U1) (pin N11))
      (node (ref U1) (pin T14))
      (node (ref U1) (pin V10))
      (node (ref U1) (pin V12))
      (node (ref U1) (pin T10))
      (node (ref U1) (pin R13))
      (node (ref U1) (pin R15))
      (node (ref U1) (pin R9))
      (node (ref U1) (pin T12))
      (node (ref U1) (pin T16))
      (node (ref U1) (pin U9))
      (node (ref U1) (pin U15))
      (node (ref U1) (pin U13))
      (node (ref U1) (pin AA17))
      (node (ref U1) (pin B14))
      (node (ref U1) (pin B18))
      (node (ref U1) (pin B9))
      (node (ref U1) (pin E21))
      (node (ref U1) (pin M8))
      (node (ref U1) (pin R11))
      (node (ref C250) (pin 1))
      (node (ref C251) (pin 1))
      (node (ref C252) (pin 1))
      (node (ref C249) (pin 1))
      (node (ref C253) (pin 1))
      (node (ref C254) (pin 1))
      (node (ref C255) (pin 1))
      (node (ref C256) (pin 1))
      (node (ref C243) (pin 1))
      (node (ref C244) (pin 1))
      (node (ref C257) (pin 1))
      (node (ref C245) (pin 1))
      (node (ref C246) (pin 1))
      (node (ref C247) (pin 1))
      (node (ref C248) (pin 1))
      (node (ref C258) (pin 1))
      (node (ref RS10) (pin 1))
      (node (ref U18) (pin 22)))
    (net (code 165) (name "Net-(S3-Pad6)")
      (node (ref S3) (pin 6)))
    (net (code 166) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref Q2) (pin 6)))
    (net (code 167) (name /Freedom-U540_2/PWM0_1)
      (node (ref J2) (pin 4))
      (node (ref Q1) (pin 5))
      (node (ref U1) (pin F21)))
    (net (code 168) (name "Net-(C137-Pad2)")
      (node (ref C137) (pin 2))
      (node (ref Y1) (pin 1))
      (node (ref R183) (pin 1))
      (node (ref R182) (pin 2)))
    (net (code 169) (name "Net-(C138-Pad2)")
      (node (ref U1) (pin A15))
      (node (ref R182) (pin 1))
      (node (ref Y1) (pin 3))
      (node (ref C138) (pin 2)))
    (net (code 170) (name "Net-(D4-Pad1)")
      (node (ref D4) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 171) (name /Freedom-U540_2/PWM0_0)
      (node (ref Q1) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref U1) (pin G19)))
    (net (code 172) (name "Net-(D1-Pad1)")
      (node (ref Q1) (pin 6))
      (node (ref D1) (pin 1)))
    (net (code 173) (name "Net-(D2-Pad1)")
      (node (ref Q1) (pin 3))
      (node (ref D2) (pin 1)))
    (net (code 174) (name "Net-(J1-Pad22)")
      (node (ref J1) (pin 22)))
    (net (code 175) (name +3.3VA)
      (node (ref J10) (pin 4))
      (node (ref Q6) (pin 3))
      (node (ref C163) (pin 2)))
    (net (code 176) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 177) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 178) (name "Net-(J1-Pad21)")
      (node (ref J1) (pin 21)))
    (net (code 179) (name "Net-(J1-Pad19)")
      (node (ref J1) (pin 19)))
    (net (code 180) (name "Net-(J1-Pad26)")
      (node (ref J1) (pin 26)))
    (net (code 181) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24)))
    (net (code 182) (name "Net-(J1-Pad20)")
      (node (ref J1) (pin 20)))
    (net (code 183) (name "Net-(J1-Pad8)")
      (node (ref J1) (pin 8)))
    (net (code 184) (name /Freedom-U540_2/QSPI0_DQ1)
      (node (ref U12) (pin 8))
      (node (ref U1) (pin H22)))
    (net (code 185) (name /Freedom-U540_2/QSPI0_SCK)
      (node (ref U12) (pin 16))
      (node (ref U1) (pin K18)))
    (net (code 186) (name /Freedom-U540_2/QSPI0_CS)
      (node (ref U1) (pin J19))
      (node (ref R15) (pin 2))
      (node (ref U12) (pin 7)))
    (net (code 187) (name VDD_COREPLL_N)
      (node (ref U1) (pin K14))
      (node (ref C207) (pin 2))
      (node (ref J14) (pin 8))
      (node (ref RS9) (pin 2)))
    (net (code 188) (name VDD_SOC_CORE_P)
      (node (ref RS10) (pin 3))
      (node (ref J14) (pin 1)))
    (net (code 189) (name AVDD_DDRPLL_P)
      (node (ref C145) (pin 1))
      (node (ref U17) (pin 5))
      (node (ref RS4) (pin 1))
      (node (ref RS6) (pin 2))
      (node (ref J14) (pin 19))
      (node (ref J14) (pin 7))
      (node (ref RS9) (pin 1))
      (node (ref J14) (pin 15)))
    (net (code 190) (name VDD_OTP_N)
      (node (ref C206) (pin 2))
      (node (ref J14) (pin 10))
      (node (ref RS8) (pin 1))
      (node (ref U1) (pin G14)))
    (net (code 191) (name VDD_DDR_MEM_N)
      (node (ref J14) (pin 6))
      (node (ref RS1) (pin 2)))
    (net (code 192) (name VDD_DDR_MEM_P)
      (node (ref RS1) (pin 3))
      (node (ref J14) (pin 5)))
    (net (code 193) (name VDD_GIVDD_P)
      (node (ref R99) (pin 1))
      (node (ref R100) (pin 1))
      (node (ref R101) (pin 1))
      (node (ref C170) (pin 2))
      (node (ref RS7) (pin 2))
      (node (ref R98) (pin 1))
      (node (ref R111) (pin 1))
      (node (ref R46) (pin 1))
      (node (ref C172) (pin 2))
      (node (ref U29) (pin 1))
      (node (ref C155) (pin 1))
      (node (ref C157) (pin 1))
      (node (ref C159) (pin 1))
      (node (ref C161) (pin 1))
      (node (ref C176) (pin 2))
      (node (ref R47) (pin 1))
      (node (ref C174) (pin 2))
      (node (ref R110) (pin 1))
      (node (ref R44) (pin 2))
      (node (ref C166) (pin 2))
      (node (ref X2) (pin 4))
      (node (ref R102) (pin 1))
      (node (ref C135) (pin 2))
      (node (ref R108) (pin 1))
      (node (ref C192) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref C187) (pin 2))
      (node (ref C188) (pin 1))
      (node (ref C191) (pin 1))
      (node (ref C189) (pin 1))
      (node (ref R45) (pin 2))
      (node (ref U28) (pin 5))
      (node (ref IC1) (pin 28))
      (node (ref R52) (pin 1))
      (node (ref R106) (pin 1))
      (node (ref R48) (pin 1))
      (node (ref R49) (pin 1))
      (node (ref R50) (pin 1))
      (node (ref R109) (pin 1))
      (node (ref U32) (pin 1))
      (node (ref R51) (pin 1))
      (node (ref U31) (pin 5))
      (node (ref R107) (pin 1))
      (node (ref R25) (pin 1))
      (node (ref R40) (pin 2))
      (node (ref R21) (pin 1))
      (node (ref U15) (pin 5))
      (node (ref R22) (pin 1))
      (node (ref C124) (pin 2))
      (node (ref R105) (pin 1))
      (node (ref R104) (pin 1))
      (node (ref R103) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R162) (pin 1))
      (node (ref C134) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref J11) (pin 4))
      (node (ref U33) (pin 5))
      (node (ref R20) (pin 1))
      (node (ref C136) (pin 2))
      (node (ref X1) (pin 4))
      (node (ref R12) (pin 2))
      (node (ref C153) (pin 1))
      (node (ref U22) (pin 5))
      (node (ref U25) (pin 1))
      (node (ref U24) (pin 1))
      (node (ref L3) (pin 2))
      (node (ref R72) (pin 2))
      (node (ref C164) (pin 1))
      (node (ref U23) (pin 1))
      (node (ref U21) (pin 1))
      (node (ref U20) (pin 1))
      (node (ref R37) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref U36) (pin 6))
      (node (ref U36) (pin 3))
      (node (ref C190) (pin 1))
      (node (ref U30) (pin 5))
      (node (ref C217) (pin 1))
      (node (ref C215) (pin 1))
      (node (ref Q4) (pin 2))
      (node (ref R114) (pin 1))
      (node (ref U38) (pin 5))
      (node (ref U37) (pin 1))
      (node (ref R113) (pin 2))
      (node (ref IC1) (pin 22))
      (node (ref R115) (pin 1))
      (node (ref C212) (pin 2))
      (node (ref J9) (pin H1))
      (node (ref J1) (pin 5))
      (node (ref J14) (pin 9))
      (node (ref J14) (pin 17))
      (node (ref U12) (pin 2))
      (node (ref IC1) (pin 49))
      (node (ref J14) (pin 11))
      (node (ref IC1) (pin 39))
      (node (ref IC1) (pin 44))
      (node (ref RS5) (pin 1))
      (node (ref D13) (pin 1))
      (node (ref RS8) (pin 2))
      (node (ref C168) (pin 2)))
    (net (code 194) (name VDD_IO_N)
      (node (ref C130) (pin 1))
      (node (ref U1) (pin L16))
      (node (ref U1) (pin M16))
      (node (ref U1) (pin N16))
      (node (ref C133) (pin 1))
      (node (ref C132) (pin 1))
      (node (ref U1) (pin K16))
      (node (ref J14) (pin 12))
      (node (ref C131) (pin 1))
      (node (ref RS7) (pin 1)))
    (net (code 195) (name "Net-(U12-Pad11)")
      (node (ref U12) (pin 11)))
    (net (code 196) (name "Net-(U12-Pad12)")
      (node (ref U12) (pin 12)))
    (net (code 197) (name "Net-(U12-Pad13)")
      (node (ref U12) (pin 13)))
    (net (code 198) (name "Net-(U12-Pad14)")
      (node (ref U12) (pin 14)))
    (net (code 199) (name "Net-(U12-Pad4)")
      (node (ref U12) (pin 4)))
    (net (code 200) (name "Net-(U12-Pad5)")
      (node (ref U12) (pin 5)))
    (net (code 201) (name "Net-(U12-Pad6)")
      (node (ref U12) (pin 6)))
    (net (code 202) (name /Freedom-U540_2/MSEL0)
      (node (ref R21) (pin 2))
      (node (ref U1) (pin A19))
      (node (ref R27) (pin 1))
      (node (ref S1) (pin 3)))
    (net (code 203) (name +5V)
      (node (ref U36) (pin 4))
      (node (ref C214) (pin 1))
      (node (ref C120) (pin 2))
      (node (ref J1) (pin 3))
      (node (ref C139) (pin 2))
      (node (ref U16) (pin 10))
      (node (ref U50) (pin 8))
      (node (ref C218) (pin 2))
      (node (ref C116) (pin 2))
      (node (ref U14) (pin 8))
      (node (ref U18) (pin 18))
      (node (ref R42) (pin 2))
      (node (ref U16) (pin 11))
      (node (ref R67) (pin 2))
      (node (ref U18) (pin 20))
      (node (ref L1) (pin 2))
      (node (ref R62) (pin 2))
      (node (ref C151) (pin 1))
      (node (ref C122) (pin 2))
      (node (ref C147) (pin 2))
      (node (ref U27) (pin 14))
      (node (ref R35) (pin 2))
      (node (ref U15) (pin 8))
      (node (ref U19) (pin 1))
      (node (ref U16) (pin 12))
      (node (ref U16) (pin 3)))
    (net (code 204) (name +12V)
      (node (ref C219) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref U27) (pin 13))
      (node (ref U18) (pin 15))
      (node (ref U18) (pin 16))
      (node (ref U18) (pin 17))
      (node (ref U27) (pin 10))
      (node (ref D8) (pin 1))
      (node (ref U27) (pin 11))
      (node (ref U27) (pin 12))
      (node (ref C118) (pin 2))
      (node (ref C149) (pin 2))
      (node (ref J1) (pin 6))
      (node (ref R174) (pin 2))
      (node (ref R173) (pin 2))
      (node (ref C117) (pin 2))
      (node (ref D7) (pin 1))
      (node (ref J19) (pin 2)))
    (net (code 205) (name VDD_SOC_CORE_N)
      (node (ref RS10) (pin 2))
      (node (ref J14) (pin 2)))
    (net (code 206) (name /Freedom-U540_2/EN_VDD_SD)
      (node (ref J2) (pin 10))
      (node (ref Q4) (pin 5))
      (node (ref U1) (pin B22))
      (node (ref R162) (pin 2)))
    (net (code 207) (name /Freedom-U540_2/GPIO15)
      (node (ref U1) (pin G17))
      (node (ref J1) (pin 7)))
    (net (code 208) (name RESET_N)
      (node (ref Q4) (pin 1))
      (node (ref R186) (pin 2))
      (node (ref D13) (pin 2))
      (node (ref R175) (pin 2))
      (node (ref R65) (pin 1))
      (node (ref C241) (pin 1))
      (node (ref R45) (pin 1))
      (node (ref D11) (pin 2))
      (node (ref J11) (pin 6))
      (node (ref J1) (pin 36))
      (node (ref U1) (pin C17))
      (node (ref S2) (pin 2)))
    (net (code 209) (name /Freedom-U540_2/QSPI0_DQ2)
      (node (ref U1) (pin J21))
      (node (ref U12) (pin 9)))
    (net (code 210) (name /Freedom-U540_2/QSPI0_DQ3)
      (node (ref U1) (pin H20))
      (node (ref U12) (pin 1)))
    (net (code 211) (name /Freedom-U540_2/HFXCLKIN)
      (node (ref U1) (pin F15))
      (node (ref X1) (pin 3)))
    (net (code 212) (name /Freedom-U540_2/QSPI0_DQ0)
      (node (ref U1) (pin H21))
      (node (ref U12) (pin 15)))
    (net (code 213) (name JTAG_TCK)
      (node (ref U1) (pin D18))
      (node (ref R26) (pin 1))
      (node (ref J11) (pin 1)))
    (net (code 214) (name JTAG_TDI)
      (node (ref R31) (pin 1))
      (node (ref J11) (pin 9))
      (node (ref U1) (pin C19)))
    (net (code 215) (name UART0_TX)
      (node (ref U29) (pin 2))
      (node (ref J1) (pin 35))
      (node (ref U1) (pin Y13)))
    (net (code 216) (name /Freedom-U540_2/UART1_TX)
      (node (ref J1) (pin 29))
      (node (ref U1) (pin AA15)))
    (net (code 217) (name /Freedom-U540_2/UART1_RX)
      (node (ref U1) (pin AA14))
      (node (ref J1) (pin 27)))
    (net (code 218) (name UART0_RX)
      (node (ref U1) (pin W14))
      (node (ref J1) (pin 33))
      (node (ref R34) (pin 1)))
    (net (code 219) (name /Freedom-U540_2/IO_PRCI_RSVD11)
      (node (ref R51) (pin 2))
      (node (ref S3) (pin 5))
      (node (ref R58) (pin 1))
      (node (ref U1) (pin D14)))
    (net (code 220) (name /Freedom-U540_2/IO_PRCI_RSVD12)
      (node (ref R57) (pin 1))
      (node (ref R50) (pin 2))
      (node (ref S3) (pin 4))
      (node (ref U1) (pin E14)))
    (net (code 221) (name /Freedom-U540_2/IO_PRCI_RSVD10)
      (node (ref R56) (pin 1))
      (node (ref S3) (pin 3))
      (node (ref U1) (pin D17))
      (node (ref R49) (pin 2)))
    (net (code 222) (name /Freedom-U540_2/IO_PRCI_RSVD0)
      (node (ref U1) (pin A16))
      (node (ref S3) (pin 1))
      (node (ref R46) (pin 2))
      (node (ref R53) (pin 1)))
    (net (code 223) (name /Freedom-U540_2/IO_PRCI_RSVD1)
      (node (ref S3) (pin 2))
      (node (ref R48) (pin 2))
      (node (ref R55) (pin 1))
      (node (ref U1) (pin D13)))
    (net (code 224) (name /Freedom-U540_2/RTCXSEL)
      (node (ref U1) (pin D15))
      (node (ref S1) (pin 2))
      (node (ref R47) (pin 2))
      (node (ref R54) (pin 1)))
    (net (code 225) (name /Freedom-U540_2/HFXSEL)
      (node (ref U1) (pin C15))
      (node (ref R59) (pin 1))
      (node (ref R52) (pin 2))
      (node (ref S1) (pin 1)))
    (net (code 226) (name JTAG_TMS)
      (node (ref J11) (pin 5))
      (node (ref R32) (pin 1))
      (node (ref U1) (pin F16)))
    (net (code 227) (name JTAG_TDO)
      (node (ref U1) (pin E17))
      (node (ref U32) (pin 2))
      (node (ref J11) (pin 3)))
    (net (code 228) (name /Freedom-U540_2/IO_PRCI_RSVD13)
      (node (ref U1) (pin F14))
      (node (ref J4) (pin 1)))
    (net (code 229) (name /Freedom-U540_2/IO_PRCI_RSVD14)
      (node (ref J5) (pin 1))
      (node (ref U1) (pin F13)))
    (net (code 230) (name /Freedom-U540_2/IO_PRCI_RSVD15)
      (node (ref J6) (pin 1))
      (node (ref U1) (pin C14)))
    (net (code 231) (name /Freedom-U540_2/IO_PRCI_RSVD2)
      (node (ref U1) (pin E13))
      (node (ref J3) (pin 1)))
    (net (code 232) (name /Freedom-U540_2/MSEL1)
      (node (ref S1) (pin 4))
      (node (ref U1) (pin C18))
      (node (ref R28) (pin 1))
      (node (ref R22) (pin 2)))
    (net (code 233) (name /Freedom-U540_2/MSEL2)
      (node (ref R29) (pin 1))
      (node (ref R24) (pin 2))
      (node (ref S1) (pin 5))
      (node (ref U1) (pin A20)))
    (net (code 234) (name /Freedom-U540_2/GPIO7)
      (node (ref U1) (pin C20))
      (node (ref J1) (pin 12)))
    (net (code 235) (name /Freedom-U540_2/I2C0_SDA)
      (node (ref R13) (pin 2))
      (node (ref U1) (pin W13))
      (node (ref J1) (pin 23)))
    (net (code 236) (name /Freedom-U540_2/GPIO0)
      (node (ref U1) (pin F17))
      (node (ref J1) (pin 17)))
    (net (code 237) (name /Freedom-U540_2/GPIO1)
      (node (ref U1) (pin C22))
      (node (ref J1) (pin 18)))
    (net (code 238) (name /Freedom-U540_2/GPIO2)
      (node (ref U1) (pin C21))
      (node (ref J1) (pin 15)))
    (net (code 239) (name /Freedom-U540_2/GPIO3)
      (node (ref U1) (pin D21))
      (node (ref J1) (pin 16)))
    (net (code 240) (name /Freedom-U540_2/GPIO4)
      (node (ref U1) (pin E18))
      (node (ref J1) (pin 13)))
    (net (code 241) (name /Freedom-U540_2/GPIO5)
      (node (ref U1) (pin D20))
      (node (ref J1) (pin 14)))
    (net (code 242) (name /Freedom-U540_2/GPIO6)
      (node (ref U1) (pin E20))
      (node (ref J1) (pin 11)))
    (net (code 243) (name /Freedom-U540_2/I2C0_SCL)
      (node (ref J1) (pin 25))
      (node (ref R14) (pin 2))
      (node (ref U1) (pin Y14)))
    (net (code 244) (name /Freedom-U540_2/GPIO8)
      (node (ref U1) (pin D19))
      (node (ref J1) (pin 9)))
    (net (code 245) (name /Freedom-U540_2/GPIO9)
      (node (ref J1) (pin 10))
      (node (ref U1) (pin A21)))
    (net (code 246) (name /Freedom-U540_2/GPIO10)
      (node (ref R186) (pin 1))
      (node (ref U1) (pin F18)))
    (net (code 247) (name /Freedom-U540_2/QSPI2_MISO)
      (node (ref R142) (pin 2))
      (node (ref U1) (pin AB15)))
    (net (code 248) (name /Freedom-U540_2/PWM1_0)
      (node (ref U1) (pin D22))
      (node (ref J2) (pin 16)))
    (net (code 249) (name /Freedom-U540_2/PWM1_1)
      (node (ref U1) (pin H17))
      (node (ref J2) (pin 18)))
    (net (code 250) (name /Freedom-U540_2/PWM1_2)
      (node (ref J2) (pin 17))
      (node (ref U1) (pin G18)))
    (net (code 251) (name /Freedom-U540_2/PWM1_3)
      (node (ref J2) (pin 19))
      (node (ref U1) (pin F19)))
    (net (code 252) (name /Freedom-U540_2/QSPI2_SCK)
      (node (ref U1) (pin W15))
      (node (ref R139) (pin 2)))
    (net (code 253) (name /Freedom-U540_2/QSPI2_MOSI)
      (node (ref R141) (pin 2))
      (node (ref U1) (pin AA16)))
    (net (code 254) (name /Freedom-U540_2/QSPI2_WP)
      (node (ref U1) (pin AB16))
      (node (ref R143) (pin 2)))
    (net (code 255) (name /Freedom-U540_2/QSPI2_HOLD)
      (node (ref R140) (pin 2))
      (node (ref U1) (pin Y15)))
    (net (code 256) (name /Freedom-U540_2/QSPI2_CS)
      (node (ref R144) (pin 2))
      (node (ref U1) (pin AB14)))
    (net (code 257) (name /Freedom-U540_2/QSPI2_MOSI_3V3)
      (node (ref U21) (pin 4))
      (node (ref U26) (pin 3)))
    (net (code 258) (name /Freedom-U540_2/QSPI2_CS_CON)
      (node (ref J10) (pin 2))
      (node (ref U26) (pin 11)))
    (net (code 259) (name /Freedom-U540_2/QSPI2_MOSI_CON)
      (node (ref U26) (pin 10))
      (node (ref J10) (pin 3)))
    (net (code 260) (name /Freedom-U540_2/QSPI2_SCK_CON)
      (node (ref J10) (pin 5))
      (node (ref U26) (pin 9)))
    (net (code 261) (name /Freedom-U540_2/QSPI2_MISO_CON)
      (node (ref J10) (pin 7))
      (node (ref U26) (pin 8)))
    (net (code 262) (name /Freedom-U540_2/QSPI2_HOLD_CON)
      (node (ref J10) (pin 8))
      (node (ref U26) (pin 7)))
    (net (code 263) (name /Freedom-U540_2/QSPI2_HOLD_3V3)
      (node (ref U24) (pin 4))
      (node (ref U26) (pin 6)))
    (net (code 264) (name /Freedom-U540_2/QSPI2_MISO_3V3)
      (node (ref U26) (pin 5))
      (node (ref R73) (pin 2))
      (node (ref U22) (pin 2)))
    (net (code 265) (name /Freedom-U540_2/QSPI2_SCK_3V3)
      (node (ref U26) (pin 4))
      (node (ref U20) (pin 4)))
    (net (code 266) (name /Freedom-U540_2/QSPI2_CS_3V3)
      (node (ref U26) (pin 2))
      (node (ref U25) (pin 4)))
    (net (code 267) (name /Freedom-U540_2/QSPI2_WP_3V3)
      (node (ref U26) (pin 1))
      (node (ref U23) (pin 4)))
    (net (code 268) (name /Freedom-U540_2/QSPI2_SCK_R)
      (node (ref U20) (pin 2))
      (node (ref R139) (pin 1)))
    (net (code 269) (name /Freedom-U540_2/QSPI2_MOSI_R)
      (node (ref U21) (pin 2))
      (node (ref R141) (pin 1)))
    (net (code 270) (name /Freedom-U540_2/QSPI2_MISO_R)
      (node (ref U22) (pin 4))
      (node (ref R142) (pin 1)))
    (net (code 271) (name /Freedom-U540_2/QSPI2_WP_R)
      (node (ref R143) (pin 1))
      (node (ref U23) (pin 2)))
    (net (code 272) (name /Freedom-U540_2/QSPI2_HOLD_R)
      (node (ref U24) (pin 2))
      (node (ref R140) (pin 1)))
    (net (code 273) (name /Freedom-U540_2/QSPI2_CS_R)
      (node (ref R144) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref U25) (pin 2)))
    (net (code 274) (name /Freedom-U540_2/IO_PRCI_RSVD4)
      (node (ref J13) (pin 2))
      (node (ref U1) (pin C16)))
    (net (code 275) (name /Freedom-U540_2/IO_PRCI_RSVD3)
      (node (ref J13) (pin 1))
      (node (ref U1) (pin D16)))
    (net (code 276) (name /Freedom-U540_2/IO_PRCI_RSVD9)
      (node (ref U1) (pin E16))
      (node (ref J13) (pin 7)))
    (net (code 277) (name /Freedom-U540_2/IO_PRCI_RSVD8)
      (node (ref J13) (pin 6))
      (node (ref U1) (pin H13)))
    (net (code 278) (name /Freedom-U540_2/IO_PRCI_RSVD7)
      (node (ref U1) (pin G13))
      (node (ref J13) (pin 5)))
    (net (code 279) (name /Freedom-U540_2/IO_PRCI_RSVD6)
      (node (ref U1) (pin B17))
      (node (ref J13) (pin 4)))
    (net (code 280) (name /Freedom-U540_2/IO_PRCI_RSVD5)
      (node (ref J13) (pin 3))
      (node (ref U1) (pin E15)))
    (net (code 281) (name /Freedom-U540_2/RTCXALTCLKIN)
      (node (ref X2) (pin 3))
      (node (ref U1) (pin B16)))
    (net (code 282) (name PORESET_N)
      (node (ref R37) (pin 1))
      (node (ref U1) (pin A17))
      (node (ref U19) (pin 4)))
    (net (code 283) (name PWR_BTN_N)
      (node (ref J1) (pin 38))
      (node (ref Q5) (pin 5)))
    (net (code 284) (name /Freedom-U540_2/QSPI2_WP_CON)
      (node (ref J10) (pin 1))
      (node (ref U26) (pin 12)))
    (net (code 285) (name "Net-(Q4-Pad3)")
      (node (ref Q4) (pin 3))
      (node (ref R161) (pin 1))
      (node (ref Q6) (pin 1)))
    (net (code 286) (name /Freedom-U540_2/QSPI1_DQ2)
      (node (ref R160) (pin 2))
      (node (ref U1) (pin F22)))
    (net (code 287) (name /Freedom-U540_2/MSEL3)
      (node (ref U1) (pin B19))
      (node (ref R30) (pin 1))
      (node (ref R25) (pin 2))
      (node (ref S1) (pin 6)))
    (net (code 288) (name VD)
      (node (ref U9) (pin J1))
      (node (ref C69) (pin 2))
      (node (ref U10) (pin J1))
      (node (ref U8) (pin J1))
      (node (ref C67) (pin 2))
      (node (ref C89) (pin 2))
      (node (ref C87) (pin 2))
      (node (ref C65) (pin 2))
      (node (ref U7) (pin J1))
      (node (ref U6) (pin J1))
      (node (ref U5) (pin J1))
      (node (ref U4) (pin J1))
      (node (ref C19) (pin 2))
      (node (ref U2) (pin J1))
      (node (ref C90) (pin 2))
      (node (ref U11) (pin 6))
      (node (ref C17) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref U3) (pin J1)))
    (net (code 289) (name +1V2)
      (node (ref U8) (pin C9))
      (node (ref C12) (pin 2))
      (node (ref U8) (pin C7))
      (node (ref C10) (pin 2))
      (node (ref U5) (pin C7))
      (node (ref C9) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U8) (pin C1))
      (node (ref C4) (pin 2))
      (node (ref U8) (pin B8))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U8) (pin B2))
      (node (ref U8) (pin H1))
      (node (ref U3) (pin F9))
      (node (ref U8) (pin F9))
      (node (ref U2) (pin B8))
      (node (ref U5) (pin A1))
      (node (ref U9) (pin E8))
      (node (ref U9) (pin E2))
      (node (ref U9) (pin C9))
      (node (ref U9) (pin C7))
      (node (ref U10) (pin H1))
      (node (ref U10) (pin F9))
      (node (ref C34) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref U10) (pin F1))
      (node (ref C28) (pin 2))
      (node (ref U10) (pin E8))
      (node (ref U10) (pin E2))
      (node (ref C11) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U10) (pin M1))
      (node (ref U4) (pin M1))
      (node (ref U10) (pin J9))
      (node (ref C7) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref U8) (pin E2))
      (node (ref U7) (pin C7))
      (node (ref U2) (pin B2))
      (node (ref U5) (pin B8))
      (node (ref U7) (pin C9))
      (node (ref U7) (pin J9))
      (node (ref U7) (pin H1))
      (node (ref U7) (pin F1))
      (node (ref U5) (pin B2))
      (node (ref U8) (pin M1))
      (node (ref U8) (pin J9))
      (node (ref U9) (pin M1))
      (node (ref C55) (pin 2))
      (node (ref C64) (pin 2))
      (node (ref U7) (pin C1))
      (node (ref U7) (pin B8))
      (node (ref U7) (pin B2))
      (node (ref RS1) (pin 1))
      (node (ref U3) (pin B8))
      (node (ref U7) (pin A1))
      (node (ref U7) (pin E8))
      (node (ref U2) (pin E2))
      (node (ref U5) (pin C1))
      (node (ref U8) (pin F1))
      (node (ref U5) (pin C9))
      (node (ref U2) (pin C1))
      (node (ref U2) (pin C7))
      (node (ref U2) (pin C9))
      (node (ref U9) (pin F9))
      (node (ref U2) (pin E8))
      (node (ref U2) (pin F1))
      (node (ref U3) (pin M1))
      (node (ref U7) (pin E2))
      (node (ref U3) (pin N9))
      (node (ref U8) (pin E8))
      (node (ref U9) (pin J9))
      (node (ref U9) (pin H1))
      (node (ref U2) (pin A1))
      (node (ref U8) (pin A1))
      (node (ref U9) (pin N9))
      (node (ref U3) (pin F1))
      (node (ref U3) (pin B2))
      (node (ref U2) (pin H1))
      (node (ref U3) (pin A1))
      (node (ref U4) (pin H1))
      (node (ref U4) (pin N9))
      (node (ref U3) (pin C7))
      (node (ref U2) (pin F9))
      (node (ref U3) (pin J9))
      (node (ref U7) (pin F9))
      (node (ref U3) (pin H1))
      (node (ref U4) (pin J9))
      (node (ref U3) (pin C9))
      (node (ref U3) (pin E2))
      (node (ref U2) (pin J9))
      (node (ref U3) (pin E8))
      (node (ref U6) (pin N9))
      (node (ref U4) (pin E8))
      (node (ref U4) (pin E2))
      (node (ref U9) (pin C1))
      (node (ref U9) (pin B8))
      (node (ref U9) (pin B2))
      (node (ref C27) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref U9) (pin A1))
      (node (ref U10) (pin N9))
      (node (ref U4) (pin A1))
      (node (ref U2) (pin N9))
      (node (ref U4) (pin C9))
      (node (ref U4) (pin C7))
      (node (ref U4) (pin C1))
      (node (ref U4) (pin B8))
      (node (ref U4) (pin B2))
      (node (ref U2) (pin M1))
      (node (ref U9) (pin F1))
      (node (ref U5) (pin N9))
      (node (ref U3) (pin C1))
      (node (ref U4) (pin F1))
      (node (ref U4) (pin F9))
      (node (ref U10) (pin C7))
      (node (ref C45) (pin 2))
      (node (ref U10) (pin B8))
      (node (ref C42) (pin 2))
      (node (ref U10) (pin C9))
      (node (ref U10) (pin C1))
      (node (ref U6) (pin A1))
      (node (ref U10) (pin B2))
      (node (ref U7) (pin N9))
      (node (ref U10) (pin A1))
      (node (ref U5) (pin M1))
      (node (ref U6) (pin B2))
      (node (ref C74) (pin 2))
      (node (ref U7) (pin M1))
      (node (ref U5) (pin F9))
      (node (ref C61) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref U6) (pin M1))
      (node (ref U6) (pin E8))
      (node (ref U6) (pin J9))
      (node (ref C51) (pin 2))
      (node (ref C50) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref C49) (pin 2))
      (node (ref C86) (pin 2))
      (node (ref C84) (pin 2))
      (node (ref U6) (pin B8))
      (node (ref C6) (pin 2))
      (node (ref C85) (pin 2))
      (node (ref C83) (pin 2))
      (node (ref U5) (pin H1))
      (node (ref C43) (pin 2))
      (node (ref C44) (pin 1))
      (node (ref C76) (pin 2))
      (node (ref U6) (pin E2))
      (node (ref C73) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref C71) (pin 2))
      (node (ref C78) (pin 2))
      (node (ref U6) (pin C9))
      (node (ref U6) (pin C7))
      (node (ref U5) (pin J9))
      (node (ref U6) (pin C1))
      (node (ref C77) (pin 2))
      (node (ref C46) (pin 2))
      (node (ref C80) (pin 2))
      (node (ref U6) (pin H1))
      (node (ref C22) (pin 2))
      (node (ref U6) (pin F9))
      (node (ref C81) (pin 2))
      (node (ref C82) (pin 2))
      (node (ref U6) (pin F1))
      (node (ref U8) (pin N9))
      (node (ref U5) (pin F1))
      (node (ref U5) (pin E8))
      (node (ref C62) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref U5) (pin E2))
      (node (ref C75) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref C48) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref C58) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C68) (pin 2))
      (node (ref C66) (pin 2))
      (node (ref C57) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref C31) (pin 2))
      (node (ref C47) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref C60) (pin 2))
      (node (ref C59) (pin 2))
      (node (ref U11) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C30) (pin 2)))
    (net (code 290) (name DDR_ODT1)
      (node (ref U5) (pin F2))
      (node (ref U7) (pin F2))
      (node (ref R184) (pin 2))
      (node (ref U10) (pin F2))
      (node (ref U3) (pin F2))
      (node (ref U8) (pin F2))
      (node (ref U6) (pin F2))
      (node (ref U2) (pin F2))
      (node (ref U4) (pin F2))
      (node (ref U1) (pin AB5))
      (node (ref U9) (pin F2)))
    (net (code 291) (name "Net-(R2-Pad2)")
      (node (ref U3) (pin B9))
      (node (ref R2) (pin 2)))
    (net (code 292) (name "Net-(R4-Pad2)")
      (node (ref U4) (pin B9))
      (node (ref R4) (pin 2)))
    (net (code 293) (name "Net-(R3-Pad2)")
      (node (ref U5) (pin B9))
      (node (ref R3) (pin 2)))
    (net (code 294) (name "Net-(C265-Pad2)")
      (node (ref R171) (pin 1))
      (node (ref R170) (pin 1))
      (node (ref C265) (pin 2)))
    (net (code 295) (name "Net-(U2-PadA3)")
      (node (ref U2) (pin A3)))
    (net (code 296) (name "Net-(U3-PadN7)")
      (node (ref U3) (pin N7)))
    (net (code 297) (name "Net-(R1-Pad2)")
      (node (ref U2) (pin B9))
      (node (ref R1) (pin 2)))
    (net (code 298) (name VAA)
      (node (ref R179) (pin 1))
      (node (ref C284) (pin 2))
      (node (ref R169) (pin 1))
      (node (ref R184) (pin 1))
      (node (ref C93) (pin 2))
      (node (ref C91) (pin 2))
      (node (ref R180) (pin 1))
      (node (ref C261) (pin 2))
      (node (ref C264) (pin 2))
      (node (ref C263) (pin 2))
      (node (ref C92) (pin 2))
      (node (ref C262) (pin 2))
      (node (ref C260) (pin 2))
      (node (ref C259) (pin 2))
      (node (ref R181) (pin 1))
      (node (ref R163) (pin 5))
      (node (ref R163) (pin 6))
      (node (ref R163) (pin 7))
      (node (ref R166) (pin 7))
      (node (ref R166) (pin 8))
      (node (ref R166) (pin 6))
      (node (ref R164) (pin 5))
      (node (ref R166) (pin 5))
      (node (ref R164) (pin 8))
      (node (ref R164) (pin 7))
      (node (ref R164) (pin 6))
      (node (ref U11) (pin 5))
      (node (ref R168) (pin 8))
      (node (ref R168) (pin 7))
      (node (ref R167) (pin 8))
      (node (ref R165) (pin 7))
      (node (ref R165) (pin 6))
      (node (ref R165) (pin 5))
      (node (ref R165) (pin 8))
      (node (ref R167) (pin 5))
      (node (ref R167) (pin 6))
      (node (ref R168) (pin 6))
      (node (ref R168) (pin 5))
      (node (ref U11) (pin 3))
      (node (ref R163) (pin 8))
      (node (ref R167) (pin 7)))
    (net (code 299) (name VDD_DDR_VPP_N)
      (node (ref C278) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U10) (pin M9))
      (node (ref U9) (pin B1))
      (node (ref C20) (pin 2))
      (node (ref U2) (pin M9))
      (node (ref U4) (pin B1))
      (node (ref U6) (pin M9))
      (node (ref U10) (pin B1))
      (node (ref C279) (pin 2))
      (node (ref C277) (pin 2))
      (node (ref C276) (pin 2))
      (node (ref C275) (pin 2))
      (node (ref C274) (pin 2))
      (node (ref C273) (pin 2))
      (node (ref C272) (pin 2))
      (node (ref C280) (pin 2))
      (node (ref C271) (pin 2))
      (node (ref U2) (pin B1))
      (node (ref U9) (pin M9))
      (node (ref U3) (pin M9))
      (node (ref U8) (pin B1))
      (node (ref U7) (pin M9))
      (node (ref C270) (pin 2))
      (node (ref C240) (pin 2))
      (node (ref C268) (pin 2))
      (node (ref U6) (pin B1))
      (node (ref C38) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref RS11) (pin 1))
      (node (ref U5) (pin M9))
      (node (ref U5) (pin B1))
      (node (ref U8) (pin M9))
      (node (ref C269) (pin 2))
      (node (ref U3) (pin B1))
      (node (ref U7) (pin B1))
      (node (ref U4) (pin M9)))
    (net (code 301) (name "Net-(U2-PadN7)")
      (node (ref U2) (pin N7)))
    (net (code 302) (name "Net-(U11-Pad9)")
      (node (ref U11) (pin 9)))
    (net (code 303) (name /DDR4_x8_32b_1/REFIN)
      (node (ref U11) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref C88) (pin 1)))
    (net (code 304) (name "Net-(U5-PadN7)")
      (node (ref U5) (pin N7)))
    (net (code 305) (name "Net-(U4-PadN7)")
      (node (ref U4) (pin N7)))
    (net (code 306) (name DDR_CS1_N)
      (node (ref R164) (pin 3))
      (node (ref U3) (pin G8))
      (node (ref U7) (pin G8))
      (node (ref U2) (pin G8))
      (node (ref U4) (pin G8))
      (node (ref U6) (pin G8))
      (node (ref U1) (pin W7))
      (node (ref U10) (pin G8))
      (node (ref U5) (pin G8))
      (node (ref U9) (pin G8))
      (node (ref U8) (pin G8)))
    (net (code 307) (name VDD_DDR_VPP_P)
      (node (ref RS11) (pin 2))
      (node (ref R138) (pin 2))
      (node (ref U50) (pin 5))
      (node (ref C281) (pin 2))
      (node (ref L6) (pin 2)))
    (net (code 308) (name DDR_DQ30)
      (node (ref U5) (pin E7))
      (node (ref U1) (pin D3)))
    (net (code 309) (name DDR_DQ29)
      (node (ref U5) (pin E3))
      (node (ref U1) (pin C2)))
    (net (code 310) (name DDR_DQ25)
      (node (ref U1) (pin D4))
      (node (ref U5) (pin D3)))
    (net (code 311) (name DDR_DQ3)
      (node (ref U2) (pin E3))
      (node (ref U1) (pin E2)))
    (net (code 312) (name DDR_DQ27)
      (node (ref U5) (pin D2))
      (node (ref U1) (pin C3)))
    (net (code 313) (name DDR_DQ17)
      (node (ref U1) (pin B2))
      (node (ref U4) (pin E7)))
    (net (code 314) (name DDR_DQ22)
      (node (ref U1) (pin B3))
      (node (ref U4) (pin E3)))
    (net (code 315) (name DDR_DQ20)
      (node (ref U1) (pin B5))
      (node (ref U4) (pin D8)))
    (net (code 316) (name DDR_DQ19)
      (node (ref U1) (pin A5))
      (node (ref U4) (pin D3)))
    (net (code 317) (name DDR_DQ21)
      (node (ref U1) (pin C5))
      (node (ref U4) (pin C2)))
    (net (code 318) (name DDR_DQ16)
      (node (ref U1) (pin B4))
      (node (ref U4) (pin B7)))
    (net (code 319) (name DDR_DQ10)
      (node (ref U3) (pin D8))
      (node (ref U1) (pin F5)))
    (net (code 320) (name DDR_DQ13)
      (node (ref U3) (pin D3))
      (node (ref U1) (pin J3)))
    (net (code 321) (name DDR_DQ14)
      (node (ref U3) (pin C2))
      (node (ref U1) (pin J2)))
    (net (code 322) (name DDR_DQ8)
      (node (ref U3) (pin B7))
      (node (ref U1) (pin H4)))
    (net (code 323) (name DDR_DQ6)
      (node (ref U2) (pin B7))
      (node (ref U1) (pin E1)))
    (net (code 324) (name DDR_DQ7)
      (node (ref U1) (pin G3))
      (node (ref U2) (pin D7)))
    (net (code 325) (name DDR_DQ12)
      (node (ref U3) (pin E3))
      (node (ref U1) (pin H1)))
    (net (code 326) (name DDR_DQ15)
      (node (ref U1) (pin J4))
      (node (ref U3) (pin D2)))
    (net (code 327) (name DDR_DQ23)
      (node (ref U1) (pin B6))
      (node (ref U4) (pin D2)))
    (net (code 328) (name "Net-(U5-PadA3)")
      (node (ref U5) (pin A3)))
    (net (code 329) (name "Net-(U3-PadA3)")
      (node (ref U3) (pin A3)))
    (net (code 330) (name "Net-(U4-PadA3)")
      (node (ref U4) (pin A3)))
    (net (code 331) (name "Net-(R23-Pad2)")
      (node (ref U13) (pin 14))
      (node (ref R23) (pin 2)))
    (net (code 332) (name "Net-(R26-Pad2)")
      (node (ref R26) (pin 2))
      (node (ref U30) (pin 4)))
    (net (code 333) (name "Net-(R31-Pad2)")
      (node (ref R31) (pin 2))
      (node (ref U31) (pin 4)))
    (net (code 334) (name "Net-(R32-Pad2)")
      (node (ref U33) (pin 4))
      (node (ref R32) (pin 2)))
    (net (code 335) (name "Net-(R34-Pad2)")
      (node (ref R34) (pin 2))
      (node (ref U28) (pin 4)))
    (net (code 336) (name "Net-(U13-Pad41)")
      (node (ref U13) (pin 41)))
    (net (code 337) (name "Net-(U13-Pad27)")
      (node (ref U13) (pin 27)))
    (net (code 338) (name "Net-(U13-Pad28)")
      (node (ref U13) (pin 28)))
    (net (code 339) (name "Net-(U13-Pad29)")
      (node (ref U13) (pin 29)))
    (net (code 340) (name "Net-(U13-Pad30)")
      (node (ref U13) (pin 30)))
    (net (code 341) (name "Net-(U13-Pad32)")
      (node (ref U13) (pin 32)))
    (net (code 342) (name "Net-(U13-Pad33)")
      (node (ref U13) (pin 33)))
    (net (code 343) (name "Net-(U13-Pad34)")
      (node (ref U13) (pin 34)))
    (net (code 344) (name "Net-(U13-Pad40)")
      (node (ref U13) (pin 40)))
    (net (code 345) (name "Net-(U13-Pad26)")
      (node (ref U13) (pin 26)))
    (net (code 346) (name "Net-(U13-Pad43)")
      (node (ref U13) (pin 43)))
    (net (code 347) (name "Net-(U13-Pad44)")
      (node (ref U13) (pin 44)))
    (net (code 348) (name "Net-(U13-Pad45)")
      (node (ref U13) (pin 45)))
    (net (code 349) (name "Net-(U13-Pad46)")
      (node (ref U13) (pin 46)))
    (net (code 350) (name "Net-(U13-Pad48)")
      (node (ref U13) (pin 48)))
    (net (code 351) (name "Net-(U13-Pad52)")
      (node (ref U13) (pin 52)))
    (net (code 352) (name "Net-(U13-Pad53)")
      (node (ref U13) (pin 53)))
    (net (code 353) (name "Net-(C114-Pad2)")
      (node (ref U13) (pin 2))
      (node (ref C114) (pin 2))
      (node (ref Y2) (pin 1)))
    (net (code 354) (name "Net-(C115-Pad2)")
      (node (ref Y2) (pin 3))
      (node (ref C115) (pin 2))
      (node (ref U13) (pin 3)))
    (net (code 355) (name "Net-(U13-Pad54)")
      (node (ref U13) (pin 54)))
    (net (code 356) (name "Net-(J7-Pad4)")
      (node (ref J7) (pin 4)))
    (net (code 357) (name "Net-(U13-Pad63)")
      (node (ref U13) (pin 63)))
    (net (code 358) (name "Net-(U13-Pad62)")
      (node (ref U13) (pin 62)))
    (net (code 359) (name "Net-(U13-Pad61)")
      (node (ref U13) (pin 61)))
    (net (code 360) (name "Net-(U13-Pad21)")
      (node (ref U13) (pin 21)))
    (net (code 361) (name "Net-(U13-Pad23)")
      (node (ref U13) (pin 23)))
    (net (code 362) (name "Net-(U13-Pad24)")
      (node (ref U13) (pin 24)))
    (net (code 363) (name "Net-(R33-Pad2)")
      (node (ref U13) (pin 6))
      (node (ref R33) (pin 2)))
    (net (code 364) (name "Net-(U13-Pad36)")
      (node (ref U13) (pin 36)))
    (net (code 365) (name "Net-(U13-Pad60)")
      (node (ref U13) (pin 60)))
    (net (code 366) (name "Net-(U13-Pad59)")
      (node (ref U13) (pin 59)))
    (net (code 367) (name "Net-(U13-Pad58)")
      (node (ref U13) (pin 58)))
    (net (code 368) (name "Net-(U13-Pad57)")
      (node (ref U13) (pin 57)))
    (net (code 369) (name "Net-(U13-Pad55)")
      (node (ref U13) (pin 55)))
    (net (code 370) (name "Net-(C111-Pad2)")
      (node (ref J7) (pin 1))
      (node (ref C111) (pin 2)))
    (net (code 371) (name VDDA)
      (node (ref U13) (pin 49))
      (node (ref U13) (pin 37))
      (node (ref U13) (pin 12))
      (node (ref C106) (pin 2))
      (node (ref C105) (pin 2))
      (node (ref C107) (pin 2))
      (node (ref C112) (pin 2))
      (node (ref U13) (pin 64))
      (node (ref C113) (pin 2)))
    (net (code 372) (name /FT2232/FT_JTAG_TCK)
      (node (ref U13) (pin 16))
      (node (ref U30) (pin 2)))
    (net (code 373) (name /FT2232/USB_D_P)
      (node (ref D5) (pin 2))
      (node (ref J7) (pin 3))
      (node (ref U13) (pin 8)))
    (net (code 374) (name /FT2232/FT_JTAG_TDI)
      (node (ref U13) (pin 17))
      (node (ref U31) (pin 2)))
    (net (code 375) (name /FT2232/FT_JTAG_TDO)
      (node (ref U13) (pin 18))
      (node (ref U32) (pin 4)))
    (net (code 376) (name /FT2232/FT_JTAG_TMS)
      (node (ref U13) (pin 19))
      (node (ref U33) (pin 2)))
    (net (code 377) (name /FT2232/VPHY_FT)
      (node (ref C109) (pin 2))
      (node (ref FB2) (pin 1))
      (node (ref U13) (pin 4))
      (node (ref C108) (pin 2)))
    (net (code 378) (name /FT2232/VPLL_FT)
      (node (ref U13) (pin 9))
      (node (ref FB1) (pin 1))
      (node (ref C100) (pin 2))
      (node (ref C101) (pin 2)))
    (net (code 379) (name /FT2232/USB_D_N)
      (node (ref J7) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref U13) (pin 7)))
    (net (code 380) (name /FT2232/FT_JTAG_SRST)
      (node (ref U13) (pin 22))
      (node (ref R74) (pin 1))
      (node (ref Q4) (pin 6)))
    (net (code 381) (name /FT2232/FT_UART_RX)
      (node (ref U13) (pin 39))
      (node (ref U29) (pin 4)))
    (net (code 382) (name /FT2232/FT_UART_TX)
      (node (ref U13) (pin 38))
      (node (ref U28) (pin 2)))
    (net (code 383) (name "Net-(D7-Pad2)")
      (node (ref D7) (pin 2))
      (node (ref J8) (pin 1)))
    (net (code 384) (name "Net-(C119-Pad2)")
      (node (ref C119) (pin 2))
      (node (ref U27) (pin 9)))
    (net (code 385) (name "Net-(J19-Pad1)")
      (node (ref J19) (pin 1)))
    (net (code 386) (name "Net-(S4-Pad1)")
      (node (ref S4) (pin 1)))
    (net (code 387) (name "Net-(L1-Pad1)")
      (node (ref U27) (pin 1))
      (node (ref U27) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref U27) (pin 3)))
    (net (code 388) (name "Net-(R35-Pad1)")
      (node (ref R35) (pin 1))
      (node (ref U27) (pin 4)))
    (net (code 389) (name /Power.sch/PWR_EN2)
      (node (ref R62) (pin 1))
      (node (ref R68) (pin 2))
      (node (ref R66) (pin 2))
      (node (ref U19) (pin 5)))
    (net (code 390) (name /Power.sch/EN_PLL)
      (node (ref U17) (pin 3))
      (node (ref R68) (pin 1)))
    (net (code 391) (name /Power.sch/EN_CORE)
      (node (ref U18) (pin 28))
      (node (ref R66) (pin 1)))
    (net (code 392) (name /Power.sch/EN_1V8)
      (node (ref R64) (pin 1))
      (node (ref U15) (pin 1)))
    (net (code 393) (name /Power.sch/EN_3V3)
      (node (ref R63) (pin 1))
      (node (ref U14) (pin 1)))
    (net (code 394) (name /Power.sch/EN_DDR)
      (node (ref U16) (pin 13))
      (node (ref R43) (pin 1)))
    (net (code 395) (name /Power.sch/PWR_EN1)
      (node (ref R42) (pin 1))
      (node (ref R63) (pin 2))
      (node (ref R64) (pin 2))
      (node (ref U19) (pin 6))
      (node (ref R177) (pin 2))
      (node (ref R43) (pin 2)))
    (net (code 396) (name "Net-(R60-Pad1)")
      (node (ref R60) (pin 1))
      (node (ref R61) (pin 2))
      (node (ref U16) (pin 5)))
    (net (code 397) (name "Net-(C220-Pad2)")
      (node (ref R69) (pin 2))
      (node (ref C220) (pin 2))
      (node (ref U18) (pin 26)))
    (net (code 398) (name "Net-(R69-Pad1)")
      (node (ref R69) (pin 1))
      (node (ref R71) (pin 2))
      (node (ref U18) (pin 25)))
    (net (code 399) (name "Net-(D9-Pad2)")
      (node (ref R36) (pin 1))
      (node (ref D9) (pin 2)))
    (net (code 400) (name "Net-(U50-Pad6)")
      (node (ref U50) (pin 6)))
    (net (code 401) (name "Net-(L6-Pad1)")
      (node (ref U50) (pin 7))
      (node (ref L6) (pin 1)))
    (net (code 402) (name "Net-(R138-Pad1)")
      (node (ref U50) (pin 4))
      (node (ref R138) (pin 1))
      (node (ref R156) (pin 1)))
    (net (code 403) (name "Net-(U14-Pad6)")
      (node (ref U14) (pin 6)))
    (net (code 404) (name "Net-(R40-Pad1)")
      (node (ref U15) (pin 4))
      (node (ref R40) (pin 1))
      (node (ref R41) (pin 1)))
    (net (code 405) (name /Power.sch/EN_DDR_VPP)
      (node (ref U50) (pin 1))
      (node (ref R177) (pin 1)))
    (net (code 406) (name "Net-(U16-Pad4)")
      (node (ref U16) (pin 4)))
    (net (code 407) (name "Net-(L3-Pad1)")
      (node (ref L3) (pin 1))
      (node (ref U15) (pin 7)))
    (net (code 408) (name "Net-(L2-Pad1)")
      (node (ref U14) (pin 7))
      (node (ref L2) (pin 1)))
    (net (code 409) (name "Net-(R38-Pad1)")
      (node (ref R38) (pin 1))
      (node (ref R39) (pin 1))
      (node (ref U14) (pin 4)))
    (net (code 410) (name "Net-(C143-Pad1)")
      (node (ref U16) (pin 9))
      (node (ref C143) (pin 1)))
    (net (code 411) (name "Net-(C142-Pad1)")
      (node (ref C142) (pin 1))
      (node (ref U16) (pin 7)))
    (net (code 412) (name "Net-(L4-Pad1)")
      (node (ref U16) (pin 1))
      (node (ref U16) (pin 2))
      (node (ref L4) (pin 1)))
    (net (code 413) (name "Net-(C146-Pad1)")
      (node (ref U18) (pin 9))
      (node (ref U18) (pin 7))
      (node (ref U18) (pin 6))
      (node (ref C146) (pin 1))
      (node (ref L5) (pin 1))
      (node (ref U18) (pin 8)))
    (net (code 414) (name "Net-(C152-Pad2)")
      (node (ref U18) (pin 21))
      (node (ref C152) (pin 2)))
    (net (code 415) (name "Net-(R117-Pad1)")
      (node (ref R117) (pin 1))
      (node (ref U18) (pin 3)))
    (net (code 416) (name "Net-(U18-Pad1)")
      (node (ref U18) (pin 1)))
    (net (code 417) (name "Net-(U18-Pad24)")
      (node (ref U18) (pin 24)))
    (net (code 418) (name "Net-(C146-Pad2)")
      (node (ref C146) (pin 2))
      (node (ref U18) (pin 5)))
    (net (code 419) (name PG_1V8)
      (node (ref U15) (pin 6))
      (node (ref J9) (pin F1)))
    (net (code 420) (name "Net-(C142-Pad2)")
      (node (ref U16) (pin 8))
      (node (ref C142) (pin 2)))
    (net (code 421) (name /Power.sch/PWR_ON)
      (node (ref C148) (pin 2))
      (node (ref U19) (pin 3))
      (node (ref D12) (pin 2))
      (node (ref Q5) (pin 3))
      (node (ref R67) (pin 1))
      (node (ref S4) (pin 2)))
    (net (code 422) (name "Net-(U17-Pad4)")
      (node (ref U17) (pin 4)))
    (net (code 423) (name "Net-(U18-Pad27)")
      (node (ref U18) (pin 27)))
    (net (code 424) (name "Net-(U18-Pad2)")
      (node (ref U18) (pin 2)))
    (net (code 425) (name "Net-(U18-Pad4)")
      (node (ref U18) (pin 4)))
    (net (code 426) (name CHIPLINK_TX_DAT4)
      (node (ref R154) (pin 5))
      (node (ref J9) (pin H7)))
    (net (code 427) (name CHIPLINK_TX_DAT5)
      (node (ref R151) (pin 6))
      (node (ref J9) (pin H8)))
    (net (code 428) (name CHIPLINK_TX_DAT8)
      (node (ref R147) (pin 7))
      (node (ref J9) (pin H10)))
    (net (code 429) (name CHIPLINK_TX_DAT9)
      (node (ref R151) (pin 5))
      (node (ref J9) (pin H11)))
    (net (code 430) (name CHIPLINK_TX_DAT6)
      (node (ref R152) (pin 6))
      (node (ref J9) (pin G9)))
    (net (code 431) (name /FMC.sch/FMC_GA1)
      (node (ref U49) (pin 2))
      (node (ref J9) (pin D35)))
    (net (code 432) (name "Net-(J9-PadD5)")
      (node (ref J9) (pin D5)))
    (net (code 433) (name "Net-(J9-PadD40)")
      (node (ref J9) (pin D40)))
    (net (code 434) (name "Net-(J9-PadD4)")
      (node (ref J9) (pin D4)))
    (net (code 435) (name "Net-(J9-PadD38)")
      (node (ref J9) (pin D38)))
    (net (code 436) (name "Net-(J9-PadD36)")
      (node (ref J9) (pin D36)))
    (net (code 437) (name "Net-(J9-PadD34)")
      (node (ref J9) (pin D34)))
    (net (code 438) (name "Net-(J9-PadD33)")
      (node (ref J9) (pin D33)))
    (net (code 439) (name "Net-(J9-PadD30)")
      (node (ref J9) (pin D30))
      (node (ref R172) (pin 1)))
    (net (code 440) (name "Net-(J9-PadD29)")
      (node (ref J9) (pin D29)))
    (net (code 441) (name "Net-(J9-PadE25)")
      (node (ref J9) (pin E25)))
    (net (code 442) (name "Net-(J9-PadE24)")
      (node (ref J9) (pin E24)))
    (net (code 443) (name "Net-(J9-PadE22)")
      (node (ref J9) (pin E22)))
    (net (code 444) (name "Net-(J9-PadE21)")
      (node (ref J9) (pin E21)))
    (net (code 445) (name "Net-(J9-PadE2)")
      (node (ref J9) (pin E2)))
    (net (code 446) (name "Net-(J9-PadE19)")
      (node (ref J9) (pin E19)))
    (net (code 447) (name "Net-(J9-PadE18)")
      (node (ref J9) (pin E18)))
    (net (code 448) (name "Net-(J9-PadE16)")
      (node (ref J9) (pin E16)))
    (net (code 449) (name "Net-(J9-PadE15)")
      (node (ref J9) (pin E15)))
    (net (code 450) (name "Net-(J9-PadE13)")
      (node (ref J9) (pin E13)))
    (net (code 451) (name "Net-(J9-PadE12)")
      (node (ref J9) (pin E12)))
    (net (code 452) (name "Net-(J9-PadE10)")
      (node (ref J9) (pin E10)))
    (net (code 453) (name "Net-(J9-PadC7)")
      (node (ref J9) (pin C7)))
    (net (code 454) (name "Net-(J9-PadC6)")
      (node (ref J9) (pin C6)))
    (net (code 455) (name "Net-(J9-PadC39)")
      (node (ref J9) (pin C39)))
    (net (code 456) (name /FMC.sch/FMC_GA0)
      (node (ref U49) (pin 1))
      (node (ref J9) (pin C34)))
    (net (code 457) (name /FMC.sch/FMC_SDA)
      (node (ref J9) (pin C31))
      (node (ref U49) (pin 5)))
    (net (code 458) (name /FMC.sch/FMC_SCL)
      (node (ref J9) (pin C30))
      (node (ref U49) (pin 6)))
    (net (code 459) (name "Net-(J9-PadC3)")
      (node (ref J9) (pin C3)))
    (net (code 460) (name "Net-(J9-PadD1)")
      (node (ref J9) (pin D1)))
    (net (code 461) (name "Net-(J9-PadF35)")
      (node (ref J9) (pin F35)))
    (net (code 462) (name "Net-(J9-PadF7)")
      (node (ref J9) (pin F7)))
    (net (code 463) (name "Net-(J9-PadF5)")
      (node (ref J9) (pin F5)))
    (net (code 464) (name "Net-(J9-PadF40)")
      (node (ref J9) (pin F40)))
    (net (code 465) (name "Net-(J9-PadF4)")
      (node (ref J9) (pin F4)))
    (net (code 466) (name "Net-(J9-PadF38)")
      (node (ref J9) (pin F38)))
    (net (code 467) (name "Net-(J9-PadF37)")
      (node (ref J9) (pin F37)))
    (net (code 468) (name "Net-(J9-PadF8)")
      (node (ref J9) (pin F8)))
    (net (code 469) (name "Net-(J9-PadF34)")
      (node (ref J9) (pin F34)))
    (net (code 470) (name "Net-(J9-PadF32)")
      (node (ref J9) (pin F32)))
    (net (code 471) (name "Net-(J9-PadF31)")
      (node (ref J9) (pin F31)))
    (net (code 472) (name "Net-(J9-PadF29)")
      (node (ref J9) (pin F29)))
    (net (code 473) (name "Net-(J9-PadF28)")
      (node (ref J9) (pin F28)))
    (net (code 474) (name "Net-(J9-PadF26)")
      (node (ref J9) (pin F26)))
    (net (code 475) (name "Net-(J9-PadE7)")
      (node (ref J9) (pin E7)))
    (net (code 476) (name "Net-(J9-PadE6)")
      (node (ref J9) (pin E6)))
    (net (code 477) (name "Net-(J9-PadE39)")
      (node (ref J9) (pin E39)))
    (net (code 478) (name "Net-(J9-PadE37)")
      (node (ref J9) (pin E37)))
    (net (code 479) (name "Net-(J9-PadE36)")
      (node (ref J9) (pin E36)))
    (net (code 480) (name "Net-(J9-PadE34)")
      (node (ref J9) (pin E34)))
    (net (code 481) (name "Net-(J9-PadE33)")
      (node (ref J9) (pin E33)))
    (net (code 482) (name "Net-(J9-PadE31)")
      (node (ref J9) (pin E31)))
    (net (code 483) (name "Net-(J9-PadE30)")
      (node (ref J9) (pin E30)))
    (net (code 484) (name "Net-(J9-PadE3)")
      (node (ref J9) (pin E3)))
    (net (code 485) (name "Net-(J9-PadE28)")
      (node (ref J9) (pin E28)))
    (net (code 486) (name "Net-(J9-PadE27)")
      (node (ref J9) (pin E27)))
    (net (code 487) (name "Net-(J9-PadF17)")
      (node (ref J9) (pin F17)))
    (net (code 488) (name "Net-(J9-PadF25)")
      (node (ref J9) (pin F25)))
    (net (code 489) (name "Net-(J9-PadF23)")
      (node (ref J9) (pin F23)))
    (net (code 490) (name "Net-(J9-PadF22)")
      (node (ref J9) (pin F22)))
    (net (code 491) (name "Net-(J9-PadF20)")
      (node (ref J9) (pin F20)))
    (net (code 492) (name "Net-(J9-PadF19)")
      (node (ref J9) (pin F19)))
    (net (code 493) (name "Net-(J9-PadF16)")
      (node (ref J9) (pin F16)))
    (net (code 494) (name "Net-(J9-PadF14)")
      (node (ref J9) (pin F14)))
    (net (code 495) (name "Net-(J9-PadF13)")
      (node (ref J9) (pin F13)))
    (net (code 496) (name "Net-(J9-PadF11)")
      (node (ref J9) (pin F11)))
    (net (code 497) (name "Net-(J9-PadF10)")
      (node (ref J9) (pin F10)))
    (net (code 498) (name "Net-(J9-PadE9)")
      (node (ref J9) (pin E9)))
    (net (code 499) (name "Net-(J9-PadB8)")
      (node (ref J9) (pin B8)))
    (net (code 500) (name "Net-(J9-PadC2)")
      (node (ref J9) (pin C2)))
    (net (code 501) (name "Net-(J9-PadB9)")
      (node (ref J9) (pin B9)))
    (net (code 502) (name "Net-(J9-PadA35)")
      (node (ref J9) (pin A35)))
    (net (code 503) (name "Net-(J9-PadA27)")
      (node (ref J9) (pin A27)))
    (net (code 504) (name "Net-(J9-PadA3)")
      (node (ref J9) (pin A3)))
    (net (code 505) (name "Net-(J9-PadA30)")
      (node (ref J9) (pin A30)))
    (net (code 506) (name "Net-(J9-PadA31)")
      (node (ref J9) (pin A31)))
    (net (code 507) (name "Net-(J9-PadA34)")
      (node (ref J9) (pin A34)))
    (net (code 508) (name "Net-(J9-PadA26)")
      (node (ref J9) (pin A26)))
    (net (code 509) (name "Net-(J9-PadA38)")
      (node (ref J9) (pin A38)))
    (net (code 510) (name "Net-(J9-PadA39)")
      (node (ref J9) (pin A39)))
    (net (code 511) (name "Net-(J9-PadA6)")
      (node (ref J9) (pin A6)))
    (net (code 512) (name "Net-(J9-PadA7)")
      (node (ref J9) (pin A7)))
    (net (code 513) (name "Net-(J9-PadA10)")
      (node (ref J9) (pin A10)))
    (net (code 514) (name "Net-(J9-PadA11)")
      (node (ref J9) (pin A11)))
    (net (code 515) (name "Net-(J9-PadA14)")
      (node (ref J9) (pin A14)))
    (net (code 516) (name "Net-(J9-PadA15)")
      (node (ref J9) (pin A15)))
    (net (code 517) (name "Net-(J9-PadA18)")
      (node (ref J9) (pin A18)))
    (net (code 518) (name "Net-(J9-PadA19)")
      (node (ref J9) (pin A19)))
    (net (code 519) (name "Net-(J9-PadA2)")
      (node (ref J9) (pin A2)))
    (net (code 520) (name "Net-(J9-PadA22)")
      (node (ref J9) (pin A22)))
    (net (code 521) (name "Net-(J9-PadA23)")
      (node (ref J9) (pin A23)))
    (net (code 522) (name "Net-(J9-PadB28)")
      (node (ref J9) (pin B28)))
    (net (code 523) (name "Net-(J9-PadB29)")
      (node (ref J9) (pin B29)))
    (net (code 524) (name "Net-(J9-PadB32)")
      (node (ref J9) (pin B32)))
    (net (code 525) (name "Net-(J9-PadB33)")
      (node (ref J9) (pin B33)))
    (net (code 526) (name "Net-(J9-PadB36)")
      (node (ref J9) (pin B36)))
    (net (code 527) (name "Net-(J9-PadB37)")
      (node (ref J9) (pin B37)))
    (net (code 528) (name "Net-(J9-PadB4)")
      (node (ref J9) (pin B4)))
    (net (code 529) (name "Net-(J9-PadB40)")
      (node (ref J9) (pin B40)))
    (net (code 530) (name "Net-(J9-PadB5)")
      (node (ref J9) (pin B5)))
    (net (code 531) (name "Net-(J9-PadB17)")
      (node (ref J9) (pin B17)))
    (net (code 532) (name "Net-(J9-PadB1)")
      (node (ref J9) (pin B1)))
    (net (code 533) (name "Net-(J9-PadB12)")
      (node (ref J9) (pin B12)))
    (net (code 534) (name "Net-(J9-PadB13)")
      (node (ref J9) (pin B13)))
    (net (code 535) (name "Net-(J9-PadB16)")
      (node (ref J9) (pin B16)))
    (net (code 536) (name "Net-(J9-PadB20)")
      (node (ref J9) (pin B20)))
    (net (code 537) (name "Net-(J9-PadB21)")
      (node (ref J9) (pin B21)))
    (net (code 538) (name "Net-(J9-PadB24)")
      (node (ref J9) (pin B24)))
    (net (code 539) (name "Net-(J9-PadB25)")
      (node (ref J9) (pin B25)))
    (net (code 540) (name "Net-(J9-PadC35)")
      (node (ref R174) (pin 1))
      (node (ref J9) (pin C37))
      (node (ref R173) (pin 1))
      (node (ref J9) (pin C35)))
    (net (code 541) (name "Net-(J9-PadH5)")
      (node (ref J9) (pin H5))
      (node (ref R175) (pin 1)))
    (net (code 542) (name "Net-(J9-PadD31)")
      (node (ref R172) (pin 2))
      (node (ref J9) (pin D31)))
    (net (code 543) (name "Net-(J9-PadK8)")
      (node (ref J9) (pin K8)))
    (net (code 544) (name "Net-(J9-PadK23)")
      (node (ref J9) (pin K23)))
    (net (code 545) (name "Net-(J9-PadK22)")
      (node (ref J9) (pin K22)))
    (net (code 546) (name "Net-(J9-PadK20)")
      (node (ref J9) (pin K20)))
    (net (code 547) (name "Net-(J9-PadK19)")
      (node (ref J9) (pin K19)))
    (net (code 548) (name "Net-(J9-PadK17)")
      (node (ref J9) (pin K17)))
    (net (code 549) (name "Net-(J9-PadK16)")
      (node (ref J9) (pin K16)))
    (net (code 550) (name "Net-(J9-PadK14)")
      (node (ref J9) (pin K14)))
    (net (code 551) (name "Net-(J9-PadK13)")
      (node (ref J9) (pin K13)))
    (net (code 552) (name "Net-(J9-PadK11)")
      (node (ref J9) (pin K11)))
    (net (code 553) (name "Net-(J9-PadK10)")
      (node (ref J9) (pin K10)))
    (net (code 554) (name "Net-(J9-PadK25)")
      (node (ref J9) (pin K25)))
    (net (code 555) (name "Net-(J9-PadK7)")
      (node (ref J9) (pin K7)))
    (net (code 556) (name "Net-(J9-PadK5)")
      (node (ref J9) (pin K5)))
    (net (code 557) (name "Net-(J9-PadK4)")
      (node (ref J9) (pin K4)))
    (net (code 558) (name "Net-(J9-PadK1)")
      (node (ref J9) (pin K1)))
    (net (code 559) (name "Net-(J9-PadJ39)")
      (node (ref J9) (pin J39)))
    (net (code 560) (name "Net-(J9-PadJ37)")
      (node (ref J9) (pin J37)))
    (net (code 561) (name "Net-(J9-PadJ36)")
      (node (ref J9) (pin J36)))
    (net (code 562) (name "Net-(J9-PadJ34)")
      (node (ref J9) (pin J34)))
    (net (code 563) (name "Net-(J9-PadJ33)")
      (node (ref J9) (pin J33)))
    (net (code 564) (name "Net-(J9-PadK40)")
      (node (ref J9) (pin K40)))
    (net (code 565) (name "Net-(U49-Pad7)")
      (node (ref U49) (pin 7)))
    (net (code 566) (name "Net-(J9-PadJ31)")
      (node (ref J9) (pin J31)))
    (net (code 567) (name "Net-(J9-PadK38)")
      (node (ref J9) (pin K38)))
    (net (code 568) (name "Net-(J9-PadK37)")
      (node (ref J9) (pin K37)))
    (net (code 569) (name "Net-(J9-PadK35)")
      (node (ref J9) (pin K35)))
    (net (code 570) (name "Net-(J9-PadK34)")
      (node (ref J9) (pin K34)))
    (net (code 571) (name "Net-(J9-PadK32)")
      (node (ref J9) (pin K32)))
    (net (code 572) (name "Net-(J9-PadK31)")
      (node (ref J9) (pin K31)))
    (net (code 573) (name "Net-(J9-PadK29)")
      (node (ref J9) (pin K29)))
    (net (code 574) (name "Net-(J9-PadK28)")
      (node (ref J9) (pin K28)))
    (net (code 575) (name "Net-(J9-PadK26)")
      (node (ref J9) (pin K26)))
    (net (code 576) (name "Net-(J9-PadG39)")
      (node (ref J9) (pin G39)))
    (net (code 577) (name "Net-(J9-PadG3)")
      (node (ref J9) (pin G3)))
    (net (code 578) (name "Net-(J9-PadH40)")
      (node (ref J9) (pin H40)))
    (net (code 579) (name "Net-(J9-PadJ16)")
      (node (ref J9) (pin J16)))
    (net (code 580) (name "Net-(J9-PadJ30)")
      (node (ref J9) (pin J30)))
    (net (code 581) (name "Net-(J9-PadJ28)")
      (node (ref J9) (pin J28)))
    (net (code 582) (name "Net-(J9-PadJ27)")
      (node (ref J9) (pin J27)))
    (net (code 583) (name "Net-(J9-PadJ25)")
      (node (ref J9) (pin J25)))
    (net (code 584) (name "Net-(J9-PadJ24)")
      (node (ref J9) (pin J24)))
    (net (code 585) (name "Net-(J9-PadJ22)")
      (node (ref J9) (pin J22)))
    (net (code 586) (name "Net-(J9-PadJ21)")
      (node (ref J9) (pin J21)))
    (net (code 587) (name "Net-(J9-PadJ19)")
      (node (ref J9) (pin J19)))
    (net (code 588) (name "Net-(J9-PadJ18)")
      (node (ref J9) (pin J18)))
    (net (code 589) (name "Net-(J9-PadJ15)")
      (node (ref J9) (pin J15)))
    (net (code 590) (name "Net-(J9-PadJ13)")
      (node (ref J9) (pin J13)))
    (net (code 591) (name "Net-(J9-PadJ12)")
      (node (ref J9) (pin J12)))
    (net (code 592) (name "Net-(J9-PadJ10)")
      (node (ref J9) (pin J10)))
    (net (code 593) (name "Net-(J9-PadJ9)")
      (node (ref J9) (pin J9)))
    (net (code 594) (name "Net-(J9-PadJ7)")
      (node (ref J9) (pin J7)))
    (net (code 595) (name "Net-(J9-PadJ6)")
      (node (ref J9) (pin J6)))
    (net (code 596) (name "Net-(J9-PadJ3)")
      (node (ref J9) (pin J3)))
    (net (code 597) (name "Net-(J9-PadJ2)")
      (node (ref J9) (pin J2)))
    (net (code 600) (name +3.3VP)
      (node (ref U49) (pin 8))
      (node (ref J9) (pin D32))
      (node (ref C267) (pin 2)))
    (net (code 601) (name "Net-(IC1-Pad56)")
      (node (ref IC1) (pin 56))
      (node (ref R92) (pin 1)))
    (net (code 602) (name "Net-(IC1-Pad1)")
      (node (ref IC1) (pin 1))
      (node (ref R93) (pin 2)))
    (net (code 603) (name "Net-(C197-Pad2)")
      (node (ref R83) (pin 2))
      (node (ref R81) (pin 1))
      (node (ref C197) (pin 2))
      (node (ref Y3) (pin 1)))
    (net (code 604) (name "Net-(IC1-Pad64)")
      (node (ref IC1) (pin 64))
      (node (ref R81) (pin 2)))
    (net (code 605) (name /Ethernet/COL)
      (node (ref IC1) (pin 18))
      (node (ref R85) (pin 4))
      (node (ref R98) (pin 2)))
    (net (code 606) (name +2V5)
      (node (ref U35) (pin 4))
      (node (ref C216) (pin 1))
      (node (ref C208) (pin 1))
      (node (ref U38) (pin 1))
      (node (ref U37) (pin 5))
      (node (ref C210) (pin 2))
      (node (ref IC1) (pin 58))
      (node (ref R112) (pin 1))
      (node (ref FB4) (pin 1))
      (node (ref C186) (pin 1))
      (node (ref C185) (pin 2))
      (node (ref R84) (pin 2))
      (node (ref R86) (pin 2)))
    (net (code 607) (name "Net-(J12-Pad11)")
      (node (ref J12) (pin 11))
      (node (ref R86) (pin 1)))
    (net (code 608) (name "Net-(J12-Pad9)")
      (node (ref R84) (pin 1))
      (node (ref J12) (pin 9)))
    (net (code 609) (name /Ethernet/CRS)
      (node (ref R99) (pin 2))
      (node (ref IC1) (pin 19))
      (node (ref R85) (pin 3)))
    (net (code 610) (name /Ethernet/RXD2)
      (node (ref R102) (pin 2))
      (node (ref R82) (pin 1))
      (node (ref IC1) (pin 26)))
    (net (code 611) (name /Ethernet/RX_CLK)
      (node (ref R79) (pin 1))
      (node (ref R109) (pin 2))
      (node (ref IC1) (pin 32)))
    (net (code 612) (name /Ethernet/RX_ER)
      (node (ref IC1) (pin 31))
      (node (ref R110) (pin 2))
      (node (ref R80) (pin 1)))
    (net (code 613) (name "Net-(C199-Pad2)")
      (node (ref T1) (pin 1))
      (node (ref C199) (pin 2)))
    (net (code 614) (name "Net-(C202-Pad2)")
      (node (ref T1) (pin 10))
      (node (ref C202) (pin 2)))
    (net (code 615) (name "Net-(R87-Pad2)")
      (node (ref T1) (pin 15))
      (node (ref R87) (pin 2)))
    (net (code 616) (name "Net-(U35-Pad5)")
      (node (ref U35) (pin 5)))
    (net (code 617) (name "Net-(C211-Pad2)")
      (node (ref C211) (pin 2))
      (node (ref U35) (pin 6)))
    (net (code 618) (name "Net-(U36-Pad2)")
      (node (ref U36) (pin 2)))
    (net (code 619) (name "Net-(R88-Pad2)")
      (node (ref R88) (pin 2))
      (node (ref T1) (pin 18)))
    (net (code 620) (name "Net-(R89-Pad2)")
      (node (ref R89) (pin 2))
      (node (ref T1) (pin 21)))
    (net (code 621) (name "Net-(R90-Pad2)")
      (node (ref R90) (pin 2))
      (node (ref T1) (pin 24)))
    (net (code 622) (name "Net-(C200-Pad2)")
      (node (ref T1) (pin 4))
      (node (ref C200) (pin 2)))
    (net (code 623) (name "Net-(C201-Pad2)")
      (node (ref T1) (pin 7))
      (node (ref C201) (pin 2)))
    (net (code 624) (name "Net-(C204-Pad2)")
      (node (ref R88) (pin 1))
      (node (ref R89) (pin 1))
      (node (ref R90) (pin 1))
      (node (ref R87) (pin 1))
      (node (ref C204) (pin 2)))
    (net (code 625) (name /Ethernet/CLK_SQUELCH_IN)
      (node (ref R96) (pin 1))
      (node (ref IC1) (pin 57)))
    (net (code 626) (name /Ethernet/ELED1)
      (node (ref IC1) (pin 59))
      (node (ref J12) (pin 12)))
    (net (code 627) (name "Net-(C193-Pad1)")
      (node (ref IC1) (pin 8))
      (node (ref IC1) (pin 11))
      (node (ref FB4) (pin 2))
      (node (ref C193) (pin 1))
      (node (ref C194) (pin 1))
      (node (ref C195) (pin 1))
      (node (ref IC1) (pin 2))
      (node (ref C196) (pin 2)))
    (net (code 628) (name /Ethernet/RXD1)
      (node (ref R101) (pin 2))
      (node (ref IC1) (pin 27))
      (node (ref R80) (pin 4)))
    (net (code 629) (name /Ethernet/ELED0)
      (node (ref J12) (pin 10))
      (node (ref IC1) (pin 60)))
    (net (code 630) (name "Net-(IC1-Pad61)")
      (node (ref R95) (pin 1))
      (node (ref IC1) (pin 61)))
    (net (code 631) (name "Net-(IC1-Pad62)")
      (node (ref R94) (pin 1))
      (node (ref IC1) (pin 62)))
    (net (code 632) (name "Net-(C198-Pad2)")
      (node (ref Y3) (pin 3))
      (node (ref R83) (pin 1))
      (node (ref IC1) (pin 63))
      (node (ref C198) (pin 2)))
    (net (code 633) (name "Net-(IC1-Pad65)")
      (node (ref IC1) (pin 65)))
    (net (code 634) (name "Net-(IC1-Pad66)")
      (node (ref IC1) (pin 66)))
    (net (code 635) (name "Net-(C205-Pad1)")
      (node (ref C205) (pin 1))
      (node (ref IC1) (pin 67)))
    (net (code 636) (name +1V0)
      (node (ref FB3) (pin 1))
      (node (ref IC1) (pin 17))
      (node (ref C213) (pin 1))
      (node (ref IC1) (pin 34))
      (node (ref C180) (pin 2))
      (node (ref C178) (pin 1))
      (node (ref C179) (pin 1))
      (node (ref U36) (pin 1)))
    (net (code 637) (name /Ethernet/RXD4)
      (node (ref R104) (pin 2))
      (node (ref IC1) (pin 24))
      (node (ref R82) (pin 3)))
    (net (code 638) (name "Net-(IC1-Pad55)")
      (node (ref IC1) (pin 55))
      (node (ref TP4) (pin 1)))
    (net (code 639) (name "Net-(IC1-Pad15)")
      (node (ref IC1) (pin 15))
      (node (ref TP5) (pin 1)))
    (net (code 640) (name "Net-(IC1-Pad16)")
      (node (ref IC1) (pin 16))
      (node (ref TP6) (pin 1)))
    (net (code 641) (name /Ethernet/FASTLINK_FAIL_2V5)
      (node (ref U38) (pin 2))
      (node (ref IC1) (pin 52)))
    (net (code 642) (name GEMGXL_MDC)
      (node (ref R113) (pin 1))
      (node (ref IC1) (pin 48))
      (node (ref U1) (pin B13)))
    (net (code 643) (name GEMGXL_MDIO)
      (node (ref U1) (pin C12))
      (node (ref R114) (pin 2))
      (node (ref IC1) (pin 50)))
    (net (code 644) (name /Ethernet/GEMGXL_RST_2V5)
      (node (ref IC1) (pin 53))
      (node (ref U37) (pin 4)))
    (net (code 645) (name /Ethernet/RX_DV)
      (node (ref IC1) (pin 30))
      (node (ref R108) (pin 2))
      (node (ref R80) (pin 2)))
    (net (code 646) (name /Ethernet/RXD0)
      (node (ref R80) (pin 3))
      (node (ref R100) (pin 2))
      (node (ref IC1) (pin 29)))
    (net (code 647) (name /Ethernet/RXD3)
      (node (ref R103) (pin 2))
      (node (ref IC1) (pin 25))
      (node (ref R82) (pin 2)))
    (net (code 648) (name /Ethernet/RXD5)
      (node (ref R105) (pin 2))
      (node (ref R82) (pin 4))
      (node (ref IC1) (pin 23)))
    (net (code 649) (name /Ethernet/RXD6)
      (node (ref IC1) (pin 21))
      (node (ref R85) (pin 1))
      (node (ref R106) (pin 2)))
    (net (code 650) (name /Ethernet/RXD7)
      (node (ref IC1) (pin 20))
      (node (ref R85) (pin 2))
      (node (ref R107) (pin 2)))
    (net (code 651) (name /Ethernet/TX_CLK)
      (node (ref R111) (pin 2))
      (node (ref R91) (pin 1))
      (node (ref IC1) (pin 36)))
    (net (code 652) (name /Ethernet/CLKOUT)
      (node (ref R112) (pin 2))
      (node (ref R97) (pin 2))
      (node (ref IC1) (pin 54)))
    (net (code 653) (name /Ethernet/P0_D3_P)
      (node (ref T1) (pin 11))
      (node (ref IC1) (pin 4)))
    (net (code 654) (name /Ethernet/P0_D3_N)
      (node (ref T1) (pin 12))
      (node (ref IC1) (pin 3)))
    (net (code 655) (name /Ethernet/MX2_P)
      (node (ref T1) (pin 20))
      (node (ref J12) (pin 6)))
    (net (code 656) (name /Ethernet/MX1_P)
      (node (ref T1) (pin 23))
      (node (ref J12) (pin 8)))
    (net (code 657) (name /Ethernet/MX1_N)
      (node (ref J12) (pin 7))
      (node (ref T1) (pin 22)))
    (net (code 658) (name /Ethernet/MX3_P)
      (node (ref J12) (pin 5))
      (node (ref T1) (pin 17)))
    (net (code 659) (name /Ethernet/MX2_N)
      (node (ref J12) (pin 3))
      (node (ref T1) (pin 19)))
    (net (code 660) (name /Ethernet/MX4_P)
      (node (ref T1) (pin 14))
      (node (ref J12) (pin 2)))
    (net (code 661) (name /Ethernet/MX4_N)
      (node (ref T1) (pin 13))
      (node (ref J12) (pin 1)))
    (net (code 662) (name /Ethernet/P0_D0_P)
      (node (ref T1) (pin 2))
      (node (ref IC1) (pin 13)))
    (net (code 663) (name /Ethernet/P0_D0_N)
      (node (ref T1) (pin 3))
      (node (ref IC1) (pin 12)))
    (net (code 664) (name /Ethernet/P0_D1_N)
      (node (ref IC1) (pin 9))
      (node (ref T1) (pin 6)))
    (net (code 665) (name /Ethernet/P0_D1_P)
      (node (ref IC1) (pin 10))
      (node (ref T1) (pin 5)))
    (net (code 666) (name /Ethernet/P0_D2_P)
      (node (ref T1) (pin 8))
      (node (ref IC1) (pin 7)))
    (net (code 667) (name /Ethernet/P0_D2_N)
      (node (ref IC1) (pin 6))
      (node (ref T1) (pin 9)))
    (net (code 668) (name /Ethernet/GEMGXL_MDINT)
      (node (ref IC1) (pin 51))
      (node (ref R115) (pin 2)))
    (net (code 669) (name /Ethernet/MX3_N)
      (node (ref J12) (pin 4))
      (node (ref T1) (pin 16)))
    (net (code 670) (name "Net-(C181-Pad1)")
      (node (ref C184) (pin 2))
      (node (ref FB3) (pin 2))
      (node (ref IC1) (pin 5))
      (node (ref IC1) (pin 14))
      (node (ref C183) (pin 1))
      (node (ref IC1) (pin 68))
      (node (ref C182) (pin 1))
      (node (ref C181) (pin 1)))
    (net (code 672) (name "Net-(R7-Pad2)")
      (node (ref R7) (pin 2))
      (node (ref U8) (pin B9)))
    (net (code 673) (name "Net-(R8-Pad2)")
      (node (ref U9) (pin B9))
      (node (ref R8) (pin 2)))
    (net (code 674) (name "Net-(R9-Pad2)")
      (node (ref R9) (pin 2))
      (node (ref U10) (pin B9)))
    (net (code 675) (name "Net-(U6-PadN7)")
      (node (ref U6) (pin N7)))
    (net (code 676) (name DDR_CKE1)
      (node (ref U7) (pin G2))
      (node (ref R163) (pin 2))
      (node (ref U6) (pin G2))
      (node (ref U5) (pin G2))
      (node (ref U1) (pin AA6))
      (node (ref U8) (pin G2))
      (node (ref U4) (pin G2))
      (node (ref U2) (pin G2))
      (node (ref U9) (pin G2))
      (node (ref U3) (pin G2))
      (node (ref U10) (pin G2)))
    (net (code 677) (name DDR_A7)
      (node (ref U1) (pin R2))
      (node (ref U5) (pin M8))
      (node (ref U8) (pin M8))
      (node (ref U4) (pin M8))
      (node (ref U10) (pin M8))
      (node (ref U3) (pin M8))
      (node (ref U7) (pin M8))
      (node (ref U6) (pin M8))
      (node (ref U9) (pin M8))
      (node (ref R168) (pin 1))
      (node (ref U2) (pin M8)))
    (net (code 678) (name DDR_A9)
      (node (ref U10) (pin M7))
      (node (ref U1) (pin T3))
      (node (ref U6) (pin M7))
      (node (ref U7) (pin M7))
      (node (ref U4) (pin M7))
      (node (ref U2) (pin M7))
      (node (ref R168) (pin 2))
      (node (ref U5) (pin M7))
      (node (ref U9) (pin M7))
      (node (ref U3) (pin M7))
      (node (ref U8) (pin M7)))
    (net (code 679) (name DDR_A8)
      (node (ref U8) (pin M2))
      (node (ref U2) (pin M2))
      (node (ref U4) (pin M2))
      (node (ref U7) (pin M2))
      (node (ref U5) (pin M2))
      (node (ref U9) (pin M2))
      (node (ref U3) (pin M2))
      (node (ref U1) (pin R3))
      (node (ref R167) (pin 4))
      (node (ref U10) (pin M2))
      (node (ref U6) (pin M2)))
    (net (code 680) (name DDR_A5)
      (node (ref U1) (pin N5))
      (node (ref R168) (pin 3))
      (node (ref U7) (pin L8))
      (node (ref U2) (pin L8))
      (node (ref U5) (pin L8))
      (node (ref U3) (pin L8))
      (node (ref U6) (pin L8))
      (node (ref U4) (pin L8))
      (node (ref U9) (pin L8))
      (node (ref U10) (pin L8))
      (node (ref U8) (pin L8)))
    (net (code 681) (name DDR_A6)
      (node (ref U3) (pin L2))
      (node (ref U7) (pin L2))
      (node (ref R167) (pin 2))
      (node (ref U5) (pin L2))
      (node (ref U8) (pin L2))
      (node (ref U4) (pin L2))
      (node (ref U1) (pin P4))
      (node (ref U6) (pin L2))
      (node (ref U9) (pin L2))
      (node (ref U10) (pin L2))
      (node (ref U2) (pin L2)))
    (net (code 682) (name DDR_A3)
      (node (ref U9) (pin K7))
      (node (ref U10) (pin K7))
      (node (ref U4) (pin K7))
      (node (ref R166) (pin 2))
      (node (ref U6) (pin K7))
      (node (ref U5) (pin K7))
      (node (ref U2) (pin K7))
      (node (ref U3) (pin K7))
      (node (ref U8) (pin K7))
      (node (ref U1) (pin P3))
      (node (ref U7) (pin K7)))
    (net (code 683) (name DDR_A4)
      (node (ref U5) (pin K3))
      (node (ref U9) (pin K3))
      (node (ref U6) (pin K3))
      (node (ref R167) (pin 1))
      (node (ref U8) (pin K3))
      (node (ref U4) (pin K3))
      (node (ref U1) (pin T1))
      (node (ref U3) (pin K3))
      (node (ref U7) (pin K3))
      (node (ref U2) (pin K3))
      (node (ref U10) (pin K3)))
    (net (code 684) (name DDR_A12)
      (node (ref U3) (pin J7))
      (node (ref U5) (pin J7))
      (node (ref U8) (pin J7))
      (node (ref U4) (pin J7))
      (node (ref U2) (pin J7))
      (node (ref U1) (pin P5))
      (node (ref U9) (pin J7))
      (node (ref R166) (pin 4))
      (node (ref U6) (pin J7))
      (node (ref U10) (pin J7))
      (node (ref U7) (pin J7)))
    (net (code 685) (name DDR_A10)
      (node (ref U2) (pin J3))
      (node (ref U7) (pin J3))
      (node (ref U6) (pin J3))
      (node (ref U5) (pin J3))
      (node (ref U4) (pin J3))
      (node (ref U8) (pin J3))
      (node (ref R165) (pin 3))
      (node (ref U9) (pin J3))
      (node (ref U10) (pin J3))
      (node (ref U1) (pin U1))
      (node (ref U3) (pin J3)))
    (net (code 686) (name "Net-(R6-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref U7) (pin B9)))
    (net (code 687) (name "Net-(U7-PadA3)")
      (node (ref U7) (pin A3)))
    (net (code 688) (name DDR_A13)
      (node (ref U7) (pin N8))
      (node (ref U2) (pin N8))
      (node (ref U4) (pin N8))
      (node (ref U10) (pin N8))
      (node (ref U1) (pin T2))
      (node (ref U6) (pin N8))
      (node (ref U3) (pin N8))
      (node (ref R169) (pin 2))
      (node (ref U5) (pin N8))
      (node (ref U8) (pin N8))
      (node (ref U9) (pin N8)))
    (net (code 689) (name "Net-(U8-PadN7)")
      (node (ref U8) (pin N7)))
    (net (code 690) (name DDR_A11)
      (node (ref U3) (pin N2))
      (node (ref U6) (pin N2))
      (node (ref U4) (pin N2))
      (node (ref U1) (pin R4))
      (node (ref U10) (pin N2))
      (node (ref U5) (pin N2))
      (node (ref U7) (pin N2))
      (node (ref U8) (pin N2))
      (node (ref U2) (pin N2))
      (node (ref U9) (pin N2))
      (node (ref R180) (pin 2)))
    (net (code 691) (name "Net-(U6-PadA3)")
      (node (ref U6) (pin A3)))
    (net (code 692) (name "Net-(U7-PadN7)")
      (node (ref U7) (pin N7)))
    (net (code 693) (name DDR_ALERT_N)
      (node (ref U5) (pin L9))
      (node (ref U3) (pin L9))
      (node (ref U10) (pin L9))
      (node (ref U4) (pin L9))
      (node (ref U2) (pin L9))
      (node (ref U6) (pin L9))
      (node (ref R178) (pin 1))
      (node (ref U1) (pin W6))
      (node (ref U9) (pin L9))
      (node (ref U7) (pin L9))
      (node (ref U8) (pin L9)))
    (net (code 694) (name "Net-(R5-Pad2)")
      (node (ref U6) (pin B9))
      (node (ref R5) (pin 2)))
    (net (code 695) (name DDR_ACT_N)
      (node (ref U3) (pin H3))
      (node (ref U8) (pin H3))
      (node (ref U1) (pin U3))
      (node (ref U10) (pin H3))
      (node (ref U2) (pin H3))
      (node (ref R165) (pin 1))
      (node (ref U5) (pin H3))
      (node (ref U7) (pin H3))
      (node (ref U6) (pin H3))
      (node (ref U4) (pin H3))
      (node (ref U9) (pin H3)))
    (net (code 696) (name DDR_RAS_N)
      (node (ref R164) (pin 1))
      (node (ref U6) (pin H8))
      (node (ref U5) (pin H8))
      (node (ref U7) (pin H8))
      (node (ref U4) (pin H8))
      (node (ref U8) (pin H8))
      (node (ref U3) (pin H8))
      (node (ref U10) (pin H8))
      (node (ref U2) (pin H8))
      (node (ref U9) (pin H8))
      (node (ref U1) (pin M2)))
    (net (code 697) (name DDR_CAS_N)
      (node (ref U8) (pin H7))
      (node (ref U1) (pin M3))
      (node (ref U3) (pin H7))
      (node (ref U4) (pin H7))
      (node (ref U10) (pin H7))
      (node (ref U7) (pin H7))
      (node (ref U6) (pin H7))
      (node (ref U9) (pin H7))
      (node (ref U2) (pin H7))
      (node (ref U5) (pin H7))
      (node (ref R164) (pin 2)))
    (net (code 698) (name DDR_WE_N)
      (node (ref U1) (pin N1))
      (node (ref U9) (pin H2))
      (node (ref U5) (pin H2))
      (node (ref U2) (pin H2))
      (node (ref U6) (pin H2))
      (node (ref U4) (pin H2))
      (node (ref R163) (pin 4))
      (node (ref U3) (pin H2))
      (node (ref U10) (pin H2))
      (node (ref U7) (pin H2))
      (node (ref U8) (pin H2)))
    (net (code 699) (name DDR_CKE)
      (node (ref U10) (pin G3))
      (node (ref U6) (pin G3))
      (node (ref R163) (pin 3))
      (node (ref U1) (pin AB6))
      (node (ref U7) (pin G3))
      (node (ref U9) (pin G3))
      (node (ref U2) (pin G3))
      (node (ref U3) (pin G3))
      (node (ref U4) (pin G3))
      (node (ref U8) (pin G3))
      (node (ref U5) (pin G3)))
    (net (code 700) (name DDR_BG1)
      (node (ref U8) (pin J8))
      (node (ref U4) (pin J8))
      (node (ref U2) (pin J8))
      (node (ref U3) (pin J8))
      (node (ref U5) (pin J8))
      (node (ref U6) (pin J8))
      (node (ref U9) (pin J8))
      (node (ref U10) (pin J8))
      (node (ref U1) (pin V3))
      (node (ref R166) (pin 3))
      (node (ref U7) (pin J8)))
    (net (code 701) (name DDR_BG0)
      (node (ref U7) (pin J2))
      (node (ref U10) (pin J2))
      (node (ref U3) (pin J2))
      (node (ref U1) (pin M5))
      (node (ref U6) (pin J2))
      (node (ref U9) (pin J2))
      (node (ref R165) (pin 2))
      (node (ref U4) (pin J2))
      (node (ref U8) (pin J2))
      (node (ref U2) (pin J2))
      (node (ref U5) (pin J2)))
    (net (code 702) (name DDR_PARITY_IN)
      (node (ref U6) (pin N3))
      (node (ref U5) (pin N3))
      (node (ref U8) (pin N3))
      (node (ref U7) (pin N3))
      (node (ref U10) (pin N3))
      (node (ref U1) (pin U2))
      (node (ref U2) (pin N3))
      (node (ref U3) (pin N3))
      (node (ref U4) (pin N3))
      (node (ref U9) (pin N3))
      (node (ref R179) (pin 2)))
    (net (code 703) (name DDR_BA1)
      (node (ref U8) (pin K8))
      (node (ref U1) (pin N2))
      (node (ref U5) (pin K8))
      (node (ref U7) (pin K8))
      (node (ref U9) (pin K8))
      (node (ref U10) (pin K8))
      (node (ref U2) (pin K8))
      (node (ref U4) (pin K8))
      (node (ref U6) (pin K8))
      (node (ref U3) (pin K8))
      (node (ref R166) (pin 1)))
    (net (code 704) (name DDR_BA0)
      (node (ref U6) (pin K2))
      (node (ref U4) (pin K2))
      (node (ref U2) (pin K2))
      (node (ref U10) (pin K2))
      (node (ref U9) (pin K2))
      (node (ref U5) (pin K2))
      (node (ref U8) (pin K2))
      (node (ref R165) (pin 4))
      (node (ref U3) (pin K2))
      (node (ref U1) (pin M4))
      (node (ref U7) (pin K2)))
    (net (code 705) (name DDR_ODT)
      (node (ref U2) (pin F3))
      (node (ref U8) (pin F3))
      (node (ref U4) (pin F3))
      (node (ref U5) (pin F3))
      (node (ref U3) (pin F3))
      (node (ref U6) (pin F3))
      (node (ref U1) (pin AA5))
      (node (ref U9) (pin F3))
      (node (ref U7) (pin F3))
      (node (ref R163) (pin 1))
      (node (ref U10) (pin F3)))
    (net (code 706) (name DDR_CS0_N)
      (node (ref U1) (pin Y6))
      (node (ref U3) (pin G7))
      (node (ref U4) (pin G7))
      (node (ref U8) (pin G7))
      (node (ref U2) (pin G7))
      (node (ref U9) (pin G7))
      (node (ref U7) (pin G7))
      (node (ref U5) (pin G7))
      (node (ref U6) (pin G7))
      (node (ref U10) (pin G7))
      (node (ref R164) (pin 4)))
    (net (code 707) (name DDR_CLK_P)
      (node (ref U9) (pin F7))
      (node (ref U7) (pin F7))
      (node (ref R170) (pin 2))
      (node (ref U1) (pin K5))
      (node (ref C266) (pin 1))
      (node (ref U10) (pin F7))
      (node (ref U5) (pin F7))
      (node (ref U4) (pin F7))
      (node (ref U3) (pin F7))
      (node (ref U6) (pin F7))
      (node (ref U8) (pin F7))
      (node (ref U2) (pin F7)))
    (net (code 708) (name DDR_CLK_N)
      (node (ref U1) (pin L5))
      (node (ref U7) (pin F8))
      (node (ref U2) (pin F8))
      (node (ref U3) (pin F8))
      (node (ref C266) (pin 2))
      (node (ref R171) (pin 2))
      (node (ref U9) (pin F8))
      (node (ref U6) (pin F8))
      (node (ref U10) (pin F8))
      (node (ref U4) (pin F8))
      (node (ref U5) (pin F8))
      (node (ref U8) (pin F8)))
    (net (code 709) (name DDR_RESET_N)
      (node (ref U4) (pin L1))
      (node (ref U2) (pin L1))
      (node (ref U8) (pin L1))
      (node (ref U6) (pin L1))
      (node (ref U10) (pin L1))
      (node (ref U7) (pin L1))
      (node (ref U5) (pin L1))
      (node (ref U9) (pin L1))
      (node (ref U1) (pin Y5))
      (node (ref U3) (pin L1)))
    (net (code 710) (name DDR_A0)
      (node (ref U3) (pin L3))
      (node (ref U2) (pin L3))
      (node (ref U6) (pin L3))
      (node (ref U5) (pin L3))
      (node (ref U10) (pin L3))
      (node (ref U4) (pin L3))
      (node (ref R167) (pin 3))
      (node (ref U1) (pin N3))
      (node (ref U9) (pin L3))
      (node (ref U7) (pin L3))
      (node (ref U8) (pin L3)))
    (net (code 711) (name "Net-(U9-PadN7)")
      (node (ref U9) (pin N7)))
    (net (code 712) (name "Net-(U10-PadN7)")
      (node (ref U10) (pin N7)))
    (net (code 713) (name DDR_A2)
      (node (ref U3) (pin M3))
      (node (ref U1) (pin N4))
      (node (ref U6) (pin M3))
      (node (ref U10) (pin M3))
      (node (ref U9) (pin M3))
      (node (ref U7) (pin M3))
      (node (ref U4) (pin M3))
      (node (ref U2) (pin M3))
      (node (ref U5) (pin M3))
      (node (ref R181) (pin 2))
      (node (ref U8) (pin M3)))
    (net (code 714) (name DDR_A1)
      (node (ref U4) (pin L7))
      (node (ref U8) (pin L7))
      (node (ref U6) (pin L7))
      (node (ref U1) (pin R1))
      (node (ref U5) (pin L7))
      (node (ref U2) (pin L7))
      (node (ref U3) (pin L7))
      (node (ref U10) (pin L7))
      (node (ref U9) (pin L7))
      (node (ref U7) (pin L7))
      (node (ref R168) (pin 4)))
    (net (code 715) (name DDR_DQ61)
      (node (ref U9) (pin E7))
      (node (ref U1) (pin AA10)))
    (net (code 716) (name DDR_DQ49)
      (node (ref U8) (pin E7))
      (node (ref U1) (pin W11)))
    (net (code 717) (name DDR_DQ54)
      (node (ref U1) (pin W12))
      (node (ref U8) (pin D8)))
    (net (code 718) (name DDR_DQ51)
      (node (ref U1) (pin W8))
      (node (ref U8) (pin D7)))
    (net (code 719) (name DDR_DQ52)
      (node (ref U8) (pin C2))
      (node (ref U1) (pin Y10)))
    (net (code 720) (name DDR_DQ36)
      (node (ref U6) (pin B7))
      (node (ref U1) (pin Y1)))
    (net (code 721) (name DDR_DQ39)
      (node (ref U6) (pin D3))
      (node (ref U1) (pin U5)))
    (net (code 722) (name DDR_ECC_DQ1)
      (node (ref U1) (pin K1))
      (node (ref U10) (pin E7)))
    (net (code 723) (name DDR_ECC_DQ6)
      (node (ref U1) (pin M1))
      (node (ref U10) (pin E3)))
    (net (code 724) (name DDR_ECC_DQ0)
      (node (ref U1) (pin H5))
      (node (ref U10) (pin D2)))
    (net (code 725) (name "Net-(U9-PadA3)")
      (node (ref U9) (pin A3)))
    (net (code 726) (name "Net-(U8-PadA3)")
      (node (ref U8) (pin A3)))
    (net (code 727) (name "Net-(U10-PadA3)")
      (node (ref U10) (pin A3)))
    (net (code 728) (name DDR_DQ59)
      (node (ref U1) (pin AB9))
      (node (ref U9) (pin D7)))
    (net (code 729) (name DDR_DQ40)
      (node (ref U7) (pin C2))
      (node (ref U1) (pin V5)))
    (net (code 730) (name DDR_DQ55)
      (node (ref U1) (pin W9))
      (node (ref U8) (pin B7)))
    (net (code 731) (name DDR_DQ53)
      (node (ref U1) (pin Y9))
      (node (ref U8) (pin D3)))
    (net (code 732) (name DDR_DQ50)
      (node (ref U8) (pin D2))
      (node (ref U1) (pin Y11)))
    (net (code 733) (name DDR_DQ48)
      (node (ref U8) (pin E3))
      (node (ref U1) (pin Y12)))
    (net (code 734) (name DDR_DQ63)
      (node (ref U1) (pin AA11))
      (node (ref U9) (pin D2)))
    (net (code 735) (name DDR_DQ62)
      (node (ref U1) (pin AA9))
      (node (ref U9) (pin B7)))
    (net (code 736) (name DDR_DQ60)
      (node (ref U1) (pin AB11))
      (node (ref U9) (pin D8)))
    (net (code 737) (name DDR_DQ41)
      (node (ref U1) (pin AA1))
      (node (ref U7) (pin D3)))
    (net (code 738) (name DDR_DQ58)
      (node (ref U9) (pin D3))
      (node (ref U1) (pin AA12)))
    (net (code 739) (name DDR_DQ57)
      (node (ref U9) (pin C2))
      (node (ref U1) (pin AB8)))
    (net (code 740) (name DDR_DQ56)
      (node (ref U9) (pin E3))
      (node (ref U1) (pin AA13)))
    (net (code 741) (name DDR_DQ5)
      (node (ref U2) (pin E7))
      (node (ref U1) (pin G4)))
    (net (code 742) (name DDR_DQ4)
      (node (ref U2) (pin C2))
      (node (ref U1) (pin C1)))
    (net (code 743) (name DDR_DQ2)
      (node (ref U2) (pin D8))
      (node (ref U1) (pin F4)))
    (net (code 744) (name DDR_DQ38)
      (node (ref U1) (pin W2))
      (node (ref U6) (pin D2)))
    (net (code 745) (name DDR_DQ18)
      (node (ref U4) (pin D7))
      (node (ref U1) (pin A4)))
    (net (code 746) (name DDR_DQ31)
      (node (ref U1) (pin C7))
      (node (ref U5) (pin D7)))
    (net (code 747) (name DDR_DQ28)
      (node (ref U1) (pin E6))
      (node (ref U5) (pin D8)))
    (net (code 748) (name DDR_DQ26)
      (node (ref U1) (pin D6))
      (node (ref U5) (pin B7)))
    (net (code 749) (name DDR_DQ24)
      (node (ref U1) (pin C4))
      (node (ref U5) (pin C2)))
    (net (code 750) (name DDR_DQ37)
      (node (ref U6) (pin D7))
      (node (ref U1) (pin W3)))
    (net (code 751) (name DDR_DQ35)
      (node (ref U1) (pin V2))
      (node (ref U6) (pin E3)))
    (net (code 752) (name DDR_DQ34)
      (node (ref U1) (pin T4))
      (node (ref U6) (pin E7)))
    (net (code 753) (name DDR_DQ33)
      (node (ref U1) (pin W1))
      (node (ref U6) (pin D8)))
    (net (code 754) (name DDR_DQ32)
      (node (ref U1) (pin R5))
      (node (ref U6) (pin C2)))
    (net (code 755) (name DDR_DQ47)
      (node (ref U7) (pin D7))
      (node (ref U1) (pin AA4)))
    (net (code 756) (name DDR_DQ46)
      (node (ref U1) (pin AB3))
      (node (ref U7) (pin D8)))
    (net (code 757) (name DDR_DQ45)
      (node (ref U7) (pin B7))
      (node (ref U1) (pin AA3)))
    (net (code 758) (name DDR_DQ44)
      (node (ref U1) (pin AB2))
      (node (ref U7) (pin E7)))
    (net (code 759) (name DDR_DQ43)
      (node (ref U7) (pin D2))
      (node (ref U1) (pin Y2)))
    (net (code 760) (name DDR_DQ42)
      (node (ref U1) (pin Y3))
      (node (ref U7) (pin E3)))
    (net (code 761) (name CHIPLINK_RX_DAT1)
      (node (ref U1) (pin AB18))
      (node (ref J9) (pin D21)))
    (net (code 762) (name CHIPLINK_RX_DAT14)
      (node (ref J9) (pin H28))
      (node (ref U1) (pin U18)))
    (net (code 763) (name CHIPLINK_RX_DAT13)
      (node (ref J9) (pin D24))
      (node (ref U1) (pin AB19)))
    (net (code 764) (name CHIPLINK_RX_DAT12)
      (node (ref J9) (pin D23))
      (node (ref U1) (pin V16)))
    (net (code 765) (name CHIPLINK_RX_DAT11)
      (node (ref U1) (pin W19))
      (node (ref J9) (pin G25)))
    (net (code 766) (name CHIPLINK_RX_DAT10)
      (node (ref J9) (pin G24))
      (node (ref U1) (pin Y19)))
    (net (code 767) (name CHIPLINK_RX_DAT9)
      (node (ref J9) (pin H26))
      (node (ref U1) (pin V18)))
    (net (code 768) (name CHIPLINK_RX_DAT8)
      (node (ref U1) (pin AA19))
      (node (ref J9) (pin H25)))
    (net (code 769) (name CHIPLINK_RX_DAT7)
      (node (ref J9) (pin G22))
      (node (ref U1) (pin Y17)))
    (net (code 770) (name CHIPLINK_RX_DAT6)
      (node (ref U1) (pin Y18))
      (node (ref J9) (pin G21)))
    (net (code 771) (name CHIPLINK_RX_DAT5)
      (node (ref U1) (pin W18))
      (node (ref J9) (pin H23)))
    (net (code 772) (name CHIPLINK_RX_DAT4)
      (node (ref J9) (pin H22))
      (node (ref U1) (pin W16)))
    (net (code 773) (name CHIPLINK_RX_DAT3)
      (node (ref J9) (pin C23))
      (node (ref U1) (pin W17)))
    (net (code 774) (name CHIPLINK_RX_DAT2)
      (node (ref U1) (pin AA18))
      (node (ref J9) (pin C22)))
    (net (code 775) (name CHIPLINK_RX_DAT15)
      (node (ref J9) (pin H29))
      (node (ref U1) (pin V19)))
    (net (code 776) (name CHIPLINK_RX_DAT0)
      (node (ref J9) (pin D20))
      (node (ref U1) (pin Y16)))
    (net (code 777) (name CHIPLINK_RX_DAT31)
      (node (ref U1) (pin Y21))
      (node (ref J9) (pin H38)))
    (net (code 778) (name CHIPLINK_RX_DAT30)
      (node (ref J9) (pin H37))
      (node (ref U1) (pin Y22)))
    (net (code 779) (name CHIPLINK_RX_DAT29)
      (node (ref J9) (pin G34))
      (node (ref U1) (pin AA21)))
    (net (code 780) (name CHIPLINK_RX_DAT28)
      (node (ref U1) (pin W20))
      (node (ref J9) (pin G33)))
    (net (code 781) (name CHIPLINK_RX_DAT27)
      (node (ref U1) (pin Y20))
      (node (ref J9) (pin H35)))
    (net (code 782) (name CHIPLINK_RX_DAT26)
      (node (ref J9) (pin H34))
      (node (ref U1) (pin AB21)))
    (net (code 783) (name CHIPLINK_RX_DAT25)
      (node (ref J9) (pin G31))
      (node (ref U1) (pin V20)))
    (net (code 784) (name CHIPLINK_RX_DAT24)
      (node (ref J9) (pin G30))
      (node (ref U1) (pin R17)))
    (net (code 785) (name CHIPLINK_RX_DAT23)
      (node (ref U1) (pin AA20))
      (node (ref J9) (pin H32)))
    (net (code 786) (name CHIPLINK_RX_DAT22)
      (node (ref U1) (pin AB20))
      (node (ref J9) (pin H31)))
    (net (code 787) (name CHIPLINK_RX_DAT21)
      (node (ref J9) (pin C27))
      (node (ref U1) (pin P18)))
    (net (code 788) (name CHIPLINK_RX_DAT20)
      (node (ref J9) (pin C26))
      (node (ref U1) (pin U17)))
    (net (code 789) (name CHIPLINK_RX_DAT19)
      (node (ref J9) (pin D27))
      (node (ref U1) (pin T18)))
    (net (code 790) (name CHIPLINK_RX_DAT18)
      (node (ref U1) (pin U19))
      (node (ref J9) (pin D26)))
    (net (code 791) (name CHIPLINK_RX_DAT17)
      (node (ref U1) (pin R18))
      (node (ref J9) (pin G28)))
    (net (code 792) (name CHIPLINK_RX_DAT16)
      (node (ref J9) (pin G27))
      (node (ref U1) (pin V17)))
    (net (code 793) (name DDR_ECC_DQ7)
      (node (ref U1) (pin L3))
      (node (ref U10) (pin D7)))
    (net (code 794) (name DDR_ECC_DQ5)
      (node (ref U1) (pin L4))
      (node (ref U10) (pin C2)))
    (net (code 795) (name DDR_ECC_DQ4)
      (node (ref U10) (pin D3))
      (node (ref U1) (pin L1)))
    (net (code 796) (name DDR_ECC_DQ3)
      (node (ref U10) (pin D8))
      (node (ref U1) (pin L2)))
    (net (code 797) (name DDR_ECC_DQ2)
      (node (ref U1) (pin K4))
      (node (ref U10) (pin B7)))
    (net (code 798) (name DDR_DQ11)
      (node (ref U1) (pin G1))
      (node (ref U3) (pin D7)))
    (net (code 799) (name DDR_DQ9)
      (node (ref U1) (pin F1))
      (node (ref U3) (pin E7)))
    (net (code 800) (name CHIPLINK_TX_DAT27)
      (node (ref J9) (pin D18))
      (node (ref R153) (pin 7)))
    (net (code 801) (name CHIPLINK_TX_DAT18)
      (node (ref J9) (pin D14))
      (node (ref R145) (pin 5)))
    (net (code 802) (name CHIPLINK_TX_DAT19)
      (node (ref J9) (pin D15))
      (node (ref R155) (pin 5)))
    (net (code 803) (name CHIPLINK_TX_DAT20)
      (node (ref J9) (pin C14))
      (node (ref R155) (pin 6)))
    (net (code 804) (name CHIPLINK_TX_DAT21)
      (node (ref J9) (pin C15))
      (node (ref R152) (pin 8)))
    (net (code 805) (name CHIPLINK_TX_DAT22)
      (node (ref R146) (pin 8))
      (node (ref J9) (pin H16)))
    (net (code 806) (name CHIPLINK_TX_DAT23)
      (node (ref R155) (pin 7))
      (node (ref J9) (pin H17)))
    (net (code 807) (name CHIPLINK_TX_DAT24)
      (node (ref R145) (pin 7))
      (node (ref J9) (pin G15)))
    (net (code 808) (name CHIPLINK_TX_DAT25)
      (node (ref J9) (pin G16))
      (node (ref R146) (pin 7)))
    (net (code 809) (name CHIPLINK_TX_DAT26)
      (node (ref J9) (pin D17))
      (node (ref R145) (pin 8)))
    (net (code 810) (name CHIPLINK_TX_DAT17)
      (node (ref R147) (pin 8))
      (node (ref J9) (pin G13)))
    (net (code 811) (name CHIPLINK_TX_DAT28)
      (node (ref J9) (pin C18))
      (node (ref R153) (pin 5)))
    (net (code 812) (name CHIPLINK_TX_DAT29)
      (node (ref J9) (pin C19))
      (node (ref R145) (pin 6)))
    (net (code 813) (name CHIPLINK_TX_DAT30)
      (node (ref J9) (pin H19))
      (node (ref R153) (pin 6)))
    (net (code 814) (name CHIPLINK_TX_DAT31)
      (node (ref R153) (pin 8))
      (node (ref J9) (pin H20)))
    (net (code 815) (name CHIPLINK_TX_DAT7)
      (node (ref J9) (pin G10))
      (node (ref R151) (pin 8)))
    (net (code 816) (name CHIPLINK_TX_DAT0)
      (node (ref R154) (pin 8))
      (node (ref J9) (pin G6)))
    (net (code 817) (name CHIPLINK_TX_DAT1)
      (node (ref J9) (pin G7))
      (node (ref R154) (pin 6)))
    (net (code 818) (name CHIPLINK_TX_DAT2)
      (node (ref J9) (pin D8))
      (node (ref R152) (pin 7)))
    (net (code 819) (name CHIPLINK_TX_DAT3)
      (node (ref J9) (pin D9))
      (node (ref R154) (pin 7)))
    (net (code 820) (name CHIPLINK_TX_DAT10)
      (node (ref J9) (pin D11))
      (node (ref R147) (pin 6)))
    (net (code 821) (name CHIPLINK_TX_DAT11)
      (node (ref R151) (pin 7))
      (node (ref J9) (pin D12)))
    (net (code 822) (name CHIPLINK_TX_DAT12)
      (node (ref J9) (pin C10))
      (node (ref R152) (pin 5)))
    (net (code 823) (name CHIPLINK_TX_DAT13)
      (node (ref R147) (pin 5))
      (node (ref J9) (pin C11)))
    (net (code 824) (name CHIPLINK_TX_DAT14)
      (node (ref R146) (pin 6))
      (node (ref J9) (pin H13)))
    (net (code 825) (name CHIPLINK_TX_DAT15)
      (node (ref R155) (pin 8))
      (node (ref J9) (pin H14)))
    (net (code 826) (name CHIPLINK_TX_DAT16)
      (node (ref J9) (pin G12))
      (node (ref R146) (pin 5)))))