{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"merged":[[1,0,2,1],[1,3,3,5],[23,0,23,8],[25,0,25,8]]}
[]
[{"$nulls":3},"xxxx xxxx xxxxx xxPCS BOM  (Sample Bill of Materials)"]
[]
[]
[]
["Item #","*Designator","*Qty","Manufacturer","*Mfg Part #","Description / Value","*Package/Footprint ","Type","Your Instructions / Notes"]
[1,"U1",1,"Linear","LTC3780EG#PBF","IC BUCK-BOOST CONV 24-SSOP","24-SSOP","SMD"]
[2,"U2,U4",2,"Fairchild","LM2904M","IC OPAMP DUAL -40-85 C 8-SOIC","8-SOIC","DNS"]
[3,"U3",1,"ON","LM317MBDTG","LM317M IC REG VOLT ADJ 500MA DPAK","DPAK","SMD"]
[4,"U5",1,"Microchip","PIC16F690-I/SS","IC PIC MCU FLASH 4KX14 20SSOP","20SSOP","SMD"]
[5,"Q1",1,"Diodes Inc","GBJ10005-F","RECT BRIDGE GPP 50V 10A GBJ","GBJ","SMD"]
[6,"R14,R18",2,"Panasonic","ERJ-6ENF4701V","RES 4.70K OHM 1/8W 1% 0805 SMD","0805","SMD"]
[7,"R15",1,"Susumu","RL3720WT-R022-F","RES .022 OHM 1W 1% 0815 SMD","0815","SMD"]
[8,"R16, R31",2,"Panasonic","ERJ-6ENF4702V","RES 47.0K OHM 1/8W 1% 0805 SMD","0805","SMD"]
[9,"C5",1,"Murata","GRM21BR71C225KA12L","CAP CER 2.2UF 16V X7R 0805","0805","SMD"]
[10,"C7",1,"Murata","GRM21BR71C475KA73L","CAP CER 4.7UF 16V X7R 0805","0805","DNS"]
[11,"C8,C22",2,"Muruta","GRM21BR71C105KA01L","CAP CER 1.0UF 16V 10% X7R 0805","0805","SMD"]
[12,"CN6",1,"Molex","538-53398-0671","1.25mm Connectors VERTICAL HDR SMT 6P","SMT 6P","SMD"]
[13,"L1,L2",2,"Coiltronics","DR127-150-R","INDUCTOR SHIELD PWR 15UH SMD","SMD","SMD"]
[14,"L3",1,"TDK","ACM1211-102-2PL-TL","CHOKE COMM MODE 1000 OHM 6A SM","SMD","SMD"]
[15,"CN3,CN4",2,"Molex","53047-0510","CONN HEADER 5POS 1.25MM VERT TIN","5POS","thru-hole"]
[]
[]
["Need a quick and accurante quote? Need an efficient production? Please read SMT Ordering Necessary Files & Info in 1 minute. Thank you very much!"]
[]
["Click for Instructions on How to Create a BOM"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}