{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sierra Sample BOM"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sierra Sample BOM","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"flags":["formulas_cached_only"]}
["This is a sample BOM for  Sierra Circuits' online BOM pricing system. Please use this preferred format for your BOM that you upload."]
["Note: DNI applies to whole row. If only some specific locations of a given ITEM are not to be installed, please create two rows for that item and mark one as DNI."]
["BOM: <Board Name Here>"]
["Assembly Part Number/Revision:"]
["Customer / Company Name: "]
[]
["Item #","Quantity per board","Manufacturer Part #","Do Not Install","Reference designators","Vendor (optional)","Vendor Part Number (optional)","Value (optional)","Size / Footprint  (optional)","Part description/ specs (optional, but recommended)","Manfacturer (optional)"]
[1,2,"T520L337M2R5ATE025",null,"C12,C15","Digi-Key","399-5134-1-ND","330uF","C6032","CAP TANT 330UF 2.5V 20% SMD","Kemet"]
[2,2,"T520L337M2R5ATE025","DNI","C16,C17","Digi-Key","399-5134-1-ND","330uF","C6032","CAP TANT 330UF 2.5V 20% SMD","Kemet"]
[3,2,"RMCF0805FT2K40",null,"R19, R24","Digi-Key","541-2.40KCCT-ND",null,null,"RES SMD 2.4K OHM 1% 1/8W 0805","Vishay Dale"]
[4,5,"C3225X7R1E106M","DNI","C65,C66,C67,C68,C119","Mouser","810-C3225X7R1E106M","10uF","C1210 (3225 metric)","CAP CER 10uF 25V X7R 20% SMD 1210","TDK"]
[5,3,"C0805C103J5GACTU",null,"C149,C151,C161","Digi-Key","399-7992-1-ND","10nF","C0805","CAP CER 10000PF 50V C0G/NP0 0805","KEMET"]
[6,3,"GRM32ER61A476KE20L",null,"C167, C169, C141","Digi-Key","490-3887-1-ND","47uF","C1210 (3225 metric)","CAP CER 47UF 10V X5R 1210","Taiyo Yuden"]
[7,5,"C0805F104K5RACTU",null,"C159, C152, C162, C166, C168","Digi-Key","478-1395-1-ND","0.1uF","C0805","CAP CER 0.1UF 50V X7R 0805","Yageo"]
[8,1,"T495D477M006ATE045",null,"C153","Digi-Key","399-5220-1-ND","470uF","C7343-31","CAP TANTALUM 470UF 6.3V 0.045ohm ESR SMD","Kemet"]
[9,2,"B540C-13-F",null,"D1,D2","Digi-Key","B540C-FDICT-ND","40V 5A","SMC ","DIODE SCHOTTKY 40V 5A SMC","Diodes Inc"]
[10,12,"APHCM2012CGCK-F01",null,"D3,D4,D5,D6,D7,D8,D9,D10,D11,D12,D13,D14","Digi-Key","754-1094-1-ND","LED","LED0805","LED 2X1.25MM LOPRO 570NM GRN SMD","Kingbright Corp"]
[11,1,"2-5177986-5",null,"J5","Digi-Key","A35089CT-ND","CON120","conn_2x60_th","CONN PLUG 120 POS VERT DUAL","TE Connectivity"]
[12,6,"961103-6404-AR",null,"J6,J7,J8,J9,J15,J17","Digi-Key","3M9448-ND","CON3","HDR1X3_TH","CONN HEADER VERT SGL 3POS GOLD","3M"]
[13,1,"961102-6404-AR",null,"J16","Digi-Key","3M9447-ND","JUMPER","HDR1X2TH","CONN HEADER VERT SGL 2POS GOLD","3M"]
[14,10,"GBC36SFBN-M30",null,"JP1-JP10","Digi-Key","S1043E-36-ND","1 PIN HEADER","HDR1x1","1 PIN HEADER; BREAK FROM 36 PIN STANDARD HEADER STRIP","Sullins"]
[15,14,"CRCW080510K0FKEA",null,"R8, R14, R16, R17, R25, R26, R27, R28, R29, R30, R31, R33, R34, R35","Mouser","71-CRCW0805-10K-E3",null,null,"Thick Film Resistors - SMD 1/8watt 10Kohms 1% 100ppm","Vishay"]
[16,3,"MSS1048-103MLB",null,"L4,L6,L7","COILCRAFT","MSS1048-103MLB","10uH","ind_Mss1048","INDUCTOR POWER 10UH 4.0A SMD 26mOHM","COILCRAFT"]
[17,1,"SRR1260-120M",null,"L5","Arrow","SRR1260-120M","12uH","ind_Srr1260","INDUCTOR POWER 12UH 5.0A SMD 23mOHM","BOURNS"]
[18,1,"SRR6603-1R5ML",null,"L8","Digi-Key","SRR6603-1R5MLCT-ND","1.5uH","ind_Srr6603","INDUCTOR POWER 1.5UH 2.8A SMD 45mOHM","BOURNS"]
[19,6,"ERJ-2GEJ271X",null,"R1,R2,R3,R4,R5,R6","Digi-Key","P270JCT-ND","270R","R0402","RES 270 OHM 1/10W 5% 0402 SMD","Panasonic"]
[20,2,"ERJ-2GEJ331X",null,"R7,R9","Digi-Key","P330JCT-ND",330,"R0402","RES 330 OHM 1/10W 5% 0402 SMD","Panasonic"]
[21,5,"ERJ-2GEJ472X",null,"R10,R11,R21,R22,R23","Digi-Key","P4.7KJCT-ND","4.7K","R0402","RES 4.7K OHM 1/10W 5% 0402 SMD","Panasonic"]
[22,2,"ERJ-6ENF6192V",null,"R15,R18","Digi-Key","P61.9KCCT-ND","61.9K","R0805","RES 61.9K OHM 1/8W 1% 0805 SMD","Panasonic"]
[23,1,"ERJ-6ENF1581V",null,"X7","Digi-Key","P1.58KCCT-ND","1.58K","R0805","RES 1.58K OHM 1/8W 1% 0805 SMD","Panasonic"]
[24,1,"NVF2955T1G",null,"Q1","Digi-Key","NVF2955T1GOSCT-ND",null,null,"MOSFET P-CH 60V 2.6A SOT223","ON Semiconductor"]
[25,1,"ERJ-6ENF2550V",null,"R48","Digi-Key","P255CCT-ND",255,"R0805","RES 255 OHM 1/8W 1% 0805 SMD","Panasonic"]
[26,4,"ERJ-3GEY0R00V",null,"R37,R45,R46,R47","Digi-Key","P0.0GCT-ND",0,"R0603","RES ZERO OHM 1/10W 5% 0603 SMD","Panasonic"]
[27,2,"SN74ALVC244NSR",null,"U1,U7","Digi-Key","296-12863-1-ND","SN74ALVC244","SOP-20","IC BUFF/DVR TRI-ST OCTAL 20SOP","Texas Instruments"]
[28,2,"LM22670TJE-ADJ/NOPB",null,"U4,U5","Digi-Key","LM22670TJE-ADJCT-ND","LM22670TJE-ADJ/NOPB","TO263-7","IC REG SWITCH BUC 3A ADJ TO263-7","Texas Instruments"]
[29,1,"ERA-6AEB1402V",null,"X2","Digi-Key","P14KDACT-ND",null,null,"RES SMD 14K OHM 0.1% 1/8W 0805","Panasonic"]
[]
["END OF BOM"]