{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["usb-firewall"],"not_rendered":{"external_links":1,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"usb-firewall","index":0,"n_rows":27,"n_cols":12,"rows_kept":27,"flags":["formulas_cached_only"]}
["BOM: usb-firewall"]
["Assembly Part Number/Revision: 1"]
["Customer / Company Name: Fork Sand, Inc."]
[]
["Item #","Quantity per board","Manufacturer Part #","Do Not Install","Reference designators","Vendor (optional)","Vendor Part Number (optional)","Value (optional)","Size / Footprint  (optional)","Part description/ specs (optional, but recommended)","Manfacturer (optional)","Note"]
[1,2,"STM32F401RCT6TR",null,"U2, U4","Digi-Key","497-19344-2-ND",null,null,"STM32F401xB: USG_footprints:LQFP-64_10x10mm_Pitch0.5mm","STMicroelectronics"]
[2,18,"CC0603KRX7R7BB104",null,"C9, C10, C11, C12, C13, C1, C7, C6, C4, C21, C22, C23, C24, C25, C16, C27, C26, C28","Digi-Key","311-1088-1-ND",null,null,"0.1u: Capacitors_SMD:C_0603","Yageo"]
[3,4,"CL10B475KQ8NQNC",null,"C5, C8, C19, C20","Digi-Key","1276-2087-1-ND",null,null,"4.7u: Capacitors_SMD:C_0603","Samsung Electro-Mechanics"]
[4,4,"CL10C180JB8NNNC",null,"C2, C3, C17, C18","Digi-Key","1276-1089-1-ND",null,null,"18p: Capacitors_SMD:C_0603","Samsung Electro-Mechanics"]
[5,4,"RC0603FR-07220RL",null,"R5, R1, R12, R16","Digi-Key","311-220HRCT-ND",null,null,"220: Resistors_SMD:R_0603","Yageo"]
[6,2,"ABLS-8.000MHZ-B4-T",null,"Y1, Y2","Digi-Key","535-10212-1-ND",null,null,"8MHz: Crystals:Crystal_HC49-SD_SMD","Abracon LLC"]
[7,1,"AZ1117CH-3.3TRG1",null,"U3","Digi-Key","AZ1117CH-3.3TRG1DICT-ND",null,null,"AZ1117CH-3.3: TO_SOT_Packages_SMD:SOT-223","Diodes Incorporated"]
[8,1,"GRM21BR61A226ME51L",null,"C15","Digi-Key","490-10511-1-ND",null,null,"22u: Capacitors_SMD:C_0805","Murata Electronics"]
[9,1,"CC0805KKX5R7BB106",null,"C14","Digi-Key","311-1865-1-ND",null,null,"10u: Capacitors_SMD:C_0805","Yageo"]
[10,1,"1001-011-01101",null,"P1","Digi-Key","1175-1008-ND",null,null,"USB_A_PLUG: USG_footprints:USB_A_PLUG","CNC Tech"]
[11,4,"RC0603FR-0710KL",null,"R4, R6, R11, R13","Digi-Key","311-10.0KHRCT-ND",null,null,"10k: Resistors_SMD:R_0603","311-10.0KHRCT-ND"]
[12,4,"RC0603FR-071KL",null,"R2, R3, R9, R10","Digi-Key","311-1.00KHRCT-ND",null,null,"1k: Resistors_SMD:R_0603","Yageo"]
[13,4,"RC0603FR-0722RL",null,"R8, R7, R15, R14","Digi-Key","311-22.0HRCT-ND",null,null,"22: Resistors_SMD:R_0603","Yageo"]
[14,2,"NUP4114UCW1T2G",null,"U1, U5","Digi-Key","NUP4114UCW1T2GOSCT-ND",null,null,"NUP4114: TO_SOT_Packages_SMD:SC-70-6","ON Semiconductor"]
[15,2,"3220-10-0100-00",null,"JTAG_UPST1, JTAG_DNST1","Arrow","3220-10-0100-00",null,null,"CONN_02X05: USG_footprints:Pin_Header_Straight_2x05_Pitch1.27mm","CNC Tech"]
[16,2,"LTST-C190KFKT",null,"FAULT_UPST1, FAULT_DNST1","Quest Components","LTST-C190KFKT",null,null,"LED: LEDs:LED-0603","Lite-On Inc."]
[17,1,"UE27AC54100",null,"P2","Digi-Key","UE27AC54100-ND",null,null,"USB_A_SOCKET: USG_footprints:USB_A_SOCKET","Amphenol ICC"]
[18,1,"BAV70LT1G",null,"D1","Digi-Key","BAV70LT1GOSCT-ND",null,null,"DOUBLE_DIODE_CCOM: TO_SOT_Packages_SMD:SOT-23","ON Semiconductor"]
[19,1,"1825910-7",null,"RESET1","Digi-Key","450-1804-ND",null,null,"SW_PUSH: USG_footprints:SW_TACT","TE Connectivity"]
[20,1,"10118194-0001LF",null,"P3","Digi-Key","609-4618-1-ND",null,null,"USB_OTG: Connect:USB_Micro-B","Amphenol ICC"]
[]
["END OF BOM"]