(export (version D)
  (design
    (source /home/antonlysak/USG_plus/USG_plus_QFN.sch)
    (date "Вс 07 мар 2021 22:08:08")
    (tool "Eeschema 5.1.6-c6e7f7d~87~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source USG_plus_QFN.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C8)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6038D77D))
    (comp (ref C9)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039A683))
    (comp (ref C11)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039A72C))
    (comp (ref C13)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039AB53))
    (comp (ref C5)
      (value 4.7u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C23733))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039B38F))
    (comp (ref R3)
      (value 220)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25091))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 603AD7C8))
    (comp (ref C3)
      (value 18p)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1549))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603B2919))
    (comp (ref C2)
      (value 18p)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1549))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603B3C8D))
    (comp (ref C4)
      (value 4.7u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C23733))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603C59F1))
    (comp (ref JP2)
      (value ID_U_B0)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60383AE8))
    (comp (ref JP5)
      (value ID_U_1)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603840E5))
    (comp (ref JP3)
      (value ID_U_B1)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60385E10))
    (comp (ref JP4)
      (value ID_U_B2)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60386811))
    (comp (ref R2)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6039A0A4))
    (comp (ref C6)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603BBB6D))
    (comp (ref R1)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 603C0B84))
    (comp (ref JP1)
      (value BOOT_U_1)
      (footprint Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_3_Bridged12) (description "3-pole Solder Jumper, pins 1+2 closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603C7955))
    (comp (ref R4)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 603DB088))
    (comp (ref D1)
      (value FAULT_U1)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C2286))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603E0EEE))
    (comp (ref R6)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6040777A))
    (comp (ref J2)
      (value Conn_01x07)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name LCSC) C225482))
      (libsource (lib Connector_Generic) (part Conn_01x07) (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60431BD6))
    (comp (ref C21)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517CAE))
    (comp (ref C22)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517CB4))
    (comp (ref C23)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517CBA))
    (comp (ref C24)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517CC0))
    (comp (ref C19)
      (value 4.7u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C23733))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517CCC))
    (comp (ref R11)
      (value 220)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25091))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D03))
    (comp (ref C17)
      (value 18p)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1549))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D0B))
    (comp (ref C16)
      (value 18p)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1549))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D11))
    (comp (ref C18)
      (value 4.7u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C23733))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D30))
    (comp (ref JP7)
      (value ID_D_B0)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D3C))
    (comp (ref JP8)
      (value ID_D_B1)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D48))
    (comp (ref JP9)
      (value ID_D_B2)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D4E))
    (comp (ref R10)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D70))
    (comp (ref C20)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D7F))
    (comp (ref R9)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25744))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D8B))
    (comp (ref JP6)
      (value BOOT_D_1)
      (footprint Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_3_Bridged12) (description "3-pole Solder Jumper, pins 1+2 closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517D9A))
    (comp (ref R12)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517DAB))
    (comp (ref D3)
      (value FAULT_D1)
      (footprint LED_SMD:LED_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C72038))
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517DB2))
    (comp (ref R13)
      (value 1K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C11702))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517DD7))
    (comp (ref J3)
      (value Conn_01x07)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical)
      (datasheet ~)
      (fields
        (field (name LCSC) C225482))
      (libsource (lib Connector_Generic) (part Conn_01x07) (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60517DF6))
    (comp (ref JP10)
      (value ID_D_1)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 605632BB))
    (comp (ref U5)
      (value NUP4202)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.onsemi.com/pub_link/Collateral/NUP4202W1-D.PDF)
      (fields
        (field (name LCSC) C970012))
      (libsource (lib Power_Protection) (part NUP4202) (description "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60576B3B))
    (comp (ref R14)
      (value 22)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25092))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6057D03C))
    (comp (ref R15)
      (value 22)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25092))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6064C014))
    (comp (ref C28)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6077370D))
    (comp (ref R16)
      (value 220)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25091))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6077DBCF))
    (comp (ref C27)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 607CBAF9))
    (comp (ref C26)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 607D65BA))
    (comp (ref R7)
      (value 22)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25092))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 608D3B99))
    (comp (ref R8)
      (value 22)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25092))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 609221C3))
    (comp (ref U3)
      (value NUP4202)
      (footprint Package_TO_SOT_SMD:SOT-363_SC-70-6)
      (datasheet http://www.onsemi.com/pub_link/Collateral/NUP4202W1-D.PDF)
      (fields
        (field (name LCSC) C970012))
      (libsource (lib Power_Protection) (part NUP4202) (description "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60937CF5))
    (comp (ref J4)
      (value USB_A_Socket)
      (footprint Connector_USB:USB_A_Molex_67643_Horizontal)
      (datasheet " ~")
      (fields
        (field (name LCSC) C2345))
      (libsource (lib Connector) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6069759E))
    (comp (ref J1)
      (value USB_A_Plug)
      (footprint Connector_USB:USB_A_CNCTech_1001-011-01101_Horizontal)
      (datasheet " ~")
      (fields
        (field (name LCSC) C319178))
      (libsource (lib Connector) (part USB_A) (description "USB Type A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60390DEF))
    (comp (ref C10)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603FA531))
    (comp (ref R5)
      (value 220)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C25091))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 603FA537))
    (comp (ref C15)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603FA54C))
    (comp (ref C12)
      (value 0.1u)
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C1525))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603FA552))
    (comp (ref U1)
      (value AZ1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223)
      (datasheet https://www.diodes.com/assets/Datasheets/AZ1117.pdf)
      (fields
        (field (name LCSC) C92102))
      (libsource (lib Regulator_Linear) (part AZ1117-3.3) (description "1A 20V Fixed LDO Linear Regulator, 3.3V, SOT-89/SOT-223/TO-220/TO-252/TO-263"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6057F800))
    (comp (ref C1)
      (value 10u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C59461))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60582667))
    (comp (ref C7)
      (value 22u)
      (footprint Capacitor_SMD:C_0603_1608Metric)
      (datasheet ~)
      (fields
        (field (name LCSC) C19702))
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6058266D))
    (comp (ref D2)
      (value D_Dual_CommonCathode_AAK)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet ~)
      (fields
        (field (name LCSC) C82479))
      (libsource (lib Device) (part D_Dual_CommonCathode_AAK) (description "Dual diode, common cathode on pin 3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606735EC))
    (comp (ref SW1)
      (value RESET)
      (footprint Button_Switch_SMD:SW_SPST_B3U-1000P)
      (datasheet ~)
      (fields
        (field (name LCSC) C231329))
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 606D79A1))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (fields
        (field (name LCSC) C400090))
      (libsource (lib Device) (part Crystal_GND24_Small) (description "Four pin crystal, GND on pins 2 and 4, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60430E06))
    (comp (ref Y2)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (fields
        (field (name LCSC) C400090))
      (libsource (lib Device) (part Crystal_GND24_Small) (description "Four pin crystal, GND on pins 2 and 4, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604BCFEA))
    (comp (ref U4)
      (value STM32F401CCUx)
      (footprint Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00086815.pdf)
      (libsource (lib MCU_ST_STM32F4) (part STM32F401CCUx) (description "ARM Cortex-M4 MCU, 256KB flash, 64KB RAM, 84MHz, 1.7-3.6V, 36 GPIO, UFQFPN-48"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60452B77))
    (comp (ref U2)
      (value STM32F401CCUx)
      (footprint Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00086815.pdf)
      (libsource (lib MCU_ST_STM32F4) (part STM32F401CCUx) (description "ARM Cortex-M4 MCU, 256KB flash, 64KB RAM, 84MHz, 1.7-3.6V, 36 GPIO, UFQFPN-48"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604617F7)))
  (libparts
    (libpart (lib Connector) (part USB_A)
      (description "USB Type A connector")
      (docs " ~")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x07)
      (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x07))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_GND24_Small)
      (description "Four pin crystal, GND on pins 2 and 4, small symbol")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Device) (part D_Dual_CommonCathode_AAK)
      (description "Dual diode, common cathode on pin 3")
      (docs ~)
      (fields
        (field (name Reference) D)
        (field (name Value) D_Dual_CommonCathode_AAK))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name A) (type passive))
        (pin (num 3) (name K) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Bridged)
      (description "Solder Jumper, 2-pole, closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Bridged))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Open)
      (description "Solder Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_3_Bridged12)
      (description "3-pole Solder Jumper, pins 1+2 closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged12*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_3_Bridged12))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name C) (type input))
        (pin (num 3) (name B) (type passive))))
    (libpart (lib MCU_ST_STM32F4) (part STM32F401CBUx)
      (aliases
        (alias STM32F401CCUx))
      (description "ARM Cortex-M4 MCU, 128KB flash, 64KB RAM, 84MHz, 1.7-3.6V, 36 GPIO, UFQFPN-48")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00086815.pdf)
      (footprints
        (fp QFN*1EP*7x7mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F401CBUx)
        (field (name Footprint) Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name PC13) (type BiDi))
        (pin (num 3) (name PC14) (type BiDi))
        (pin (num 4) (name PC15) (type BiDi))
        (pin (num 5) (name PH0) (type input))
        (pin (num 6) (name PH1) (type input))
        (pin (num 7) (name NRST) (type input))
        (pin (num 8) (name VSSA) (type power_in))
        (pin (num 9) (name VREF+) (type power_in))
        (pin (num 10) (name PA0) (type BiDi))
        (pin (num 11) (name PA1) (type BiDi))
        (pin (num 12) (name PA2) (type BiDi))
        (pin (num 13) (name PA3) (type BiDi))
        (pin (num 14) (name PA4) (type BiDi))
        (pin (num 15) (name PA5) (type BiDi))
        (pin (num 16) (name PA6) (type BiDi))
        (pin (num 17) (name PA7) (type BiDi))
        (pin (num 18) (name PB0) (type BiDi))
        (pin (num 19) (name PB1) (type BiDi))
        (pin (num 20) (name PB2) (type BiDi))
        (pin (num 21) (name PB10) (type BiDi))
        (pin (num 22) (name VCAP1) (type power_in))
        (pin (num 23) (name VSS) (type power_in))
        (pin (num 24) (name VDD) (type power_in))
        (pin (num 25) (name PB12) (type BiDi))
        (pin (num 26) (name PB13) (type BiDi))
        (pin (num 27) (name PB14) (type BiDi))
        (pin (num 28) (name PB15) (type BiDi))
        (pin (num 29) (name PA8) (type BiDi))
        (pin (num 30) (name PA9) (type BiDi))
        (pin (num 31) (name PA10) (type BiDi))
        (pin (num 32) (name PA11) (type BiDi))
        (pin (num 33) (name PA12) (type BiDi))
        (pin (num 34) (name PA13) (type BiDi))
        (pin (num 35) (name VSS) (type power_in))
        (pin (num 36) (name VDD) (type power_in))
        (pin (num 37) (name PA14) (type BiDi))
        (pin (num 38) (name PA15) (type BiDi))
        (pin (num 39) (name PB3) (type BiDi))
        (pin (num 40) (name PB4) (type BiDi))
        (pin (num 41) (name PB5) (type BiDi))
        (pin (num 42) (name PB6) (type BiDi))
        (pin (num 43) (name PB7) (type BiDi))
        (pin (num 44) (name BOOT0) (type input))
        (pin (num 45) (name PB8) (type BiDi))
        (pin (num 46) (name PB9) (type BiDi))
        (pin (num 47) (name VSS) (type power_in))
        (pin (num 48) (name VDD) (type power_in))
        (pin (num 49) (name VSS) (type power_in))))
    (libpart (lib Power_Protection) (part NUP4202)
      (description "Transient voltage suppressor designed to protect high speed data lines from ESD, EFT, and lightning")
      (docs http://www.onsemi.com/pub_link/Collateral/NUP4202W1-D.PDF)
      (footprints
        (fp SOT?363*))
      (fields
        (field (name Reference) U)
        (field (name Value) NUP4202)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-363_SC-70-6))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))))
    (libpart (lib Regulator_Linear) (part AZ1117-1.2)
      (aliases
        (alias AZ1117-1.5)
        (alias AZ1117-1.8)
        (alias AZ1117-2.5)
        (alias AZ1117-2.85)
        (alias AZ1117-3.3)
        (alias AZ1117-5.0))
      (description "1A 20V Fixed LDO Linear Regulator, 1.2V, SOT-89/SOT-223/TO-220/TO-252/TO-263")
      (docs https://www.diodes.com/assets/Datasheets/AZ1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp SOT?89*)
        (fp TO?220*)
        (fp TO?252*)
        (fp TO?263*))
      (fields
        (field (name Reference) U)
        (field (name Value) AZ1117-1.2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Jumper)
      (uri /usr/share/kicad/library/Jumper.lib))
    (library (logical MCU_ST_STM32F4)
      (uri /usr/share/kicad/library/MCU_ST_STM32F4.lib))
    (library (logical Power_Protection)
      (uri /usr/share/kicad/library/Power_Protection.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib)))
  (nets
    (net (code 1) (name "Net-(U4-Pad10)")
      (node (ref U4) (pin 10)))
    (net (code 2) (name "Net-(U4-Pad11)")
      (node (ref U4) (pin 11)))
    (net (code 3) (name "Net-(U4-Pad31)")
      (node (ref U4) (pin 31)))
    (net (code 4) (name "Net-(U4-Pad12)")
      (node (ref U4) (pin 12)))
    (net (code 5) (name "Net-(U4-Pad29)")
      (node (ref U4) (pin 29)))
    (net (code 6) (name "Net-(U4-Pad30)")
      (node (ref U4) (pin 30)))
    (net (code 7) (name "Net-(U4-Pad18)")
      (node (ref U4) (pin 18)))
    (net (code 8) (name "Net-(U4-Pad19)")
      (node (ref U4) (pin 19)))
    (net (code 9) (name "Net-(U4-Pad21)")
      (node (ref U4) (pin 21)))
    (net (code 10) (name "Net-(JP10-Pad2)")
      (node (ref JP10) (pin 2))
      (node (ref U4) (pin 25)))
    (net (code 11) (name "Net-(JP9-Pad2)")
      (node (ref U4) (pin 26))
      (node (ref JP9) (pin 2)))
    (net (code 12) (name GND)
      (node (ref C5) (pin 2))
      (node (ref JP4) (pin 1))
      (node (ref JP3) (pin 1))
      (node (ref JP5) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 49))
      (node (ref JP2) (pin 1))
      (node (ref U2) (pin 47))
      (node (ref U2) (pin 35))
      (node (ref JP1) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref JP10) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref U2) (pin 20))
      (node (ref J2) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 23))
      (node (ref C2) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref U4) (pin 49))
      (node (ref JP9) (pin 1))
      (node (ref U4) (pin 20))
      (node (ref JP8) (pin 1))
      (node (ref SW1) (pin 2))
      (node (ref U4) (pin 23))
      (node (ref U4) (pin 35))
      (node (ref U4) (pin 47))
      (node (ref C10) (pin 2))
      (node (ref R5) (pin 1))
      (node (ref Y1) (pin 2))
      (node (ref Y1) (pin 4))
      (node (ref Y2) (pin 2))
      (node (ref Y2) (pin 4))
      (node (ref JP7) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref U4) (pin 8))
      (node (ref J1) (pin 4))
      (node (ref J4) (pin 4))
      (node (ref C20) (pin 1))
      (node (ref C26) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref JP6) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C15) (pin 2)))
    (net (code 13) (name "Net-(JP7-Pad2)")
      (node (ref JP7) (pin 2))
      (node (ref U4) (pin 28)))
    (net (code 14) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 15) (name "Net-(U4-Pad4)")
      (node (ref U4) (pin 4)))
    (net (code 16) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref U4) (pin 40)))
    (net (code 17) (name "Net-(U4-Pad41)")
      (node (ref U4) (pin 41)))
    (net (code 18) (name "Net-(U4-Pad42)")
      (node (ref U4) (pin 42)))
    (net (code 19) (name "Net-(U4-Pad43)")
      (node (ref U4) (pin 43)))
    (net (code 20) (name "Net-(U4-Pad45)")
      (node (ref U4) (pin 45)))
    (net (code 21) (name "Net-(U4-Pad46)")
      (node (ref U4) (pin 46)))
    (net (code 22) (name "Net-(R12-Pad2)")
      (node (ref R12) (pin 2))
      (node (ref U4) (pin 2)))
    (net (code 23) (name "Net-(C18-Pad1)")
      (node (ref C18) (pin 1))
      (node (ref U4) (pin 22)))
    (net (code 24) (name "Net-(C10-Pad1)")
      (node (ref C10) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 25) (name +3V3)
      (node (ref C21) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref D3) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref JP1) (pin 3))
      (node (ref R9) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref U5) (pin 5))
      (node (ref JP6) (pin 3))
      (node (ref C23) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref U4) (pin 48))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 48))
      (node (ref U2) (pin 36))
      (node (ref U2) (pin 24))
      (node (ref U2) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref U4) (pin 24))
      (node (ref U4) (pin 36))
      (node (ref U4) (pin 9))
      (node (ref U1) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 26) (name +5V)
      (node (ref C27) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref C15) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 27) (name "Net-(D2-Pad3)")
      (node (ref D2) (pin 3))
      (node (ref SW1) (pin 1)))
    (net (code 28) (name /UPST_RST)
      (node (ref R1) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref J2) (pin 7))
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 7)))
    (net (code 29) (name /DNST_RST)
      (node (ref U4) (pin 7))
      (node (ref R9) (pin 1))
      (node (ref C20) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref J3) (pin 7)))
    (net (code 30) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 31) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 32) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 33) (name "Net-(U2-Pad29)")
      (node (ref U2) (pin 29)))
    (net (code 34) (name "Net-(U2-Pad30)")
      (node (ref U2) (pin 30)))
    (net (code 35) (name "Net-(U2-Pad31)")
      (node (ref U2) (pin 31)))
    (net (code 36) (name /UPST_D-)
      (node (ref R8) (pin 1))
      (node (ref U2) (pin 32)))
    (net (code 37) (name /UPST_D+)
      (node (ref R7) (pin 1))
      (node (ref U2) (pin 33)))
    (net (code 38) (name "Net-(JP1-Pad2)")
      (node (ref JP1) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 39) (name "Net-(U2-Pad41)")
      (node (ref U2) (pin 41)))
    (net (code 40) (name "Net-(U2-Pad42)")
      (node (ref U2) (pin 42)))
    (net (code 41) (name "Net-(U2-Pad43)")
      (node (ref U2) (pin 43)))
    (net (code 42) (name "Net-(U2-Pad45)")
      (node (ref U2) (pin 45)))
    (net (code 43) (name "Net-(U2-Pad46)")
      (node (ref U2) (pin 46)))
    (net (code 44) (name "Net-(C4-Pad1)")
      (node (ref U2) (pin 22))
      (node (ref C4) (pin 1)))
    (net (code 45) (name "Net-(JP5-Pad2)")
      (node (ref JP5) (pin 2))
      (node (ref U2) (pin 25)))
    (net (code 46) (name "Net-(JP8-Pad2)")
      (node (ref JP8) (pin 2))
      (node (ref U4) (pin 27)))
    (net (code 47) (name "Net-(JP4-Pad2)")
      (node (ref U2) (pin 26))
      (node (ref JP4) (pin 2)))
    (net (code 48) (name "Net-(JP3-Pad2)")
      (node (ref U2) (pin 27))
      (node (ref JP3) (pin 2)))
    (net (code 49) (name "Net-(JP2-Pad2)")
      (node (ref U2) (pin 28))
      (node (ref JP2) (pin 2)))
    (net (code 50) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 51) (name "Net-(U2-Pad21)")
      (node (ref U2) (pin 21)))
    (net (code 52) (name /U_PH0)
      (node (ref Y1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 53) (name /U_PH1)
      (node (ref R3) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 54) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 55) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 56) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 57) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 58) (name /UPST_JTDO)
      (node (ref J2) (pin 6))
      (node (ref U2) (pin 39)))
    (net (code 59) (name "Net-(R6-Pad2)")
      (node (ref R6) (pin 2))
      (node (ref U2) (pin 40)))
    (net (code 60) (name /U_D+)
      (node (ref R7) (pin 2))
      (node (ref U3) (pin 6))
      (node (ref U3) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 61) (name "Net-(JP6-Pad2)")
      (node (ref R10) (pin 2))
      (node (ref JP6) (pin 2)))
    (net (code 62) (name /D_PH0)
      (node (ref Y2) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref C16) (pin 1)))
    (net (code 63) (name /D_PH1)
      (node (ref U4) (pin 6))
      (node (ref R11) (pin 1)))
    (net (code 64) (name /DNST_JTDO)
      (node (ref U4) (pin 39))
      (node (ref J3) (pin 6)))
    (net (code 65) (name "Net-(R2-Pad1)")
      (node (ref U2) (pin 44))
      (node (ref R2) (pin 1)))
    (net (code 66) (name /SPI_TX_OK)
      (node (ref U4) (pin 13))
      (node (ref U2) (pin 13)))
    (net (code 67) (name /SPI_NSS)
      (node (ref U4) (pin 14))
      (node (ref U2) (pin 14)))
    (net (code 68) (name /SPI_SCK)
      (node (ref U4) (pin 15))
      (node (ref U2) (pin 15)))
    (net (code 69) (name /SPI_MISO)
      (node (ref U4) (pin 16))
      (node (ref U2) (pin 16)))
    (net (code 70) (name /SPI_MOSI)
      (node (ref U4) (pin 17))
      (node (ref U2) (pin 17)))
    (net (code 71) (name "Net-(D1-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref D1) (pin 1)))
    (net (code 72) (name /UPST_JTDI)
      (node (ref J2) (pin 5))
      (node (ref U2) (pin 38)))
    (net (code 73) (name /UPST_JTCK)
      (node (ref J2) (pin 4))
      (node (ref U2) (pin 37)))
    (net (code 74) (name /UPST_JTMS)
      (node (ref J2) (pin 3))
      (node (ref U2) (pin 34)))
    (net (code 75) (name "Net-(C17-Pad1)")
      (node (ref Y2) (pin 3))
      (node (ref C17) (pin 1))
      (node (ref R11) (pin 2)))
    (net (code 76) (name "Net-(C3-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref Y1) (pin 3)))
    (net (code 77) (name "Net-(C28-Pad1)")
      (node (ref J4) (pin 5))
      (node (ref R16) (pin 2))
      (node (ref C28) (pin 1)))
    (net (code 78) (name /D_D+)
      (node (ref U5) (pin 6))
      (node (ref J4) (pin 3))
      (node (ref U5) (pin 1))
      (node (ref R14) (pin 1)))
    (net (code 79) (name /DNST_D+)
      (node (ref R14) (pin 2))
      (node (ref U4) (pin 33)))
    (net (code 80) (name /D_D-)
      (node (ref R15) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref U5) (pin 4)))
    (net (code 81) (name /DNST_D-)
      (node (ref U4) (pin 32))
      (node (ref R15) (pin 2)))
    (net (code 82) (name /U_D-)
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 4))
      (node (ref R8) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 83) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U4) (pin 44)))
    (net (code 84) (name "Net-(D3-Pad1)")
      (node (ref D3) (pin 1))
      (node (ref R12) (pin 1)))
    (net (code 85) (name /DNST_JTDI)
      (node (ref J3) (pin 5))
      (node (ref U4) (pin 38)))
    (net (code 86) (name /DNST_JTCK)
      (node (ref J3) (pin 4))
      (node (ref U4) (pin 37)))
    (net (code 87) (name /DNST_JTMS)
      (node (ref U4) (pin 34))
      (node (ref J3) (pin 3)))))