(export (version D)
  (design
    (source /home/antonlysak/KiCAD/KeyCon/KeyCon/KeyCon.sch)
    (date "Sun 17 Mar 2019 21:32:09 MSK")
    (tool "Eeschema 5.0.0-rc3-6a2723a~65~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source KeyCon.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value Ext_conn)
      (footprint Connector_PinSocket_2.00mm:PinSocket_2x20_P2.00mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C823E9B))
    (comp (ref J2)
      (value Carrier_conn)
      (footprint Connector_PinHeader_2.00mm:PinHeader_2x20_P2.00mm_Vertical_SMD)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x20_Odd_Even) (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C82407E))
    (comp (ref U2)
      (value ICE40HX1K-TQ144)
      (footprint Package_QFP:TQFP-144_20x20mm_P0.5mm)
      (datasheet http://www.latticesemi.com/Products/FPGAandCPLD/iCE40)
      (libsource (lib FPGA_Lattice) (part ICE40HX1K-TQ144) (description "iCE40 HX FPGA, 1280 LUTs, 1.2V, TQFP-144"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C88C132))
    (comp (ref C1)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8C0B88))
    (comp (ref C2)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8F4C9D))
    (comp (ref R1)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C91AA23))
    (comp (ref R2)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9268A8))
    (comp (ref R3)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C92A795))
    (comp (ref R4)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C92E76C))
    (comp (ref U1)
      (value MX25R3235FM1xx1)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf)
      (libsource (lib Memory_Flash) (part MX25R3235FM1xx1) (description "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOIC-8"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7C448A))
    (comp (ref U3)
      (value NCV8114ASN120T1G)
      (footprint Package_TO_SOT_SMD:TSOT-23-5)
      (datasheet https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf)
      (libsource (lib Regulator_Linear) (part NCV8114ASN120T1G) (description "300 mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.2V fixed positive output, TSOT-23-5"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9782F3))
    (comp (ref C4)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C978969))
    (comp (ref C3)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C97D988))
    (comp (ref R5)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9B8C07))
    (comp (ref J24)
      (value Conn_01x24)
      (footprint Connector_FFC-FPC:TE_2-84953-4_1x24-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x24) (description "Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7E40CC))
    (comp (ref J26)
      (value Conn_01x26)
      (footprint Connector_FFC-FPC:TE_2-84953-6_1x26-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x26) (description "Generic connector, single row, 01x26, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7E4343))
    (comp (ref J32)
      (value Conn_01x32)
      (footprint KeyCon:Noname_1x32-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x32) (description "Generic connector, single row, 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7E46D0))
    (comp (ref J34)
      (value Conn_01x34)
      (footprint KeyCon:Noname_1x34-1MP_P1.0mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x34) (description "Generic connector, single row, 01x34, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C85406F))
    (comp (ref X1)
      (value XO53)
      (footprint Oscillator:Oscillator_SMD_EuroQuartz_XO53-4Pin_5.0x3.2mm)
      (datasheet http://cdn-reichelt.de/documents/datenblatt/B400/XO53.pdf)
      (libsource (lib Oscillator) (part XO53) (description "Low Power Consumption Clock Oscillator"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDC274E))
    (comp (ref C5)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDCFDE6))
    (comp (ref C10)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C82EF63))
    (comp (ref R193)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C851CD1))
    (comp (ref C11)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8834C5))
    (comp (ref R101)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C8DC40C))
    (comp (ref R103)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C911F72))
    (comp (ref R102)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C92A602))
    (comp (ref R104)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C95C08A))
    (comp (ref R105)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C976147))
    (comp (ref R107)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C976150))
    (comp (ref R106)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C976159))
    (comp (ref R108)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C976162))
    (comp (ref R109)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9BB649))
    (comp (ref R111)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9BB652))
    (comp (ref R110)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9BB65B))
    (comp (ref R112)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9BB664))
    (comp (ref R192)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9E8EA9))
    (comp (ref R151)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA75A3D))
    (comp (ref R153)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA75A46))
    (comp (ref R152)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA75A4F))
    (comp (ref R154)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA75A58))
    (comp (ref R155)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAB57BB))
    (comp (ref R157)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAB57C4))
    (comp (ref R156)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAB57CD))
    (comp (ref R158)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAB57D6))
    (comp (ref R159)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAE121A))
    (comp (ref R161)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAE1223))
    (comp (ref R160)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CAE122C))
    (comp (ref R162)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF4B))
    (comp (ref R164)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF54))
    (comp (ref R163)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF5D))
    (comp (ref R165)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF66))
    (comp (ref R166)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF6F))
    (comp (ref R168)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF78))
    (comp (ref R167)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF81))
    (comp (ref R169)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF8A))
    (comp (ref R170)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF93))
    (comp (ref R171)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB0EF9C))
    (comp (ref C14)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB48841))
    (comp (ref C15)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB4884F))
    (comp (ref C12)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC842F7))
    (comp (ref C13)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC84305))
    (comp (ref C16)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D226EAA))
    (comp (ref C17)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D226EB8))
    (comp (ref C6)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C924E20))
    (comp (ref C7)
      (value "10 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C98CFE1))
    (comp (ref R6)
      (value 100)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C9DC8D2))
    (comp (ref D4)
      (value TO-1608BC-PG)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D3484EE))
    (comp (ref R204)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D3B7F17))
    (comp (ref C9)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA8511F))
    (comp (ref C8)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA85126))
    (comp (ref R8)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA8513C))
    (comp (ref U4)
      (value NCV8114ASN330T1G)
      (footprint Package_TO_SOT_SMD:TSOT-23-5)
      (datasheet https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf)
      (libsource (lib Regulator_Linear) (part NCV8114ASN330T1G) (description "300 mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 3.3V fixed positive output, TSOT-23-5"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAC1B82))
    (comp (ref D5)
      (value TO-1608BC-PG)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DD44272))
    (comp (ref R205)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DD44279))
    (comp (ref D6)
      (value TO-1608BC-PG)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DD63AE4))
    (comp (ref R206)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DD63AEB))
    (comp (ref R120)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7CA4DA))
    (comp (ref R251)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7EB2C5))
    (comp (ref R252)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7EB2CC))
    (comp (ref R253)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E7EB2D3))
    (comp (ref D7)
      (value 1PS76SB10)
      (footprint Diode_SMD:D_SOD-323)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C882C3C))
    (comp (ref D1)
      (value TO-1608BC-MYF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C89610F))
    (comp (ref R201)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C896116))
    (comp (ref D2)
      (value TO-1608BC-MYF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C89611F))
    (comp (ref R202)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C896126))
    (comp (ref D3)
      (value TO-1608BC-MYF)
      (footprint Diode_SMD:D_0603_1608Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C89612F))
    (comp (ref R203)
      (value 200)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C896136))
    (comp (ref R113)
      (value 300)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CD9E4A0))
    (comp (ref R300)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26016))
    (comp (ref R302)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2601F))
    (comp (ref R301)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26028))
    (comp (ref R303)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26031))
    (comp (ref R304)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2603A))
    (comp (ref R306)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26043))
    (comp (ref R305)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2604C))
    (comp (ref R307)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26055))
    (comp (ref R308)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2605E))
    (comp (ref R310)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26067))
    (comp (ref R309)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26070))
    (comp (ref R312)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26079))
    (comp (ref R314)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26082))
    (comp (ref R313)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2608B))
    (comp (ref R315)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE26094))
    (comp (ref R316)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE2609D))
    (comp (ref R318)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE260A6))
    (comp (ref R317)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE260AF))
    (comp (ref R319)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE260B8))
    (comp (ref R320)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE260C1))
    (comp (ref R311)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE260CA))
    (comp (ref R322)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357C8))
    (comp (ref R321)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357D1))
    (comp (ref R324)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357DA))
    (comp (ref R326)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357E3))
    (comp (ref R325)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357EC))
    (comp (ref R327)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357F5))
    (comp (ref R328)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF357FE))
    (comp (ref R330)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF35807))
    (comp (ref R329)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF35810))
    (comp (ref R331)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF35819))
    (comp (ref R332)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF35822))
    (comp (ref R323)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF3582B))
    (comp (ref R333)
      (value 10K)
      (footprint Resistor_SMD:R_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF6C2BA))
    (comp (ref C54)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDC492A))
    (comp (ref C55)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDFD04F))
    (comp (ref C53)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE356F7))
    (comp (ref C52)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE6DD9C))
    (comp (ref C51)
      (value "10 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CEDF710))
    (comp (ref C56)
      (value "0.01 uF")
      (footprint Capacitor_SMD:C_0402_1005Metric)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CF51FCF)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x24)
      (description "Generic connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x24))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x26)
      (description "Generic connector, single row, 01x26, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x26))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x32)
      (description "Generic connector, single row, 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x32))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x34)
      (description "Generic connector, single row, 01x34, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x34))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x20_Odd_Even)
      (description "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x20_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib FPGA_Lattice) (part ICE40HX1K-TQ144)
      (description "iCE40 HX FPGA, 1280 LUTs, 1.2V, TQFP-144")
      (docs http://www.latticesemi.com/Products/FPGAandCPLD/iCE40)
      (footprints
        (fp TQFP*20x20mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ICE40HX1K-TQ144)
        (field (name Footprint) Package_QFP:TQFP-144_20x20mm_P0.5mm))
      (pins
        (pin (num 1) (name IOL_1A) (type BiDi))
        (pin (num 2) (name IOL_1B) (type BiDi))
        (pin (num 3) (name IOL_2A) (type BiDi))
        (pin (num 4) (name IOL_2B) (type BiDi))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name VCCIO_3) (type power_in))
        (pin (num 7) (name IOL_3A) (type BiDi))
        (pin (num 8) (name IOL_3B) (type BiDi))
        (pin (num 9) (name IOL_4A) (type BiDi))
        (pin (num 10) (name IOL_4B) (type BiDi))
        (pin (num 11) (name IOL_5A) (type BiDi))
        (pin (num 12) (name IOL_5B) (type BiDi))
        (pin (num 13) (name GND) (type passive))
        (pin (num 14) (name GND) (type passive))
        (pin (num 15) (name NC) (type NotConnected))
        (pin (num 16) (name NC) (type NotConnected))
        (pin (num 17) (name NC) (type NotConnected))
        (pin (num 18) (name NC) (type NotConnected))
        (pin (num 19) (name IOL_6A) (type BiDi))
        (pin (num 20) (name IOL_6B_GBIN7) (type BiDi))
        (pin (num 21) (name IOL_7A_GBIN6) (type BiDi))
        (pin (num 22) (name IOL_7B) (type BiDi))
        (pin (num 23) (name IOL_8A) (type BiDi))
        (pin (num 24) (name IOL_8B) (type BiDi))
        (pin (num 25) (name IOL_9A) (type BiDi))
        (pin (num 26) (name IOL_9B) (type BiDi))
        (pin (num 27) (name VCC) (type power_in))
        (pin (num 28) (name IOL_10A) (type BiDi))
        (pin (num 29) (name IOL_10B) (type BiDi))
        (pin (num 30) (name VCCIO_3) (type passive))
        (pin (num 31) (name IOL_11A) (type BiDi))
        (pin (num 32) (name IOL_11B) (type BiDi))
        (pin (num 33) (name IOL_12A) (type BiDi))
        (pin (num 34) (name IOL_12B) (type BiDi))
        (pin (num 35) (name VCCPLL) (type power_in))
        (pin (num 36) (name GNDPLL) (type power_in))
        (pin (num 37) (name IOB_24) (type BiDi))
        (pin (num 38) (name IOB_25) (type BiDi))
        (pin (num 39) (name IOB_26) (type BiDi))
        (pin (num 40) (name NC) (type NotConnected))
        (pin (num 41) (name IOB_27) (type BiDi))
        (pin (num 42) (name IOB_28) (type BiDi))
        (pin (num 43) (name IOB_29) (type BiDi))
        (pin (num 44) (name IOB_30) (type BiDi))
        (pin (num 45) (name IOB_31) (type BiDi))
        (pin (num 46) (name VCCIO_2) (type power_in))
        (pin (num 47) (name IOB_32) (type BiDi))
        (pin (num 48) (name IOB_33) (type BiDi))
        (pin (num 49) (name IOB_35_GBIN5) (type BiDi))
        (pin (num 50) (name IOB_36_GBIN4) (type BiDi))
        (pin (num 51) (name VCC) (type passive))
        (pin (num 52) (name IOB_34) (type BiDi))
        (pin (num 53) (name NC) (type NotConnected))
        (pin (num 54) (name NC) (type NotConnected))
        (pin (num 55) (name NC) (type NotConnected))
        (pin (num 56) (name IOB_37) (type BiDi))
        (pin (num 57) (name VCCIO_2) (type passive))
        (pin (num 58) (name IOB_38) (type BiDi))
        (pin (num 59) (name GND) (type passive))
        (pin (num 60) (name IOB_39) (type BiDi))
        (pin (num 61) (name IOB_40) (type BiDi))
        (pin (num 62) (name IOB_41) (type BiDi))
        (pin (num 63) (name IOB_42_CBSEL0) (type BiDi))
        (pin (num 64) (name IOB_43_CBSEL1) (type BiDi))
        (pin (num 65) (name CDONE) (type openCol))
        (pin (num 66) (name ~CRESET_B) (type input))
        (pin (num 67) (name IOB_44_SDO) (type BiDi))
        (pin (num 68) (name IOB_45_SDI) (type BiDi))
        (pin (num 69) (name GND) (type passive))
        (pin (num 70) (name IOB_46_SCK) (type BiDi))
        (pin (num 71) (name IOB_47_SS) (type BiDi))
        (pin (num 72) (name VCC_SPI) (type power_in))
        (pin (num 73) (name IOR_48) (type BiDi))
        (pin (num 74) (name IOR_49) (type BiDi))
        (pin (num 75) (name IOR_50) (type BiDi))
        (pin (num 76) (name IOR_51) (type BiDi))
        (pin (num 77) (name NC) (type NotConnected))
        (pin (num 78) (name IOR_52) (type BiDi))
        (pin (num 79) (name IOR_53) (type BiDi))
        (pin (num 80) (name IOR_54) (type BiDi))
        (pin (num 81) (name IOR_55) (type BiDi))
        (pin (num 82) (name NC) (type NotConnected))
        (pin (num 83) (name NC) (type NotConnected))
        (pin (num 84) (name NC) (type NotConnected))
        (pin (num 85) (name NC) (type NotConnected))
        (pin (num 86) (name GND) (type passive))
        (pin (num 87) (name IOR_56) (type BiDi))
        (pin (num 88) (name IOR_57) (type BiDi))
        (pin (num 89) (name VCCIO_1) (type power_in))
        (pin (num 90) (name IOR_58) (type BiDi))
        (pin (num 91) (name IOR_59) (type BiDi))
        (pin (num 92) (name VCC) (type passive))
        (pin (num 93) (name IOR_60_GBIN3) (type BiDi))
        (pin (num 94) (name IOR_61_GBIN2) (type BiDi))
        (pin (num 95) (name IOR_62) (type BiDi))
        (pin (num 96) (name IOR_63) (type BiDi))
        (pin (num 97) (name IOR_64) (type BiDi))
        (pin (num 98) (name IOR_65) (type BiDi))
        (pin (num 99) (name IOR_66) (type BiDi))
        (pin (num 100) (name VCCIO_1) (type passive))
        (pin (num 101) (name IOR_67) (type BiDi))
        (pin (num 102) (name IOR_68) (type BiDi))
        (pin (num 103) (name GND) (type passive))
        (pin (num 104) (name IOR_69) (type BiDi))
        (pin (num 105) (name IOR_70) (type BiDi))
        (pin (num 106) (name IOR_71) (type BiDi))
        (pin (num 107) (name IOR_72) (type BiDi))
        (pin (num 108) (name VPP_2V5) (type power_in))
        (pin (num 109) (name VPP_FAST) (type power_in))
        (pin (num 110) (name NC) (type NotConnected))
        (pin (num 111) (name VCC) (type passive))
        (pin (num 112) (name IOT_73) (type BiDi))
        (pin (num 113) (name IOT_74) (type BiDi))
        (pin (num 114) (name IOT_75) (type BiDi))
        (pin (num 115) (name IOT_76) (type BiDi))
        (pin (num 116) (name IOT_77) (type BiDi))
        (pin (num 117) (name IOT_78) (type BiDi))
        (pin (num 118) (name IOT_79) (type BiDi))
        (pin (num 119) (name IOT_80) (type BiDi))
        (pin (num 120) (name IOT_81) (type BiDi))
        (pin (num 121) (name IOT_82) (type BiDi))
        (pin (num 122) (name IOT_83) (type BiDi))
        (pin (num 123) (name VCCIO_0) (type power_in))
        (pin (num 124) (name NC) (type NotConnected))
        (pin (num 125) (name NC) (type NotConnected))
        (pin (num 126) (name NC) (type NotConnected))
        (pin (num 127) (name NC) (type NotConnected))
        (pin (num 128) (name IOT_84_GBIN1) (type BiDi))
        (pin (num 129) (name IOT_85_GBIN0) (type BiDi))
        (pin (num 130) (name NC) (type NotConnected))
        (pin (num 131) (name NC) (type NotConnected))
        (pin (num 132) (name GND) (type passive))
        (pin (num 133) (name VCCIO_0) (type passive))
        (pin (num 134) (name IOT_87) (type BiDi))
        (pin (num 135) (name IOT_88) (type BiDi))
        (pin (num 136) (name IOT_89) (type BiDi))
        (pin (num 137) (name IOT_90) (type BiDi))
        (pin (num 138) (name IOT_91) (type BiDi))
        (pin (num 139) (name IOT_92) (type BiDi))
        (pin (num 140) (name GND) (type passive))
        (pin (num 141) (name IOT_93) (type BiDi))
        (pin (num 142) (name IOT_94) (type BiDi))
        (pin (num 143) (name IOT_95) (type BiDi))
        (pin (num 144) (name IOT_96) (type BiDi))))
    (libpart (lib Memory_Flash) (part MX25R3235FM1xx1)
      (aliases
        (alias MX25R3235FM2xx1)
        (alias MX25R3235FZNxx1)
        (alias MX25R3235FZBxx1))
      (description "32-Mbit, Wide Range Voltage SPI Serial Flash Memory, SOIC-8")
      (docs http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf)
      (footprints
        (fp SOIC?8*3.9x4.9mm*P1.27mm*)
        (fp SSOP?8*5.25x5.24mm*P1.27mm*)
        (fp WSON?8?1EP*6x5mm*P1.27mm*)
        (fp USON?8*3x4mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MX25R3235FM1xx1))
      (pins
        (pin (num 1) (name ~CS) (type input))
        (pin (num 2) (name SO/SIO1) (type BiDi))
        (pin (num 3) (name ~WP~/SIO2) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SI/SIO0) (type BiDi))
        (pin (num 6) (name SCLK) (type input))
        (pin (num 7) (name ~HOLD~/SIO3) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib Oscillator) (part XO53)
      (description "Low Power Consumption Clock Oscillator")
      (docs http://cdn-reichelt.de/documents/datenblatt/B400/XO53.pdf)
      (footprints
        (fp Oscillator*SMD*EuroQuartz*XO53*5.0x3.2mm*))
      (fields
        (field (name Reference) X)
        (field (name Value) XO53)
        (field (name Footprint) Oscillator:Oscillator_SMD_EuroQuartz_XO53-4Pin_5.0x3.2mm))
      (pins
        (pin (num 1) (name EN) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name V+) (type power_in))))
    (libpart (lib Regulator_Linear) (part NCV8114ASN120T1G)
      (aliases
        (alias NCV8114ASN150T1G)
        (alias NCV8114ASN165T1G)
        (alias NCV8114ASN180T1G)
        (alias NCV8114ASN250T1G)
        (alias NCV8114ASN280T1G)
        (alias NCV8114ASN300T1G)
        (alias NCV8114ASN330T1G)
        (alias NCV8114BSN120T1G)
        (alias NCV8114BSN150T1G)
        (alias NCV8114BSN180T1G)
        (alias NCV8114BSN280T1G)
        (alias NCV8114BSN300T1G)
        (alias NCV8114BSN330T1G))
      (description "300 mA, Low Noise, Linear Regulator with output active discharge function, 1.7-5.5V input voltage range, 1.2V fixed positive output, TSOT-23-5")
      (docs https://ru.mouser.com/datasheet/2/308/NCV8114-D-1107616.pdf)
      (footprints
        (fp TSOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) NCV8114ASN120T1G)
        (field (name Footprint) Package_TO_SOT_SMD:TSOT-23-5))
      (pins
        (pin (num 1) (name IN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name OUT) (type power_out)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical FPGA_Lattice)
      (uri /usr/share/kicad/library/FPGA_Lattice.lib))
    (library (logical Memory_Flash)
      (uri /usr/share/kicad/library/Memory_Flash.lib))
    (library (logical Oscillator)
      (uri /usr/share/kicad/library/Oscillator.lib))
    (library (logical Regulator_Linear)
      (uri /usr/share/kicad/library/Regulator_Linear.lib)))
  (nets
    (net (code 1) (name "Net-(D4-Pad2)")
      (node (ref R204) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 2) (name /NUM_LOCK)
      (node (ref U2) (pin 1))
      (node (ref R204) (pin 1)))
    (net (code 3) (name "Net-(C6-Pad1)")
      (node (ref C6) (pin 1))
      (node (ref U2) (pin 36))
      (node (ref C7) (pin 1)))
    (net (code 4) (name "Net-(C6-Pad2)")
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 35))
      (node (ref R6) (pin 2))
      (node (ref C7) (pin 2)))
    (net (code 5) (name /DEBUG_TX)
      (node (ref J1) (pin 17))
      (node (ref R120) (pin 2)))
    (net (code 6) (name /SCROLL_LOCK)
      (node (ref R206) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 7) (name /CAPS_LOCK)
      (node (ref R205) (pin 1))
      (node (ref U2) (pin 2)))
    (net (code 8) (name /+1V8_EXT)
      (node (ref C16) (pin 2))
      (node (ref C17) (pin 2))
      (node (ref R251) (pin 1))
      (node (ref R252) (pin 1))
      (node (ref R253) (pin 1))
      (node (ref U2) (pin 100))
      (node (ref J2) (pin 36))
      (node (ref U2) (pin 89))
      (node (ref J1) (pin 5)))
    (net (code 9) (name "Net-(R120-Pad1)")
      (node (ref R120) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 10) (name "Net-(U4-Pad4)")
      (node (ref U4) (pin 4)))
    (net (code 11) (name "Net-(R8-Pad2)")
      (node (ref R8) (pin 2))
      (node (ref U4) (pin 3)))
    (net (code 12) (name "Net-(D5-Pad2)")
      (node (ref R205) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 13) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref R206) (pin 2)))
    (net (code 14) (name "Net-(R110-Pad1)")
      (node (ref R110) (pin 1))
      (node (ref U2) (pin 56)))
    (net (code 15) (name "Net-(R111-Pad1)")
      (node (ref U2) (pin 58))
      (node (ref R111) (pin 1)))
    (net (code 16) (name "Net-(R109-Pad1)")
      (node (ref U2) (pin 52))
      (node (ref R109) (pin 1)))
    (net (code 17) (name "Net-(R108-Pad1)")
      (node (ref R108) (pin 1))
      (node (ref U2) (pin 48)))
    (net (code 18) (name "Net-(R106-Pad1)")
      (node (ref R106) (pin 1))
      (node (ref U2) (pin 45)))
    (net (code 19) (name "Net-(R107-Pad1)")
      (node (ref U2) (pin 47))
      (node (ref R107) (pin 1)))
    (net (code 20) (name "Net-(R152-Pad1)")
      (node (ref R152) (pin 1))
      (node (ref U2) (pin 113)))
    (net (code 21) (name "Net-(R153-Pad1)")
      (node (ref R153) (pin 1))
      (node (ref U2) (pin 114)))
    (net (code 22) (name "Net-(R151-Pad1)")
      (node (ref U2) (pin 112))
      (node (ref R151) (pin 1)))
    (net (code 23) (name "Net-(R112-Pad1)")
      (node (ref U2) (pin 60))
      (node (ref R112) (pin 1)))
    (net (code 24) (name "Net-(U2-Pad21)")
      (node (ref U2) (pin 21))
      (node (ref X1) (pin 3)))
    (net (code 25) (name "Net-(R105-Pad1)")
      (node (ref U2) (pin 44))
      (node (ref R105) (pin 1)))
    (net (code 26) (name "Net-(R104-Pad1)")
      (node (ref R104) (pin 1))
      (node (ref U2) (pin 41)))
    (net (code 27) (name "Net-(R102-Pad1)")
      (node (ref U2) (pin 38))
      (node (ref R102) (pin 1)))
    (net (code 28) (name "Net-(R103-Pad1)")
      (node (ref R103) (pin 1))
      (node (ref U2) (pin 39)))
    (net (code 29) (name "Net-(R101-Pad1)")
      (node (ref R101) (pin 1))
      (node (ref U2) (pin 37)))
    (net (code 30) (name "Net-(R170-Pad1)")
      (node (ref U2) (pin 143))
      (node (ref R170) (pin 1)))
    (net (code 31) (name "Net-(R169-Pad1)")
      (node (ref R169) (pin 1))
      (node (ref U2) (pin 142)))
    (net (code 32) (name "Net-(R167-Pad1)")
      (node (ref U2) (pin 139))
      (node (ref R167) (pin 1)))
    (net (code 33) (name "Net-(R168-Pad1)")
      (node (ref R168) (pin 1))
      (node (ref U2) (pin 141)))
    (net (code 34) (name "Net-(R166-Pad1)")
      (node (ref U2) (pin 138))
      (node (ref R166) (pin 1)))
    (net (code 35) (name "Net-(R165-Pad1)")
      (node (ref R165) (pin 1))
      (node (ref U2) (pin 137)))
    (net (code 36) (name "Net-(R163-Pad1)")
      (node (ref R163) (pin 1))
      (node (ref U2) (pin 135)))
    (net (code 37) (name "Net-(R171-Pad1)")
      (node (ref U2) (pin 144))
      (node (ref R171) (pin 1)))
    (net (code 38) (name "Net-(R158-Pad1)")
      (node (ref R158) (pin 1))
      (node (ref U2) (pin 119)))
    (net (code 39) (name "Net-(R156-Pad1)")
      (node (ref U2) (pin 117))
      (node (ref R156) (pin 1)))
    (net (code 40) (name "Net-(R157-Pad1)")
      (node (ref R157) (pin 1))
      (node (ref U2) (pin 118)))
    (net (code 41) (name "Net-(R159-Pad1)")
      (node (ref R159) (pin 1))
      (node (ref U2) (pin 120)))
    (net (code 42) (name "Net-(R155-Pad1)")
      (node (ref R155) (pin 1))
      (node (ref U2) (pin 116)))
    (net (code 43) (name "Net-(R154-Pad1)")
      (node (ref R154) (pin 1))
      (node (ref U2) (pin 115)))
    (net (code 44) (name "Net-(R164-Pad1)")
      (node (ref R164) (pin 1))
      (node (ref U2) (pin 136)))
    (net (code 45) (name "Net-(R162-Pad1)")
      (node (ref R162) (pin 1))
      (node (ref U2) (pin 134)))
    (net (code 46) (name "Net-(R160-Pad1)")
      (node (ref U2) (pin 121))
      (node (ref R160) (pin 1)))
    (net (code 47) (name "Net-(R161-Pad1)")
      (node (ref R161) (pin 1))
      (node (ref U2) (pin 122)))
    (net (code 48) (name /KBD_RC_33)
      (node (ref R333) (pin 2))
      (node (ref J34) (pin 1))
      (node (ref R113) (pin 2)))
    (net (code 49) (name /KBD_RC_28)
      (node (ref J34) (pin 26))
      (node (ref J26) (pin 25))
      (node (ref J32) (pin 25))
      (node (ref R108) (pin 2))
      (node (ref J24) (pin 12))
      (node (ref R328) (pin 2)))
    (net (code 50) (name /KBD_RC_27)
      (node (ref J24) (pin 9))
      (node (ref R327) (pin 2))
      (node (ref J26) (pin 24))
      (node (ref J32) (pin 24))
      (node (ref R107) (pin 2))
      (node (ref J34) (pin 25)))
    (net (code 51) (name /KBD_RC_25)
      (node (ref J26) (pin 22))
      (node (ref R105) (pin 2))
      (node (ref R325) (pin 2))
      (node (ref J24) (pin 6))
      (node (ref J32) (pin 19))
      (node (ref J34) (pin 23)))
    (net (code 52) (name /KBD_RC_26)
      (node (ref J32) (pin 23))
      (node (ref J26) (pin 23))
      (node (ref R106) (pin 2))
      (node (ref J24) (pin 8))
      (node (ref J34) (pin 24))
      (node (ref R326) (pin 2)))
    (net (code 53) (name /KBD_RC_24)
      (node (ref R104) (pin 2))
      (node (ref R324) (pin 2))
      (node (ref J26) (pin 21))
      (node (ref J24) (pin 5))
      (node (ref J34) (pin 22))
      (node (ref J32) (pin 12)))
    (net (code 54) (name /KBD_RC_23)
      (node (ref R103) (pin 2))
      (node (ref R323) (pin 2))
      (node (ref J34) (pin 21))
      (node (ref J26) (pin 20))
      (node (ref J24) (pin 3))
      (node (ref J32) (pin 10)))
    (net (code 55) (name /KBD_RC_32)
      (node (ref J34) (pin 30))
      (node (ref R112) (pin 2))
      (node (ref R332) (pin 2)))
    (net (code 56) (name /+12V_EXT)
      (node (ref J1) (pin 6))
      (node (ref J1) (pin 4))
      (node (ref J2) (pin 37))
      (node (ref J2) (pin 35)))
    (net (code 57) (name "Net-(J2-Pad33)")
      (node (ref J2) (pin 33)))
    (net (code 58) (name /GPIO15)
      (node (ref J2) (pin 34))
      (node (ref J1) (pin 7)))
    (net (code 59) (name /GPIO1)
      (node (ref J1) (pin 18))
      (node (ref J2) (pin 23)))
    (net (code 60) (name "Net-(J2-Pad17)")
      (node (ref J2) (pin 17)))
    (net (code 61) (name /KBD_RC_21)
      (node (ref J32) (pin 7))
      (node (ref J34) (pin 19))
      (node (ref J24) (pin 1))
      (node (ref J26) (pin 18))
      (node (ref R321) (pin 2))
      (node (ref R101) (pin 2)))
    (net (code 62) (name /QSPI1_DQ1_R)
      (node (ref J2) (pin 9))
      (node (ref J1) (pin 32)))
    (net (code 63) (name /PWR_BTN_N)
      (node (ref J2) (pin 3))
      (node (ref J1) (pin 38)))
    (net (code 64) (name /DEBUG_LED3)
      (node (ref R203) (pin 1))
      (node (ref U2) (pin 9)))
    (net (code 65) (name /DEBUG_LED2)
      (node (ref R202) (pin 1))
      (node (ref U2) (pin 8)))
    (net (code 66) (name /DEBUG_LED1)
      (node (ref R201) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 67) (name /KBD_RC_01)
      (node (ref R152) (pin 2))
      (node (ref R301) (pin 2))
      (node (ref J32) (pin 3))
      (node (ref J26) (pin 2))
      (node (ref J24) (pin 7))
      (node (ref J34) (pin 3)))
    (net (code 68) (name /KBD_RC_13)
      (node (ref J24) (pin 22))
      (node (ref R313) (pin 2))
      (node (ref R164) (pin 2))
      (node (ref J32) (pin 20))
      (node (ref J26) (pin 14))
      (node (ref J34) (pin 15)))
    (net (code 69) (name /KBD_RC_12)
      (node (ref R163) (pin 2))
      (node (ref J26) (pin 13))
      (node (ref J34) (pin 14))
      (node (ref R312) (pin 2))
      (node (ref J24) (pin 21))
      (node (ref J32) (pin 18)))
    (net (code 70) (name /KBD_RC_10)
      (node (ref J26) (pin 11))
      (node (ref J34) (pin 12))
      (node (ref R310) (pin 2))
      (node (ref R161) (pin 2))
      (node (ref J32) (pin 16))
      (node (ref J24) (pin 19)))
    (net (code 71) (name /KBD_RC_09)
      (node (ref J26) (pin 10))
      (node (ref J32) (pin 15))
      (node (ref J34) (pin 11))
      (node (ref J24) (pin 18))
      (node (ref R160) (pin 2))
      (node (ref R309) (pin 2)))
    (net (code 72) (name /KBD_RC_08)
      (node (ref J32) (pin 14))
      (node (ref J24) (pin 17))
      (node (ref J26) (pin 9))
      (node (ref R308) (pin 2))
      (node (ref J34) (pin 10))
      (node (ref R159) (pin 2)))
    (net (code 73) (name /KBD_RC_07)
      (node (ref J26) (pin 8))
      (node (ref J32) (pin 13))
      (node (ref J24) (pin 16))
      (node (ref J34) (pin 9))
      (node (ref R307) (pin 2))
      (node (ref R158) (pin 2)))
    (net (code 74) (name /KBD_RC_06)
      (node (ref R306) (pin 2))
      (node (ref J24) (pin 15))
      (node (ref J26) (pin 7))
      (node (ref J32) (pin 11))
      (node (ref J34) (pin 8))
      (node (ref R157) (pin 2)))
    (net (code 75) (name /KBD_RC_04)
      (node (ref R304) (pin 2))
      (node (ref R155) (pin 2))
      (node (ref J34) (pin 6))
      (node (ref J24) (pin 13))
      (node (ref J26) (pin 5))
      (node (ref J32) (pin 6)))
    (net (code 76) (name /KBD_RC_02)
      (node (ref R302) (pin 2))
      (node (ref R153) (pin 2))
      (node (ref J32) (pin 4))
      (node (ref J26) (pin 3))
      (node (ref J34) (pin 4))
      (node (ref J24) (pin 10)))
    (net (code 77) (name /KBD_RC_14)
      (node (ref J26) (pin 15))
      (node (ref R165) (pin 2))
      (node (ref J34) (pin 16))
      (node (ref J24) (pin 23))
      (node (ref J32) (pin 21))
      (node (ref R314) (pin 2)))
    (net (code 78) (name /KBD_RC_00)
      (node (ref J32) (pin 2))
      (node (ref R151) (pin 2))
      (node (ref R300) (pin 2))
      (node (ref J34) (pin 2))
      (node (ref J24) (pin 4))
      (node (ref J26) (pin 1)))
    (net (code 79) (name "Net-(R113-Pad1)")
      (node (ref U2) (pin 61))
      (node (ref R113) (pin 1)))
    (net (code 80) (name /KBD_RC_03)
      (node (ref J32) (pin 5))
      (node (ref R303) (pin 2))
      (node (ref J34) (pin 5))
      (node (ref J26) (pin 4))
      (node (ref J24) (pin 11))
      (node (ref R154) (pin 2)))
    (net (code 81) (name /KBD_RC_18)
      (node (ref R169) (pin 2))
      (node (ref J32) (pin 28))
      (node (ref R318) (pin 2))
      (node (ref J34) (pin 32)))
    (net (code 82) (name /KBD_RC_16)
      (node (ref J32) (pin 26))
      (node (ref R316) (pin 2))
      (node (ref J26) (pin 17))
      (node (ref J34) (pin 18))
      (node (ref R167) (pin 2)))
    (net (code 83) (name /KBD_RC_15)
      (node (ref J24) (pin 24))
      (node (ref R166) (pin 2))
      (node (ref J32) (pin 22))
      (node (ref R315) (pin 2))
      (node (ref J26) (pin 16))
      (node (ref J34) (pin 17)))
    (net (code 84) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R201) (pin 2)))
    (net (code 85) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R202) (pin 2)))
    (net (code 86) (name "Net-(D7-Pad1)")
      (node (ref U2) (pin 108))
      (node (ref D7) (pin 1)))
    (net (code 87) (name "Net-(D3-Pad2)")
      (node (ref D3) (pin 2))
      (node (ref R203) (pin 2)))
    (net (code 88) (name /KBD_RC_17)
      (node (ref J32) (pin 27))
      (node (ref R317) (pin 2))
      (node (ref J34) (pin 31))
      (node (ref R168) (pin 2)))
    (net (code 89) (name /KBD_RC_11)
      (node (ref J32) (pin 17))
      (node (ref R311) (pin 2))
      (node (ref R162) (pin 2))
      (node (ref J24) (pin 20))
      (node (ref J26) (pin 12))
      (node (ref J34) (pin 13)))
    (net (code 90) (name /KBD_RC_22)
      (node (ref J26) (pin 19))
      (node (ref R102) (pin 2))
      (node (ref J24) (pin 2))
      (node (ref J34) (pin 20))
      (node (ref J32) (pin 9))
      (node (ref R322) (pin 2)))
    (net (code 91) (name /KBD_RC_05)
      (node (ref R156) (pin 2))
      (node (ref J32) (pin 8))
      (node (ref R305) (pin 2))
      (node (ref J24) (pin 14))
      (node (ref J26) (pin 6))
      (node (ref J34) (pin 7)))
    (net (code 92) (name Earth)
      (node (ref U2) (pin 103))
      (node (ref J1) (pin 40))
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 14))
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 39))
      (node (ref U2) (pin 13))
      (node (ref J2) (pin 40))
      (node (ref U2) (pin 132))
      (node (ref J1) (pin 39))
      (node (ref C4) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 59))
      (node (ref U2) (pin 69))
      (node (ref U2) (pin 86))
      (node (ref U2) (pin 140))
      (node (ref C1) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref D3) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref C56) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref C55) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref C52) (pin 1))
      (node (ref C51) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref D6) (pin 1)))
    (net (code 93) (name /GPIO9)
      (node (ref J2) (pin 31))
      (node (ref J1) (pin 10)))
    (net (code 94) (name /GPIO7)
      (node (ref J2) (pin 29))
      (node (ref J1) (pin 12)))
    (net (code 95) (name /GPIO5)
      (node (ref J1) (pin 14))
      (node (ref J2) (pin 27)))
    (net (code 96) (name /GPIO3)
      (node (ref J2) (pin 25))
      (node (ref J1) (pin 16)))
    (net (code 97) (name /QSPI1_DQ0_R)
      (node (ref J1) (pin 28))
      (node (ref J2) (pin 13)))
    (net (code 98) (name /QSPI1_CS0_R)
      (node (ref J1) (pin 30))
      (node (ref J2) (pin 11)))
    (net (code 99) (name /QSPI1_SCK_R)
      (node (ref J2) (pin 7))
      (node (ref J1) (pin 34)))
    (net (code 100) (name /RESET_N)
      (node (ref J2) (pin 5))
      (node (ref J1) (pin 36)))
    (net (code 101) (name "Net-(U2-Pad109)")
      (node (ref U2) (pin 109)))
    (net (code 102) (name +1V2)
      (node (ref U3) (pin 5))
      (node (ref R6) (pin 1))
      (node (ref C4) (pin 2))
      (node (ref C54) (pin 2))
      (node (ref U2) (pin 111))
      (node (ref U2) (pin 27))
      (node (ref U2) (pin 51))
      (node (ref C53) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref C51) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref C55) (pin 2))
      (node (ref U2) (pin 92)))
    (net (code 103) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref U3) (pin 3)))
    (net (code 104) (name /+5V_EXT)
      (node (ref U4) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref J2) (pin 38))
      (node (ref J1) (pin 3))
      (node (ref C8) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 105) (name "Net-(R3-Pad2)")
      (node (ref U1) (pin 3))
      (node (ref R3) (pin 2)))
    (net (code 106) (name "Net-(R4-Pad2)")
      (node (ref U1) (pin 7))
      (node (ref R4) (pin 2)))
    (net (code 107) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 108) (name /GPIO8)
      (node (ref J2) (pin 32))
      (node (ref J1) (pin 9)))
    (net (code 109) (name /GPIO6)
      (node (ref J2) (pin 30))
      (node (ref J1) (pin 11)))
    (net (code 110) (name /GPIO4)
      (node (ref J2) (pin 28))
      (node (ref J1) (pin 13)))
    (net (code 111) (name /GPIO2)
      (node (ref J1) (pin 15))
      (node (ref J2) (pin 26)))
    (net (code 112) (name /INTERRUPT)
      (node (ref U2) (pin 97))
      (node (ref R253) (pin 2))
      (node (ref J2) (pin 24)))
    (net (code 113) (name "Net-(J2-Pad22)")
      (node (ref J2) (pin 22)))
    (net (code 114) (name "Net-(J2-Pad21)")
      (node (ref J2) (pin 21)))
    (net (code 115) (name "Net-(J2-Pad20)")
      (node (ref J2) (pin 20)))
    (net (code 116) (name "Net-(J2-Pad19)")
      (node (ref J2) (pin 19)))
    (net (code 117) (name "Net-(J2-Pad15)")
      (node (ref J2) (pin 15)))
    (net (code 118) (name /UART1_RX)
      (node (ref J2) (pin 14))
      (node (ref J1) (pin 27)))
    (net (code 119) (name "Net-(J2-Pad4)")
      (node (ref J2) (pin 4)))
    (net (code 120) (name /ICE_MISO)
      (node (ref U1) (pin 2))
      (node (ref J1) (pin 26))
      (node (ref U2) (pin 68)))
    (net (code 121) (name /ICE_MOSI)
      (node (ref U2) (pin 67))
      (node (ref J1) (pin 24))
      (node (ref U1) (pin 5)))
    (net (code 122) (name /ICE_SCK)
      (node (ref J1) (pin 22))
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 70))
      (node (ref U1) (pin 6)))
    (net (code 123) (name /ICE_CDONE)
      (node (ref J1) (pin 21))
      (node (ref U2) (pin 65))
      (node (ref R193) (pin 2)))
    (net (code 124) (name /ICE_SS)
      (node (ref J1) (pin 20))
      (node (ref U2) (pin 71))
      (node (ref U1) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 125) (name /ICE_CRST_B)
      (node (ref U2) (pin 66))
      (node (ref R192) (pin 2))
      (node (ref J1) (pin 19)))
    (net (code 126) (name /UART1_TX)
      (node (ref J1) (pin 29))
      (node (ref J2) (pin 12)))
    (net (code 127) (name "Net-(J2-Pad10)")
      (node (ref J2) (pin 10)))
    (net (code 128) (name +3V3)
      (node (ref R326) (pin 1))
      (node (ref U2) (pin 30))
      (node (ref U2) (pin 6))
      (node (ref R325) (pin 1))
      (node (ref R323) (pin 1))
      (node (ref U2) (pin 57))
      (node (ref R322) (pin 1))
      (node (ref R333) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref C9) (pin 2))
      (node (ref R332) (pin 1))
      (node (ref R324) (pin 1))
      (node (ref X1) (pin 1))
      (node (ref R310) (pin 1))
      (node (ref R305) (pin 1))
      (node (ref R330) (pin 1))
      (node (ref R306) (pin 1))
      (node (ref R304) (pin 1))
      (node (ref R327) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref X1) (pin 4))
      (node (ref R307) (pin 1))
      (node (ref R328) (pin 1))
      (node (ref R308) (pin 1))
      (node (ref R300) (pin 1))
      (node (ref R329) (pin 1))
      (node (ref C12) (pin 2))
      (node (ref D7) (pin 2))
      (node (ref R302) (pin 1))
      (node (ref R301) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref R303) (pin 1))
      (node (ref R316) (pin 1))
      (node (ref R319) (pin 1))
      (node (ref R317) (pin 1))
      (node (ref R318) (pin 1))
      (node (ref R320) (pin 1))
      (node (ref R321) (pin 1))
      (node (ref R311) (pin 1))
      (node (ref R331) (pin 1))
      (node (ref U2) (pin 72))
      (node (ref C14) (pin 2))
      (node (ref J1) (pin 8))
      (node (ref U2) (pin 46))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref C15) (pin 2))
      (node (ref U1) (pin 8))
      (node (ref U2) (pin 123))
      (node (ref R314) (pin 1))
      (node (ref R312) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref R313) (pin 1))
      (node (ref R193) (pin 1))
      (node (ref U2) (pin 133))
      (node (ref R192) (pin 1))
      (node (ref R315) (pin 1))
      (node (ref R309) (pin 1)))
    (net (code 129) (name "Net-(J1-Pad37)")
      (node (ref J1) (pin 37)))
    (net (code 130) (name /UART0_TX)
      (node (ref J2) (pin 6))
      (node (ref J1) (pin 35)))
    (net (code 131) (name /UART0_RX)
      (node (ref J1) (pin 33))
      (node (ref J2) (pin 8)))
    (net (code 132) (name "Net-(J1-Pad31)")
      (node (ref J1) (pin 31)))
    (net (code 133) (name "Net-(U2-Pad75)")
      (node (ref U2) (pin 75)))
    (net (code 134) (name "Net-(U2-Pad91)")
      (node (ref U2) (pin 91)))
    (net (code 135) (name "Net-(U2-Pad90)")
      (node (ref U2) (pin 90)))
    (net (code 136) (name "Net-(U2-Pad88)")
      (node (ref U2) (pin 88)))
    (net (code 137) (name "Net-(U2-Pad87)")
      (node (ref U2) (pin 87)))
    (net (code 138) (name "Net-(U2-Pad82)")
      (node (ref U2) (pin 82)))
    (net (code 139) (name "Net-(U2-Pad81)")
      (node (ref U2) (pin 81)))
    (net (code 140) (name "Net-(U2-Pad80)")
      (node (ref U2) (pin 80)))
    (net (code 141) (name "Net-(U2-Pad79)")
      (node (ref U2) (pin 79)))
    (net (code 142) (name "Net-(U2-Pad78)")
      (node (ref U2) (pin 78)))
    (net (code 143) (name "Net-(U2-Pad76)")
      (node (ref U2) (pin 76)))
    (net (code 144) (name "Net-(U2-Pad93)")
      (node (ref U2) (pin 93)))
    (net (code 145) (name "Net-(U2-Pad74)")
      (node (ref U2) (pin 74)))
    (net (code 146) (name "Net-(U2-Pad73)")
      (node (ref U2) (pin 73)))
    (net (code 147) (name "Net-(U2-Pad55)")
      (node (ref U2) (pin 55)))
    (net (code 148) (name "Net-(U2-Pad54)")
      (node (ref U2) (pin 54)))
    (net (code 149) (name "Net-(U2-Pad53)")
      (node (ref U2) (pin 53)))
    (net (code 150) (name "Net-(U2-Pad40)")
      (node (ref U2) (pin 40)))
    (net (code 151) (name "Net-(U2-Pad107)")
      (node (ref U2) (pin 107)))
    (net (code 152) (name "Net-(U2-Pad106)")
      (node (ref U2) (pin 106)))
    (net (code 153) (name "Net-(U2-Pad105)")
      (node (ref U2) (pin 105)))
    (net (code 154) (name "Net-(U2-Pad104)")
      (node (ref U2) (pin 104)))
    (net (code 155) (name "Net-(U2-Pad50)")
      (node (ref U2) (pin 50)))
    (net (code 156) (name "Net-(U2-Pad49)")
      (node (ref U2) (pin 49)))
    (net (code 157) (name "Net-(U2-Pad43)")
      (node (ref U2) (pin 43)))
    (net (code 158) (name "Net-(U2-Pad42)")
      (node (ref U2) (pin 42)))
    (net (code 159) (name "Net-(U2-Pad102)")
      (node (ref U2) (pin 102)))
    (net (code 160) (name "Net-(U2-Pad124)")
      (node (ref U2) (pin 124)))
    (net (code 161) (name "Net-(U2-Pad110)")
      (node (ref U2) (pin 110)))
    (net (code 162) (name "Net-(U2-Pad99)")
      (node (ref U2) (pin 99)))
    (net (code 163) (name "Net-(U2-Pad98)")
      (node (ref U2) (pin 98)))
    (net (code 164) (name /I2C0_SDA)
      (node (ref J1) (pin 23))
      (node (ref J2) (pin 18))
      (node (ref R252) (pin 2))
      (node (ref U2) (pin 96)))
    (net (code 165) (name /I2C0_SCL)
      (node (ref R251) (pin 2))
      (node (ref U2) (pin 95))
      (node (ref J1) (pin 25))
      (node (ref J2) (pin 16)))
    (net (code 166) (name "Net-(U2-Pad94)")
      (node (ref U2) (pin 94)))
    (net (code 167) (name "Net-(U2-Pad101)")
      (node (ref U2) (pin 101)))
    (net (code 168) (name "Net-(U2-Pad77)")
      (node (ref U2) (pin 77)))
    (net (code 169) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 170) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 171) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 172) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 173) (name "Net-(U2-Pad129)")
      (node (ref U2) (pin 129)))
    (net (code 174) (name "Net-(U2-Pad128)")
      (node (ref U2) (pin 128)))
    (net (code 175) (name "Net-(C5-Pad1)")
      (node (ref X1) (pin 2))
      (node (ref C5) (pin 1)))
    (net (code 176) (name "Net-(U2-Pad83)")
      (node (ref U2) (pin 83)))
    (net (code 177) (name "Net-(U2-Pad130)")
      (node (ref U2) (pin 130)))
    (net (code 178) (name "Net-(U2-Pad127)")
      (node (ref U2) (pin 127)))
    (net (code 179) (name "Net-(U2-Pad126)")
      (node (ref U2) (pin 126)))
    (net (code 180) (name "Net-(U2-Pad125)")
      (node (ref U2) (pin 125)))
    (net (code 181) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 182) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 183) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 184) (name "Net-(U2-Pad85)")
      (node (ref U2) (pin 85)))
    (net (code 185) (name "Net-(U2-Pad84)")
      (node (ref U2) (pin 84)))
    (net (code 186) (name "Net-(U2-Pad131)")
      (node (ref U2) (pin 131)))
    (net (code 187) (name "Net-(U2-Pad64)")
      (node (ref U2) (pin 64)))
    (net (code 188) (name "Net-(U2-Pad63)")
      (node (ref U2) (pin 63)))
    (net (code 189) (name "Net-(U2-Pad62)")
      (node (ref U2) (pin 62)))
    (net (code 190) (name "Net-(U2-Pad29)")
      (node (ref U2) (pin 29)))
    (net (code 191) (name "Net-(U2-Pad34)")
      (node (ref U2) (pin 34)))
    (net (code 192) (name "Net-(U2-Pad33)")
      (node (ref U2) (pin 33)))
    (net (code 193) (name "Net-(U2-Pad32)")
      (node (ref U2) (pin 32)))
    (net (code 194) (name "Net-(U2-Pad31)")
      (node (ref U2) (pin 31)))
    (net (code 195) (name "Net-(U2-Pad28)")
      (node (ref U2) (pin 28)))
    (net (code 196) (name "Net-(U2-Pad26)")
      (node (ref U2) (pin 26)))
    (net (code 197) (name "Net-(U2-Pad25)")
      (node (ref U2) (pin 25)))
    (net (code 198) (name "Net-(U2-Pad24)")
      (node (ref U2) (pin 24)))
    (net (code 199) (name "Net-(U2-Pad23)")
      (node (ref U2) (pin 23)))
    (net (code 200) (name "Net-(U2-Pad22)")
      (node (ref U2) (pin 22)))
    (net (code 201) (name "Net-(U2-Pad20)")
      (node (ref U2) (pin 20)))
    (net (code 202) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 203) (name /KBD_RC_31)
      (node (ref R111) (pin 2))
      (node (ref J34) (pin 29))
      (node (ref J32) (pin 1))
      (node (ref R331) (pin 2)))
    (net (code 204) (name /KBD_RC_30)
      (node (ref J34) (pin 28))
      (node (ref R330) (pin 2))
      (node (ref R110) (pin 2))
      (node (ref J32) (pin 32)))
    (net (code 205) (name /KBD_RC_29)
      (node (ref J34) (pin 27))
      (node (ref R109) (pin 2))
      (node (ref J26) (pin 26))
      (node (ref J32) (pin 31))
      (node (ref R329) (pin 2)))
    (net (code 206) (name /KBD_RC_20)
      (node (ref R171) (pin 2))
      (node (ref J34) (pin 34))
      (node (ref R320) (pin 2))
      (node (ref J32) (pin 30)))
    (net (code 207) (name /KBD_RC_19)
      (node (ref R319) (pin 2))
      (node (ref J34) (pin 33))
      (node (ref R170) (pin 2))
      (node (ref J32) (pin 29)))))